ZIP-drive mini-HOWTO

Grant Guenther, grant@torque.net

ěŃ: A&˛ advances@nownuri.net

řü [tŹ ZIP-Drive mini HOWTOõ ěŃć ,œ£ c^˚ P>¸ ›¸ `yüq –ř. (]Á §Á:‚ 8ù ; Å P>ú ıQăŞ MUř.) ŤýL ¸ [tŹ ZIP driveõ LINUXĆ zXăŹ YAĆ [ć ;Ł:‚ Pĺú §Á ć ,œ£ §Á:‚ 8ù ;Å sŻüq –Ş Mř. ŤýL Łȷè SCSI HOWTOő ›¸ œLč ,ú Ďćř. ȷœ #˝ êÓ¸ üč ĘĹř. ˇ‹ %ß ÙÛ¸ –ř8 Æ‚Ć3 -‹ú s§ ĘĹř. ¸ ěŃ[t˚ PÌù GPLĆ u ćř. IOMEGA ZIP driveŹ Gý PÌüL –Ź removable media disk drive¸ř. ¸,ù SCSIő parallel¿ort˚~ `Ş˚ sý version¸ –ř. ¸ [tŹ LINUXĆt ZIP Driveõ qN3 PÌăŹŞõ §ÁăL –ř. ¸,ù SCSI

HOWTOő ›¸ ›qbˇ ćř. @ ò C 1 < AÃ 2

C 2 < ZIP ȷĘ¸õ 2 2.1 SSbèÌ . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2

2.2 ZIP Zoom ÒSS! qSSâ . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3

2.3 CăčÌ . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3

C 3 < ZIP ȷĘ¸õõ æć vG zA 3 3.1 SSbèÌ . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4 3.2 vG 1.2.13 ˚ PPA ȷĘ¸č . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4 3.3 Ç& ŢjüŹ vGú æć PPA ȷĘ¸č . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4

3.4 PPA <ž Ę‚Ćt˚ ž¡ . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 5

C 4 < ZIP ȷĘ¸õ PÌ 5 4.1 Ù6èĆ ȷĘ¸č ü§ . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 5

4.2 Fdisk, mke2fs, mount, etc. . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

4.2.1 êSS jȷ˚ %SS¿ . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6

4.2.2 ýĄSS£ řè jȷă§ . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7

4.2.3 ZIP Tools %SS¿ . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7

4.3 %SS¿ Ã4§ . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7

C 5 < Ů[Y ż 7

5.1 ZIP drive£ Ùâ èSSðú §ôč¡ (booting č¡) –Ź`? . . . . . . . . . . . . . . . . . . . 8

5.2 ů IOMEGAŹ 7/Ő ěÒõ 4ěú PÌăŹ`? . . . . . . . . . . . . . . . . . . . . . . . . . 8

5.3 boot timeèĆ qN3 diskõ mountč ¡ –Ź`? . . . . . . . . . . . . . . . . . . . . . . . . . 8

1. AÃ 2

5.4 4` ˇ‹ bootè diskõ Oq nŞ Mú EÍ qE‹¸ ŇfăŹ`? . . . . . . . . . . . . . . . 8 5.5 qE SCSI adapters` ZIP driveő ÒÞ¸ üŹ `... . . . . . . . . . . . . . . . . . . . . . . . . 8

5.6 parallel driveõ real SCSI disk ˛ď PÌč ¡ –Ź`? . . . . . . . . . . . . . . . . . . . . . . 8

5.7 parallel driveĆ printõ ffŒ PÌč ¡ –Ź`? . . . . . . . . . . . . . . . . . . . . . . . . . . 9

5.8 PPAĆt EPP/ECPõ ŞÙľv 3è¸ –Ź`? . . . . . . . . . . . . . . . . . . . . . . . . . . 9

5.9 PPA` IOMEGA˚ parallel port tape driveő ›¸ PÌ¸ `ăć`? . . . . . . . . . . . . . . 9

5.10 PPA` parallel SyQuest EZ135ő ›¸ ȷôú ăŹ`? . . . . . . . . . . . . . . . . . . . . . . 9

C 6 < Ãř /ê˚ AÃõ uúš8... 9

C 1 < AÃ

Iomega ZIP driveŹ ö`<, low-performanceõ "Ĳœ£ăŹ ö `<˚ 'Âă§ ^şć removal media disk drive¸ř. ¸,ù 96MB˚ Ì§ú `ŞŹ disk¸L ȷĘ¸õŹ SCSIő parallel˚ ~`Ş čLú ¸Ìč ¡ –

ř. parallel port versionù ì&£Ź SCSI deviceő ›œ6, IOMEGAP˚ PPA-3 parallel-to-SCSI protocolú PÌăŁ zAú ćř.

¸ [tŹ ýĄSSĆt ZIP driveõ qN3 PÌăŹ`õ §Áćř. ¸,ù SCSI device¸§ :[Ć ŁăÛù

SCSI HOTOõ ›¸ ›Ź ,¸ Is |Åăř. SCSIĆ [ć [tŹ LINUX SCSI systemĆ [ć ;Ł:‚ A

Ãõ uř.

¸ [tŹ řô PŁffiĆ ˚ľ ¡ŽüL Ňśý AÃffiú jěăL –ŹÚ, "&:

ffl Scot Wilcoxon, sewilco@fielday.mn.org

ffl Joe Mack, mack@ncifcrf.gov

ffl Byron Jeff, byron@cc.gatech.edu

#Ź Ťffi˚ Is |Åć §ŁĆ ˇPõ vă6, 4` ‚Ìć ,˚ qE errorĆê þ„ú Ş9ř.

C 2 < ZIP ȷĘ¸õ

3`Ş version˚ Iomega ZIP 100 drive` –ř. Ťffiù ?~ 100 Mbytes õ 9$č¡ –Ź 3.5” FDõ ůù " ¡ć cartridgesõ PÌćř. ¸ %SS¿Ź ì&£Ź 96cyl-2048sec-512byte õ 9$ćř. ¸,ù A\:œ£Ź

96 M bytesĘL ľbćř.

„ěń version ù SCSI interfaceõ ‚Ź <Łm¸˚ 5.25” 4$Í drive¸ř. řô 2`ŞŹ ȷù 7Ĺ_˚ `ÿÏ plastic caseõ ‚Ź ¡$Í drive£t ¡Ù ;Ùú ŃŹř. ¸ ¡$Íù SCSI versionY parallel port

version¸ –ř.

?fi driveŹ ;8Ć À push buttonú `ŞL –ř. ¸,ù diskõ ejectèÅŹÚ PÌýř.

LINUXŹ driveõ PÌăŹ ôKĆŹ drive˚ [ú Ć nŹř. ăŞˇ door` ĆK –Ź ôKĆ button¸

ĎăŞ8 ZIP driveŹ Ť,ú §răLt software unlockõ èÅ8t OĘ£ diskõ eject èÇř.

2.1 SSbèÌ

¡$Í SCSI versionù drive˚ ó8Ć 2„˚ DB25F Ŋ@ şıő 2„˚ configuration switchõ `Ţř. Ť| ă#Ź drive˚ target addressõ xØăŹ ,¸ř : ì&£ xØù 5 ő 6œ£ ćA¸ üq –ř. (SSbè IDõ

@AăŹ ,¸ř.) řô ă#Ź drive` Ŋ@ý chainĆt ˝Ş˚‹ EÍĆ internal terminatorõ SSĄÜ èÅ Ź ,¸ř. 25 pin SCSI connectorŹ Z¿ć »Çùè Í˚ Ţxú PÌćř.

ˇc ¿ê¸ Centronix ZŹ high-density connectorõ `Ţ host adapterõ PÌč EÍĆ (Âv:œ£

AHA1542CF ` ¸ Í˚ connectorõ ŻÅ£ ęęř.) ŤýL ˇc ȷĘ¸õĆ Mcintosh type cable¸ ffiq –

ř8 standard cableY converterõ Ö3 uč¡ –ř. (¸ ¸b§Ź ˇ‹ ŁăÛ¸ `Ţ SCSI host adapter`

centronix high-density connectorõ PÌăŹ ,¸Ę8, ZIP driveŹ 25pin connectorõ PÌăt£ ¸ ˚ P

¸õ žÞèĹv cable¸ ŻÅ£ ćřŹ ,¸ř. ¸,ù ÌS\`Ćt c 2ˇÙAêĆ uč ¡ –ř.)

#Ź 4$Í SCSI driveõ ÃŞŹ Gřř. ăŞˇ #Ź ¸,ù vu 50pin DIP header connectorő [ ›ù~ „˚ SSæXõ `Ů,¸ĘL f´ćř.

¿ê¸ xØć target address( SCSI id )` řô SCSI $Xő ?îăŞ MŹ řŹ ,ú Ý‚ăêÀ ăïè ą. ŤýL SCSIĆ Ŋ@ý ˝Ş˚ $X˚ terminator` enableüq –ŹŞ Ý‚ăêÀ ăïèą. ZŹ external

terminator` zAüq –ŹŞ Ý‚ăêÀ ăïèą.

ˇc ¿ê¸ internal SCSI disk# CD-ROM ú `Ţř8 ŤýL ZIP driveõ ¸y U&ăŹ adapterĆ Ŋ@ ú ćř8 ¿êù bȷĆ –Ź qNć terminatorê ¸y C$ üq –řŹ ,ú checkăŁbˇ ęęř. SCSI bus˚ jÅ ˙şĆtˇ terminator` ÝĄÜ üq –qbˇ ęęř. ˇc ¿ê˚ bus` ‹ÙŹ 4$Í, ‹ÙŹ ¡$Í¸Ę8 terminatorŹ ¡$Í˚ ˙ş $Xő 4$Í˚ ˝Ş˚ $XĆ zAüqb ćř. Ťă# adapter

card ı–ĆŹ terminator` {ř.

?fi cable¸ >L& Ùóüq –ŹŞ Ý‚ú ăĘ.

2.2 ZIP Zoom ÒSS! qSSâ

IOMEGAŹ ZIP Zoom ¸ĘŹ ¸ö˚ SCSI host adapterõ ;L –ř. ¸,ù ŰÆ:œ£ Adaptec 1520 G

Ő˚ adapter¸ř. ¸,ù Macintosh type DB25F connectorõ `ŞL ZIP driveő ›¸ ąŹ cable Y ÒÞý ř. LINUX Ź ¸ host adapterõ aha152x driver £t ŞÙćř.

2.3 CăčÌ

Parallel port ZIP driveŹ Ńè ~„˚ DB25 connectorõ `Ţř ¸,ù Äiù(DB25M)ù CWüŹ parallel

cable£t ŁăÛ˚ {Ňâ˚ parallel port£ Ŋ@èÇř. řô ,ù (female, DB25F) printerõ ŞÙă§ æć

,¸ř. LINUXŹ Ç& ZIP driveő Ŋ@ý printerõ ôèĆ ŞÙăŞŹ MŹř. ÂĲ:‚ ȷzù modulesú ¸Ìľt ›¸ PÌč ¡Ź –Şˇ ˚ú ôèĆ PÌč ¡Ź {ř. ¸Ć Âć configuration switchŹ {ř.

Parallel port ZIP driveŹ =`ŞÍŒ˚ £ţj!ő ÒÞ¸ ýř, Ťă# Ç&˚ Linux driver Ź vuÍY j

ŞşĄ £ţj!ˇú ŞÙćř. ˇc ¿ê¸ £ţj!` hardwareĆt# CMOS setup screenĆt configura-

tion¸ `ăăř8 ¸ ˚| ă#˚ ?ȷ£ setupú ľbˇ ćř.

?fi cable¸ >Lă3 Ùóü}ŹŞ řèćě Ý‚ú ăĘ...

C 3 < ZIP ȷĘ¸õõ æć vG zA

ZIP driveõ LINUXő ›¸ PÌă§ æľtŹ ¿êù SCSI systemY SCSI driveõ ŞÙăêÀ kernel con-

figurationú !Ib ă6, ¿ê¸ PÌăL –Ź host adapterõ ŞÙăêÀ ľb ćř. ˇc ¿ê¸ kernelú

^£ ˇȷŹÚ ˛¿ăŞ Mř8 /usr/src/linux£ `t $§Ć –Ź README fileú ŊuăŁb ćř. /ê č L˚ documentation subdirectoryĆŹ îÌć AÃ` –ř.

¿êù configuration şGÙâ kernelú ˇȷŹ YAú èȷľbćř. Ł§t ŁăÛù ¿ê¸ ŻÅć "¡ć

kernel˚ uĄÅŹõ Ň>č ¡ –ř. make configŹ L;:¸8t, £ò:¸L, ŮżÍé˚ kernel configu-

ration Şł¸ř.

/Ű˚ vGffiù =`Ş ^£Ï žÍú CWćř : make menuconfigŹ menu-oriented interfaceõ `Ş6,

make xconfigŹ X PÌăĆt tk toolkitú ¸ÌăŹ version¸ř.

‹ş ŁăÛffi¸ ¿ê˚ kernel configuration ¸ ȷ#L #8 make dep ŤýL make zlilo (ˇ‹ LILOõ P ÌăŞ MŹř8 make zImage õ PÌăĘ)õ PÌăŁ ^£Ï kernelú ˇffiL ¸,ú install èÇř. ]Á

shutdown & rebootăŹ YAú Ş ˝Ę.

SCSI system˚ ‹Ù ZŹ ;Ùõ modules£t fĄč ¡ –ř. ˇ‹ ŁăÛffi¸ ¸ő ›¸ řř8 ŁăÛ¸

ZIP driveõ accessă§ ;Ć scsi.oõ ďýL řü sd.o ŤýL ˝Ş˚œ£ ŁăÛ˚ host adapterõ ďýŹ

,ú Ý‚ľbćř.

3.1 SSbèÌ

ˇc ŁăÛffi¸ ¸y systemĆ SCSI disk` –ř8, ŤýL ZIP drive` ›ù controllerĆ Ŋ@üq –ř8 Ì¸\˚ kernel configurationù ŻÅ{ř. ŤľŞ Mř8 ŁăÛffiù Ż& kernelú &zAľt compileľb ˇ ćř.

ˇc ¿ê¸ SCSI version˚ ZIP driveõ supportăêÀ kernelú ˇffi}ř8, SCSIő SCSI diskõ ŞÙăê À ˇffiqbˇ ćř. ŤýL ŁăÛffiù ŁăÛ˚ SCSI host adapterõ ŞÙăŹ driver Ńè Û xØľ sq bˇćř. ˇc ZIP Zoomú PÌćř8 aha152x driverõ xØľbˇ ćř.

Linux source tree˚ drivers/scsi subdirectoryĆ –Ź README fileY SCSI HOWTOõ Łȷè ›êÀ ăĘ.

¿ê˚ adapterõ #§ÜăŹ command parameterĆ s˚õ §ÐŁb ćř.

Žõ ffi8, ˇc ¿ê¸ ZIP Zoom cardõ PÌćř8, boot commandĆ ŁăÛù řüY ›¸ parameterõ 8`ľ sqb ćř.(ZŹ /etc/lilo.conf fileĆ appen<£t 8`õ ľ uř.)

aha152x=0x340,11,7,1

¸,ù driverĆ3 ZIP Zoom card˚ port address, IRQõ ˙ľu ,¸ř. - ¿ê˚ bȷĆ jumper` CÂ£ !Å –ŹŞ Ý‚ăêÀ ăŁĘ.

ŁăÛffiù LILO# LOADLIN Ćt kernel configurationú æăŁ Paul Gortmaker’s BOOTPROMPT

HOWTO Ńè ›qbˇ ćř.

3.2 vG 1.2.13 ˚ PPA ȷĘ¸č

ˇc ŁăÛffi¸ KA vGčL 1.2.13Ćt parallel port ZIP driveõ PÌăč Ùćř8 driver˚ version 0.18ú `Kőbˇ ćř. ¸,ù <ftp://gear.torque.net/pub/ppa.c>Ćt anonymous ftpõ `ăŁ `K ď¡ – œ6, qN3 loadable module£t ˇȷŹŞ zX Şłù ppa.c source 4Ć ffi z<üq –ř.

ŁăÛffiù $˚ ĺ\ ^£Ï vGú ˇffiqb ćřŹ ,Ć î]ú ăêÀ ăïèą. "& Slackware˚ pre-

built kernelĆtŹ ppaő ›¸ ȷôăŞ MŹř. ¿ê˚ kernel¸ SCSI support, SCSI disk supportõ ăê

À ăL, lp printer driverŹ supportăêÀ include èĹtŹ <Â Kýř. 1.2.13ĆtŹ ¸ ~ driver` ›ù

kernel 4Ć ›¸ U&č ¡` {ř.

ŁăÛffiù ppa driverõ ď`: (load èĆ) port numberő c^˚ timing parameterõ ”8qsqb č ŻÅ Ą¸ –ř. ¸ľć SAù ppa.c file 4Ć <èüq –ř. default£ driverŹ ZIP drive` parallel port 0x378Ć ]š –řL f´ú ćř.

1.2.13 kernelú æć ¸ driverŹ Ì ¸\˚ Ąăş\ù {ú ,¸ř. ŁăÛffiù ¡„Úó 2.0 kernel¸ #ď

: ¸,¸ PĘŞč §Âľb ćř. (I˝ê ¸[t˚ ȷĄè§` §(¸wÅ.)

3.3 Ç& ŢjüŹ vGú æć PPA ȷĘ¸č

version 1.3.74 ¸ó ppa driverŹ vG˚ vu˚ ‹Ù` ü}ř. 1.3.78 Ű˛£ ľt kernel˚ řô ÙÛĆ ‹

Ù˚ žÜ` –}ř. Ťă# 1.3.85ÙâŹ version 0.26 driverŹ \¿& KAüq Př. LINUX 2.0 ú æć

code-freeze` îÌľ P§ :[Ć 0.26¸ řü vGŽĆ ffiq¨,œ£ §Âćř. (¸y ffiq` –ŞÅ.)

ppaõ ŞÙăêÀ kernelú ˇffi§ æľtŹ low-level SCSI adapter˚ list£ Ùâ SCSI support, SCSI disk

support, IOMEGA ZIP/PPA-3 supportõ `ăăêÀ include èĹbˇ ćř. ŁăÛffiù driverõ loadable

module£t ˇffiqb ćř.

ŁăÛffiù driverõ SAă§ æăŁ /etc/lilo.conf# insmod Ćt command parameterõ PÌăŁbˇ ćř. ¸,ffiù ?~ kernel source tree˚ drivers/scsi/README.ppaĆ §Áüq –ř. řüsectionĆt ¸Ć [ć ^Ĳć Åcú §ÁăêÀ ă9ř.

ˇc ŁăÛffi¸ lpő ppa driverõ ›ù parallel portĆt ?~ PÌăš ćř8 loadable module£t vG {7‹ú ăŁ ŻÅè ´´ lŒt PÌľb ćř. ôèĆ ˚ú ?~ PÌč ¡Ź {ř.

loadable moduleù ÌÎÌ LINUXõ ˛şă3 ˇȷŹ Pj¸ ü}ř. ŤýL #(¸ ÌÎ Ä!ľK`L –ř.

ŁăÛffiù kernel source tree˚ docs/modules.txtõ ›qbˇ ćř.

3.4 PPA <ž Ę‚Ćt˚ ž¡

ˇc ŁăÛffi¸ ¿ê˚ kernelĆt ppaõ fĄăŢř8 ŁăÛffiù parameterõ LILO # LOADLINœ£ Ù â řüY ›ù [łœ£ parameterõ S<ľ sqb ćř.

ppa=base[,speed_high[,speed_low[,nybble]]]

Ł§t baseŹ ŁăÛffi parallel port˚ i/o addressõ ˙ă6, speed highŹ driverĆt fast loopõ æć

timing constant¸ř. speed lowŹ slower loopõ æć timing constant¸6, ŤýL nybbleù driver` 4-bit,

ZŹ nybble modeõ PÌč¡ –êÀ ľsŹ flag¸ř.

Žõ ffi8, defaultsŹ řüY ›¸ §Áþ ¡ –ř :

ppa=0x378,1,6,0

C 4 < ZIP ȷĘ¸õ PÌ

ˇc ŁăÛffi¸ ?fi ŻÅć ÙÛú zAřř8, kernelù ŁăÛffi˚ adapterő driveõ booting ê|Ć ‚é č ,¸ř. ˇc loadable module£t ŁăÛ˚ driverõ zAřř8 ?ú ď`: ćěÌ řü˚ ù˚õ 0 òb ćř.

4.1 Ù6èĆ ȷĘ¸č ü§

ŁăÛffi˚ system¸ boot þ: adapter, drive ŤýL drive4˚ diskĆ [ć =`Ş AÃffiú ÃŁuř. ˇc ŁăÛffi¸ drive4Ć disk` {ř8 ¸ffi AÃ| ‹ÙŹ Ã¸Ş Mú ¡ –œ6, diskõ Oú : ZŹ driveõ

accessčšL touchč EÍĆ ÃŁŞ3 ýř. #Ãıffiù system bootèĆ drive4Ć diskõ OL booting ľ

sč ?Lćř. - Ñ ŕŕýŹ Şł¸ř.

¸ľć message` q%Ć AÝ& #Í## ăŹ ,ù ŁăÛffi¸ systemú configurationăŹ ŞłĆ ţš – ř. Ťă# ¸ffiù /var/adm/messageő ›ù log file£ 9$üq –ř. ˇ‹ q%Ćtê ¸ľć messageõ Ň >č ¡ {ř8, ‹Ł:œ£ ŁăÛffiù dmesg command£ ¸ľć messageõ Ç¡ –åęř.

ˇ‹ Ăw`Ćt êÓú »čš8 ¸ffi log information message` Is ŻÅăř. bug reportèĆê ¸ mes-

sageõ Łȷè bŸľ sqb ćř.

Ł§Ć kernel’s log message˚ Ž` –ř. řüY ›¸ Ã‹ ,¸ř :

scsi0 : PPA driver version 0.26 using 8-bit mode on port 0x378.

scsi : 1 host.

  Vendor: IOMEGA Model: ZIP 100 Rev: N*32

  Type: Direct-Access ANSI SCSI revision: 02

Detected scsi disk sda at scsi0, channel 0, id 6, lun 0

scsi : detected 1 SCSI disk total.

SCSI device sda: hdwr sector= 512 bytes. Sectors= 196608 [96 MB] [0.1 GB]

  sda: Write Protect is off

Partition check:

  sda: sda1

¸ľć outputù parallel ZIP driveõ `Ţ 1.3.87 system˚ output¸ř. AÝć outputù ŁăÛffi˚ host

adapterY ŁăÛffi¸ řô SCSI deviceõ `ŞL –Ź`Ć 0Ę řjč ,¸ř.

„ńvù host adapterõ æć low-level driver£ Ùâ˚ initialization messageõ vèć ,¸ř. ¸ EÍĆ Ź PPA¸ř. řüvù drive˚ éżAÃ` SCSI busĆt Ň>üŹ ´´˚ deviceĆ˚ ˚ľt ÃLüq Ţř.

Line 5Ź driveĆ ‚`ý device ¸ö¸ ÃLýř. ¸EÍŹ /dev/sda1¸ř. ¸ffiÃLŹ ˇ‹ ŁăÛffi¸ ă#

¸\˚ SCSI adapter, =„˚ driveõ `Př8 ă#¸\˚ t£ \¸ć ?ffi£Ùâ ÃLüq Ş6 ´´˚

sectionù ÌÎÌ \Čć AÃõ jěćř.

ˇcĆ ŁăÛffi¸ ^£Ï diskõ PÌćř8 partition checkĆt /dev/sda4ĘŹ ă#˚ 7/Őú ÃŁ v, ¸ř. ˇ‹ ŁăÛffi¸ řô SCSI deviceõ `ŞL –ř8 ŁăÛffiù ZIP drive` /dev/sdb #Y ›ù řô

device£Ź #Í&řŹ ,ú ¸ľľbˇ ćř. - ŤŠt messageõ checkľb ćř.

ˇc ¸ć vffi¸ Ã¸Ş MŹř8, X|‚` ¿ê˚ hardwareZŹ kernelĆt ffiG zAý ,¸ř. mailú Ã 4§ ;Ć SîSSě3 ?fi YAú check ľÃêÀ ăĘ.

ˇ‹ scsi0: line¸ #Í#Ş MŹ ř8 Ťă8 ¿êù host adapterő Ť,˚ driverõ :<ă3 configura-

tionú ľ sŞ Mù ,¸ř. řô driverŹ ¿êĆ3 X|¸ %źŹŞ hintõ v ,¸ř. ˇc ¿ê˚ driver` detectionüŞ MŹř8 cable¸ ffiGý ,¸ř. ˇ‹ driver ¸ö¸ č¿üŞ MŹř8 ¿êù I˝ê SCSI disk supportõ kernelĆ include èÅŹ ,ú q #}ú ,¸ř.

řô debugging AÃõ æľt kernel source tree˚ driver/scsi 4˚ README fileú œLăL SCSI HOWTO õ œLăĘ.

4.2 Fdisk, mke2fs, mount, etc.

‹ş ŁăÛffi¸ ZIP drive˚ drive ¸öú NL ¸õ ”8qb ćř. ŁăÛffiù ¸ driveõ A\:‚ LINUX

disk management commandõ `ŞL řÛ¡ –ř. fdisk (ZŹ cfdisk)Ź diskĆt˚ partition diskõ řØ

§ æľ PÌýř. mke2fsŹ partitionú ext2 file systemœ£ formată§ æľt PÌýř. - LINUXĆt` $ Gý PÌüŹ file system¸ř. mountŹ formatted partitionú ŁăÛ˚ GW:‚ %ńùý uS£ Ŋ@ă §æľ PÌýř.

ŁăÛffiù ¸ľć toolsĆ [ć man pageõ Ż& WÙõ ăŁbă6 ¸ffiĆ ˛¿ľ Kb ćř. ¸C =`Ş ˚ Is \¸ć version˚ fdisk program¸ –œt£ s˚ľbˇ ćř. #Ź ~`Ş˚ ¯ć è#ýąĆ Âľ z<ú ă9ř.

4.2.1 êSS jȷ˚ %SS¿

$c ŁăÛffi¸ ÙŠ˚ IOMEGA˚ toolsĆ ˚ľ fĄý DOS file structureõ `Ţ ZIP diskõ `ŞL –ř 8 ¸ffiù partition scan\Ćt disk` /dev/sda4 ˚ ă#˚ 7/Őˇú `ŢřL ÃLõ č ,¸ř. ŁăÛffiù ¸ffi diskõ /zipĘŹ directoryĆ mountõ čš8 ¸ćéœ£ ľbˇ ćř.

mkdir /zip

mount -t msdos /dev/sda4 /zip

¸C ŁăÛffi˚ diskŹ /zipĆ ˝Ï!üq Ã‹ ,¸ř. disk` mount üq –Ź ôKĆ ŁăÛffiù Ť,ú C$ăš ľtŹ Kýř. ŁăÛffi¸ diskõ `ŞL ȷz¸ ȷ.ú EÍ Ť,ú umount èÅL release èĹ G W:‚ directory£ Ùâ ÛýèÅ8 ýř.

umount /zip

‹ş ŁăÛffi¸ mountüŹ directory /zipõ ˇffiL #8 ŁăÛffiù řè ¸,ú č ŻÅŹ {œ6 óĆ ř è q%x` mountõ èÅ8 ýř.

4.2.2 ýĄSS£ řè jȷă§

ˇc ŁăÛffi¸ ZIP diskõ ŞÍL Ť æĆ Linux native file systemú ˇffi§õ Ùă8, ; diskĆ ÂăŁ

fdiskõ ľ sqb ćř.

     fdisk /dev/sda

ŤýL ?fi §U˚ 7/Őffiú ŞŒb ćř. (d <žú PÌćř) ŤýL #t n <ž ¸ÌăŁ ^£Ï parti-

tionú ˇffiq sL w <žœ£ žÜPĺú §«ú ăL q <žœ£ ˝Zř.

7/Őú formatćř.

mke2fs /dev/sda1

(Ł§t 1¸Ĺ ¡Ź ŁăÛffi¸ fdiskĆt partitionĆ ÙŁć ěÒ¸ř. ¸C ŁăÛffiù diskõ mountăŁ PÌă8 ýř.

mount -t ext2 /dev/sda1 /zip

(æĆt PÌć mount pointõ řè PÌćř.)

4.2.3 ZIP Tools %SS¿

ŁăÛffiù ZIP driveő ›¸ ąŹ diskõ ¸ÌăŁ Xs` řô ȷzú č ¡ –ř. Žõ ffi8 software con-

trolled write protection¸ `ăăř. ÂÙÛ˚ PŁffiù ¸,ú LinuxĆt PÌă§ æľŁ DOSĆt unlockú

èÇř. LINUXŹ locked diskõ accessč ¡ {ř. ŤýL ¸,ù Iomega˚ toolsú ¸ÌăŁ unlock èĹbˇ ćř. řô X|Ãřê write protection §ă¸ Linux native programĆt O ìÇüqb č ,¸ř.

4.3 %SS¿ Ã4§

ŁăÛffiù disk` mountüq –Ş Mú : eject èÈ¡ –ř. Ç&Ź disk õ eject èÈ¡ –Ź <žq` { ř. diskõ „4§ æľtŹ drive˚ XĆ –Ź buttonú Ďă sqbˇ ćř.

LinuxŹ disk` unlock ü§;Ć 5ŁŢ ?fi ıÒõ ÃŠćř.

^£ù Linuxõ æć ZIP tools programù SCSI and parallel version drive ˚řĆt IOMEGA˚ "żć § ăú ŞÙč ,¸ř. ( software-controlled ejection & write protection)

C 5 < Ů[Y ż

Ł§Ć Íý` ıs ?ăŹ ˚[ffiY żú :q nUř. ¸ffiú řè \§;Ć żú $9 ›q s§ ĘĹř.

5.1 ZIP drive£ Ùâ èSSðú §ôč¡ (booting č¡) –Ź`?

¸,ù ŁăÛffi¸ PÌăŹ host adapterĆ ţš –ř. ˇc ŁăÛffi¸ 5,6ě SCSI£ Ùâ bootingú č¡ –Ź ROM BIOSõ `Ţ host adapterõ `ŞL –ř8 SCSI ZIP drive£ Ùâ booting č¡ê –ř. parallel

port drive£ ÙâŹ booting č ¡Ź {ř.

ˇc ŁăÛffi¸ main diskĆ êSSõ Ó&ăL –L ZIP disk£ Ùâ Linuxõ Ù6ăL òř8 ¸,ù LOAD- LINú ¸ÌăŁ `ăăř. ŁăÛffi˚ kernel imageŹ Łȷè DOS disk˚ q’`Ć U&ăL –qbˇ ćř. ŁăÛffi¸ PÌăŹ kernel¸ ďĘô 4$ driverõ `ŞL –ŹŞ Ý‚ăĘ.

4` IŹ ć parallel ZIP driveĆ jěý qNć ‹Ł:‚ ŢjÆĆê installation boot floppyŹ {ř. Ťă # ¸,ù Linux 2.0¸ #ą8 Ę¸ ,¸ř.

5.2 ů IOMEGAŹ 7/Ő ěÒõ 4ěú PÌăŹ`?

¸,ù `$ ¯ă3 Ů[ăŹ , |˚ ă#¸ř. ăŞˇ IXê ¸Ć Âć <Ýć żú ffiL –ŞŹ Mř. I˝ ê żřô ¸îŹ {ú ,¸ř.

5.3 boot timeèĆ qN3 diskõ mountč ¡ –Ź`?

ŁăÛffi¸ ľb č ,ù /etc/fstab fileú LflsŹ ,¸ř. Žõ ffi8 ŁăÛffi¸ booting èĆ ĺ\ DOS

diskˇú PÌćřL `Aú ă8 řü Y ›¸ /etc/fstab 7‹Ć §«ú ľ uř.

/dev/sda4 /zip msdos defaults 0 0

ŢjÆĆ 0ĘtŹ initialization scripts` fstab Ć §Áý 7/Őú Â\œ£ fsckõ ìśă§ê ćř. ¸ľ ć Pìù ŁăÛffi¸ ˇ‹ bootèĆ driveĆ diskõ Oq nŞ MfiŞ ZŹ řô file system˚ diskõ Oq n ú EÍ [Cõ b§č ¡ –řŹ >ú <îă§ ĘĹř.

5.4 4` ˇ‹ bootè diskõ Oq nŞ Mú EÍ qE‹¸ ŇfăŹ`?

kernelù partition tableú ›úšL èêõ č ,¸ř. ăŞˇ ¸ľć ȷôù è^ˇ /üă3 þ ,¸ř. Ť

ă# %Ač ŻÅŹ {ř. ‹ş ŁăÛffi¸ diskõ OqsL #8 ŤýL #t kernelĆ3 Ť§Ć disk` –œ ę rescanú ăĘL Nš s§ˇ ă8 ýř.

HINT : ŁăÛffi¸ diskõ ĘœšL č: ^£Ï disk˚ partitionú ‚éăêÀ ă§ æăŁ fdisk õ ìś è

Ĺ sŹ ,¸ Is öñć â¡¸ř.

qE SCSI host adapter˚ BIOSŹ bootăŹ ôKĆ 7/Ő tableú ›úšL èêăŹ EÍê –ř. ˇ‹¸ ľć checking YAú disable èĹ nŞ Mœ8 ŁăÛffiù boot YAôK ĺ\ driveĆ diskõ Oq nIb č ,¸ř.

5.5 qE SCSI adapters` ZIP driveő ÒÞ¸ üŹ `...

IomegaŹ ÜÞ¸ üŹ host adapterõ řü˚ siteĆ §Áľ nUř.

<http://www.iomega.com/techs/zip/what063.html>

5.6 parallel driveõ real SCSI disk ˛ď PÌč ¡ –Ź`?

PPA-3 parallel-to-SCSI adapterŹ single ASIC chipœ£t uÇüq –ü IomegaŹ VPI0 õ callćř. ¸,ù ZIP drive˚ controller cardĆ 4$¸ üq –ř. ì&£ SCSI bus` U&ăL –ř. Ťă# îÌć formù I ęř. 4` ~ cards õ üpčšL èêć ĘĆ ˚ă8 SCSI busõ ¡Ù£ Ý$č : ÅuüŹ conventional electrical

buffering circuitsõ VIP0£ Â–ăŹ ,¸ fý:œ£ Ã‚ř.

5.7 parallel driveĆ printõ ffŒ PÌč ¡ –Ź`?

]Á č¡ –ř. Ťă# Ç&ńŞ ŁăÛffiù lpő ppa driverõ ôèĆ ›ù parallel portĆt SSĄÜ èĹ t PÌč ¡Ź {ř. resource sharing protocol¸ Ç& „Ň|Ć –œ6 #§ čL¸ #ő–ř. Ťă# Linux 2.0¸ release ü§ ;ńŹ Ý`ă č ,¸ř. (ŞŽ čLĆtê I˝ê Ý`ăăŞÅ.) @Á:œ£ ˙ľt printerő ZIP driveõ Ŋ@č¡Ź –ř. ŤýL ¸,ú ŁăÛù lpő ppa driverõ loadable

module£t rebootingăŞ ML PÌč ¡ –ř. ¸ľ3 ăL #t ŁăÛffi¸ ˇc printõ ăč Ùćř8 lp moduleú insmod£ load ľbˇ ćř. ŤýL ˇ‹ ZIP driveõ accessčš8 insmod£ ppa driverõ loadľ

bˇ ćř.

]Á ˇc ŁăÛffi¸ ~„˚ parallel portõ `ŞL –L ăŹ printer, #"Ş ă#Ź ZIP driveÌœ£ P Ìú ćř8 %Ač ŻÅ` {ř. şŞ kernelú lpő ppa driverõ ˚ř jěèĹt {7‹ľ s8 ýř. Ť ăL #t :<ć configuration commandsõ kernel command lineĆ jěèĹ s8 ýř. ˇ‹ ŁăÛffi¸

LILOõ PÌăL –L, ŤýL printerõ 0x378Ć ŤýL ZIPú 0x3bcĆ Ŋ@ľt PÌćř8 řü line ú

/etc/lilo.conf 7‹Ć 8`ľ uř.

     append = "lp=0x378 ppa=0x3bc"

5.8 PPAĆt EPP/ECPõ ŞÙľv 3è¸ –Ź`?

ppaŹ ˛üĆ parallel busĆ Âć qNć command protocolY technical specificationê `ŞŞ MLt „Ň

ü}ř. ÂêĆ DOS emulatorŹ protocol˚ reverse engineer£ AÃõ ?ú¡ –êÀ üq –ř. emulatoră Ćt enhaced modeõ ŞÙľsŹ driverõ uŹ ,ù Ý`ăăř.

IOMEGA˚ technical reference manual¸ ¸C ¸Ì¸ `ăăř. ŤýL enhanced parallel port chipĆ [ć data sheetõ üUř. ŤŠt ¸CŹ driver˚ upgrade` `ăăř.

5.9 PPA` IOMEGA˚ parallel port tape driveő ›¸ PÌ¸ `ăć`?

¸ffi driveŹ floppy-tape drive¸ř. ŤýL SCSI` [Łüq –Ş Mř.

== PŁffiù ¸ffi tape driverõ „ŇăŹÚ #˚ Şłú :Ì èÅŹ ,¸ Œy–řL Ş:ř}ř. „ěń şGŹ DOSemu ăĆt ȷôăŹ dos driverõ uŹ ,¸ř. #Ź ĂuĆ3tê ¸ľć Şł¸ ĄWřřŹ m §õ ffiq ÃŞ Gřř.

5.10 PPA` parallel SyQuest EZ135ő ›¸ ȷôú ăŹ`?

Kýř. EZ135Ź ShuttlePort parallel-to-IDE converterõ 4$ăL –Ź IDE drive ¸ř. #Ź ȷôú ăŹ § Æ:‚ driverõ `ŞL –ř. Ťă# sC driver` řĄþ ,‚ŞĆ ÂľtŹ IŤ ŽA¸ {ř. #˚ web page <http://www.torque.net/ez135.html> Ć [îú `K s§ ĘĹř. #Ź @vĆŹ c^˚ őÍ ìSSâõ ŻÅ£ă3 þ,¸ř.

6. Ãř /ê˚ AÃõ uúš8... 10

C 6 < Ãř /ê˚ AÃõ uúš8...

#Ź #˚ home pageĆ ĺ\ /Ű˚ updateý mini-HOWTOõ îŞ č ,¸ř.

<http://www.torque.net/zip.html>.

Ãř ‹Ł:‚ ZIP FAQ web oage` îŞüL –ř. (XÌ Macintosh:‚ >ľĆt)

<http://earth.cnct.com/home/steveg/zip.html>.

Iomega˚ web pageê œLă§ ĘĹř.

<http://www.iomega.com/>.

ŤýL ˇ‹ parallel port programmingĆ ÂăŁ XÌ ‹Ł:‚ AÃõ Ùćř8 řüú Ş[ľ Ã§ ĘĹř.

<http://www.lvr.com/parport.htm>