SSM ýĄSS N7 čL zX K4t

XĄ ŹŠ!SSq 1čÖ ýĄSS PÌß ?`

A £ ¡

1998[ 9Ú 22¡ #Æ

@ ò

i

C 1 < "�

řüù SSM ýĄSS zX K4t¸ř. Ç& SSM ýĄSSŹ N7 "êÌˇ –œ6 >;:œ£ Ã ˛ľ #¨ ŽA¸ř.

SSM ýĄSSŹ §U˚ Ű[ łȷŕ ýĄSSĆ Nă3˚ ¸ˇÌńY ě£ôńÍt ˇȷê´ [ CÅŞffiú Ã˛ăL, XĄ ŹŠ!SSq 1čÖ˚ ssmLUGĘŹ Ź?„Ćt §U˚ ¸čľń Ít ˇȷê CÅŞõ jěć ,¸ř.

Ç& ýĄSSÌ CÅŞffi| ˘ù ÙÛ¸ ‚ïÌ¸¡Ćê N7Ì, SS8Ì, 7ŒPCÌ¸ –œ #, ‚ïÌú C¡ăLŹ N7Ì¸ Sê:œ£ ˘¸ ˇffiq ŞL –ř. Ç& ýĂSS ùŇŃõ üÅăŁ ýĄSS vGú Cȷ|‚ ˘ù ýĄtffi¸ N7 "êú YÌăL –qt, N7Ì CÅ Şffi¸ Xœ£ XÌ ˘¸ ˇffiqŮ ,¸ĘŹ §Âõ ľÆř.

N7"êú fSăÏ %ŞÐP` {Dœ£ Jq^ řüĆ, Íý#Ę˚ XĄĆt N7_ f SĆ îýć LŞõ òŞăL –qt Íý#ĘĆt˚ N7 "ê˚ SSÌê` mIŮ ŁŞ`˘ ù " ăř. {Ňâ -?ýĆt řŢ ;ı §Á¸ ČGĆt /L£ ˇòřŹ N7_ zG §Á £ Ň;č ¡ –"¸, ŹŠ!SSq ÛbĆtê ŤôK ‚ïGŐĆt řŢ §Á¸ N7 ýĄSSĆ t äŸŒ Íý#Ę` N7_ fS< IęĘ Ť §Ł ŹŠ!SSq ÛbĆtê ČGõ Xt#¨ ¡ –œ8 ^9ř.

C 2 < N7"êY zX Pj

Íx N7"ê¸ qE,¸ –#õ è U_Ã8 řü 3`Ş` –ř.

ffl N7 tč N7 tč 800, 4000, 8200# ˛şć §ă˚ tčÌ {Ňâ¸ř. „‚:œ£ N 7 tč 4000ú ˚ÎŹÚ, Ű 2GBĆ –v Š£ČtĆt ¿ł¸ ÙN{Ňâ Ąă˚ 1/10A ê˚ Ąăú ;}ř.

ffl N7 Œ¿SSì¸Ő N7 SSì¸Ő 200/250, 400, 500, 600, 600A#Y DEC 200 AXP, 300 AXP#¸ –œ6, Żı` PÌľ ÃŞ Gć §[œ£ s£ Œ¿SSì¸ŐÌœ£ #č " ăř. ffl N7 PC N7 PCŹ 164, 164LX, 164SX#¸ –œ6, N7_ 21164ő 21264õ ˚t ˇfi ,œ£, XĄĆt %ŞÐĆt OEMœ£ ˇffiL –Ź §[ffi¸ř. Ç& SSM N7 ýĄSS õ ˇffiL –Ź N7"ê¸§ê ăř.

Ťď N7 ýĄSSĆt ŞÙüŹ ăȷSSq PÌú Ã8 řüY ›ř.

ffl AlphaPC64 (Cabriolet, Aspen Telluride) ffl AxpPC133 ffl EB64++ (Aspen Alpine) ffl EB66 (Neko Tech Mach 1) ffl EB66+ ffl EB164 ffl Jensen ffl AlphaStation 200, 250, 255, 400

ffl Alpha-XL, Alpha-XLT

ffl AlphatPC 164, 164LX, 164SX

Ç& GŽľt N7 êCĄ¸ #ąL –œt£, æ˚ ýSS!` GŽ Ã˛þ ¡ –ř.

C 3 < N7 łȷŕ ýĄSS˚ zX

N7 ýĄSS˚ zXŹ #§ YAˇ c^ řòL ‚ï ýĄSS zXő ô‹ăř.

Íx N7 ýĄSS` ‚ï ýĄSSő řô >ù N7 ýĄSSĆtŹ ‚ïĆt 5Ź LILOõ 5Ş ML N7 RSSq` ?fi ,ú ă3 üŹ >¸ř. Ň N7õ Ù6ăL #8 EEPROMĆ t RSSqõ ›qffi¸L, ¸ RSSqĆt ÏŰ–Cõ Ýăffi¸3 ýř. N7 ýĄSSÌ RSSq £ MILO(MiniLoader)` –œ6, %ŞÐ îğSSÌœ£Ź SRM Şİ, MS èêÍŃNTÌœ£ Ź ARCŞİ¸ –ř.

N7 ýĄSSõ zXă§ æľtŹ §U˚ Ù6 %SS¿ő Ø! ¸yŞ ¸¡Ćê Xt z<ć

MILO ¸yŞ` –qb ćř. Ň uüľbč Ť£Ÿ %SSĘ¸ 3$‚Ğ¸ř.

ffl MILO ¸yŞ

ffl vG (Ù6 %SS¿) ffl Ű %SS¿ (Ø! %SS¿)

ı, Ťď æ˚ MILO ¸yŞő Ù6 %SS¿, Ű %SS¿õ ˇffiq Ãı. ŤćÚ, N7 "ê˚ §[Ć 0Ę MILO ¸yŞő Ù6 %SS¿õ PĘ}băŹÚ, ´ §[Ć 0ô MILO ¸yŞő Ù6 %SS¿Ź řü vő ›ř.

Family/Model Alias MILO Image Boot Image JENSEN N/A jensen-s DECpc 150 JENSEN DEC 2000 Model 300 JENSEN DEC 2000 Model 500 CULZEAN ALCOR xlt-alcor alcor, alcor-s AS 600 ALCOR AS 500 5/3xx MAVERICK AS 500 5/5xx BRET

XL-300 XLT XL-366 XLT XL-433 XLT

XL xl xl XL-233 XL XL-266 XL AVANTI avanti, avanti-s xl AS 200 4/* MUSTANG AS 205 4/* LX3 AS 250 4/* M3 AS 255 4/* LX3+ AS 300 4/* MELMAC AS 400 4/* AVANTI

Family/Model Alias MILO Image Boot Image Personal Workstation MIATA miata, miata-s miata PWS 433a, 433au PWS 500a, 500au PWS 600a, 600au

SABLE AS 2100 4/xxx SABLE N/A sable-s AS 2000 4/xxx DEMI-SABLE N/A sable-s AS 2100 5/xxx GAMMA-SABLE N/A sable-s-5 AS 2100 5/xxx DEMI-GAMMA-SABLE N/A sable-s-5 MIKASA AS 1000 4/xxx MIKASA N/A mikasa-s AS 1000 5/xxx MIKASA-PRIMO N/A mikasa-s-5 NORITAKE AS 1000A 4/xxx NORITAKE N/A noritake-s AS 1000A 5/xxx NORITAKE-PRIMO N/A noritake-s-5 AS 600A 5/xxx ALCOR-PRIMO N/A noritake-s-5 AS 800 5/xxx CORELLE N/A noritake-s-5 RAWHIDE N/A rawhide-s AS 4000 WRANGLER/DURANGO AS 4100 DODGE AS 1200 TINCUP

Family/Model Alias MILO Image Boot Image ALPHABOOK(laptop) ALPHABOOK1 N/A alphabook1-s NONAME udb-noname noname AXPpci33 NONAME

UDB MULTIA EB64+ EB64+ EB64+ eb64p eb64p AlphaPC64 CABRIOLET cabrio cab, cab-s AlphaPCI-64

PC164 AlphaPC164 PC164 pc164 pc164 AlphaPC164-LX LX164 lx164 lx164 AlphaPC164-SX SX164 sx164 sx164 EB164 EB164 eb164 eb164 EB66+ EB66+ eb66p eb66p EB66 EB66 eb66 eb66 TSUNAMI

DP264 GOLDRUSH N/A dp264-s TAKARA TAKARA takara takara

3.1 MILO, BOOT, RAM %SS¿ ˇŒ§

řü 4Ìù ssmLUG˚ ěć¡ń¸ 5ê “RedHat zX%SS¿ ˇffi§”˚ 4Ìú ^8š Æ, ¸ř. ŹÅý %SSĘù 1.44MB 3$¸6, „ %SS¿Ź ‘MILO’, ~ěńŹ ‘Boot’, ČěńŹ ‘Ramdisk’ ¸ř. ¸| MILOŹ DOS Format œ£ ÄP` `ăăL, #"Ş ~„Ź Linux jȷ¸ř. ȷĄŞłù řüY ›ř. (AlphaPC 164LXõ §uœ£ ě.)

ffl disk1

1. êSS jȷý 1.44MB 3.5” %SSĘú uüě

2. RedHat˚ CÅŞĆt milo %ńùý£ ¸ô

3. êSS‹ EÍ v—ȷĘ‚Ćt “copy linload.exe a:” ă6, ýĄSS‹ EÍ v—ȷĘ‚ Ćt “mcopy linload.exe a:” ( “A” drive Ć %SSĘú Où EÍ) ĘL «şăL ì ś 4. êSS‹ EÍ v—ȷĘ‚Ćt “copy lx164 a:milo”ĘL «şăL ìś ýĄSS‹ EÍ v—ȷĘ‚Ćt “mcopy lx164 a:milo”ĘL «şăL ìś

ffl disk2

1. 1.44MB 3.5” %SSĘú uüě

2. RedHat˚ CÅŞĆt images %ńùý£ ¸ô

3. êSS‹ EÍ v—ȷĘ‚Ćt “rawrite”ú ìśăL «ş7‹ú lx164£ ˇ ýĄSS‹ EÍ v—ȷĘ‚Ćt “dd bs=18432 if=lx164.img of=/dev/fd0” (bs=block size Ź "Ać ¯ú ŞAăŞ MIê ß)ĘL «şăL ìś

ffl disk3

1. 1.44MB 3.5” %SSĘú uüě

2. RedHat˚ CÅŞĆt images %ńùý£¸ô

3. êSS‹ EÍ v—ȷĘ‚Ćt “rawrite”ú ìśăL «ş7‹ú ramdisk.img£ ˇ ý ĄSS‹ EÍ v—ȷĘ‚Ć “dd bs=18432 if=ramdisk.img of=/dev/fd0” ĘL «ş ăL ìś

3.2 N7 ĘffąSS zA

¸C MILO %SS¿ő Ù6, Ű %SS¿` ˇffiqPœ8 N7˚ Ę¸ąSSõ zAľbćř.

1. zAÅ(F2) Ăò§

N7 "ê˚ ;Ùú Ĺ8 Űú #§ÜăL, AlphaPoweredĘŹ £Lő ěÍ ´[ èSSð Ć [ć AÃ` #čř. ¸: Ü8 ĚĆ F2õ Ăò8 SETUPœ£ ffiq^řŹ vè` – ř. Ù6|Ć F2õ Ďăt zAœ£ ffiq^ř.

2. OS Selection zAă§

¸C zA Ü8Ćt #Í( ,¸ř. ¸: ÜUvõ ¸ÌăŁ -Śõ ¸ôč ¡ –ŹÚ OS

Selection-Ś£ ffiq` Ã8 Windows NT -Ś` –ú,¸ř. Ł§t řüY ›¸ -Ś

õ ˇfiř. (`$ æ -ŚĆ –Ź ,¸ ıôœ£ Ù6üŹ -Ś¸ř. ŤýL, ýĄSS ;Ì œ£ 5š8 Windows NT-Śõ ŞÍêÀ ăı.)

Boot Name: Alpha Linux 5.1
Boot File : A: \linload.exe
OS Path : CD: \milo
OS Options:

3. MILO %SS¿õ OL Ù6ćř.

¸C -Śõ ˇffi}œ8 ;Ùú Å8, Ù6ó Íý` ˇfi Alpha Linux 5.1 ¸ĘŹ -Ś ` Ã‹ ,¸ř. 3.5” Ť£Ÿ %SS¿Ć yý uüý MILO %SS¿õ OL, ¸ -Śõ xØ ćř. 4. Ù6ă§

¸C MILOĘŹ ŠÃŠ!` v,¸ř. ¸: MILO %SS¿õ „4L yý uüć Ù6 % SS¿õ 3.5” Ť£Ÿ %SS¿Ć OL MILO ŠÃŠ!Ć řüY ›¸ XL Ù6ćř.

MILO> boot fd0:vmlinux.gz root=/dev/fd0 load_ramdisk=1 prompt_ramdisk=1

5. Ø! ¸yŞ OL ýĄSS zXă§ ¸C Ù6| Ű %SS¿õ OœĘŹ -èŞ` #ą8 Ù6 %SS¿õ „L, Ű %SS¿ő N 7 ýĄSS CDõ OL ýĄSSõ zXćř. (¸CÙâŹ ‚ïĆt˚ ýĄSS zXő ô‹ă ř.) ¸: ›˚ ıô Ù6ú ă§ æľt FATŰŃ¸ ŻÅćÚ, ýĄSS zXè ˛ü 7/Őù FATœ£ ăL, 6-` Aêõ zAćř. ¸,ù N7 Ę¸ąSS` FAT¸# ISO9660 7‹ Íéˇ ›ú¡ –§ :[¸ř.

6. FAT ŰŃĆ MILO ¸yŞ ÄPă§

¸C èSSðú řè 3.5”Ť£Ÿ %SS¿Ć MILO ¸yŞõ OL ýĄSS£ Ù6ćř. (Ø! %Ę¸SS` sda5ĘL `A)

MILO> boot sda5:vmlinux.gz root=/dev/sda5

ýĄSS£ Ù6ćó řüY ›¸ 3.5” Ť£Ÿ %SS¿Ć MILO ¸yŞõ OL MILO ¸y Şõ FATŰŃœ£ ÄPõ ăŁ, Xœ£Ź Ť£Ÿ %SS¿ÂêĆ ¸ FAT ŰŃú ¸ÌăŁ ıô Ù6ăêÀ ćř.

# mount -t msdos /dev/sda1 /mnt/floppy
# mcopy a:* /mnt/floppy

7. ıô Ù6 zAă§

¸C N7 Ę¸ąSSĆ ıô Ù6ăŹ -Śõ ˇffiq nı.

æĆ z<ř"¸ OS Selection -Ś˚ C‹ „ěń -Ś` ıôÙ6üŹ -Ś¸6, ıê ¸ zXć ýĄSS Ø! %Ę¸SS` sda5¸8 řüY ›¸ zAćř.

Boot Name: Alpha Linux 5.1
Boot File : Disk 0, Partion 1 \linload.exe
OS Path : CD: \milo
OS Options: boot sda5:vmlinux.gz root=/dev/sda5

C 4 < ÆŹ �

ssmLUGĆt N7 ýĄSS Š£D!õ ŢśăŹ YAĆt ˘ù Ûffi˚ êÓ¸ –}ř. ˛ü¸

Š£D!õ u\ăL 8Ţăê ěć¡ńY ¸y \¿ÙÛ N7 ýĄSS Ţj:ú ˇffiq nœê ¸čľńY Š£D! |^Ć ¸y Nă3Ćt öñć ćŸ N7 ýĄSS CÅŞffiú ˇffiq n œèL ¸,ffi˚ PÌú ťĞľ sê ě£ôńÍ ˇPõ ȷ^ęř.

œL t:

[1] Alpha Linux zXő SSÌ, ćôõ, ýĄSS Úȷ, 1998[ 2ÚÒ

[2] http://www.redhat.com/alpha, łȷŕ N7 ýĄSS ŒW¸Ş

[3] http://www.aztarnet.com/¸axplinux, N7 ýĄSS ŒW¸Ş

[4] http://www.digital.com, %ŞÐ ŒW¸Ş

[5] http://alpha.secsm.org/alpha, ssmLUG N7 ýĄSS ŒW¸Ş

[6] XĄŹŠ!SSq1čÖ ssmLUG DB, ěć¡

[7] ssmLUG C 1ç Čy# , ¸čľ