4$ ćŞã �vG - Kernel compile ¸ŚÒ

Prologue... K‘ăČÅ.ýĄt ŁăÛ ˇ#t Ł˘åęř. ŞŽÙâ ŁăÛY ěÍă3 üq Ł˘uÅ. ŁăÛĆ3

˘ù êÓ¸ ü}œ8 ęęř. $9 vG {7‹ú ˛ü ?ăèŹ Ûffiú |îœ£ ŢśèĹ #`9åęř. @ ò ˛üÙâ vG{7‹ú CX qšŒăì ŻÅ {åęř. vG{7‹ù XŞ Öåęř. ýĄSSê ˛ü zXč :Ź qůŞˇ IXf´{¸ ‹şćě ŕL#8 Ť řüÙâŹ ıêˇ˚ zXŠ£ŤŰú PĘ zXľt #ˇ ˚ ýĄSSõ ŕ "¸ {7‹ê ˛ü IXf´{¸ ‹ş ăèŹ +ęř. ŤýL I, gŞŹ CĘê ¸ľ3 ŤB üŹu#.ăL ŮffŹ +ęř. ćěĆ ř IŹ ,ù Xý«ęř. ŤB IX Ùž {¸ Š£ŤŰ ŕ"¸ ŤB ć ě ľÃŹ+ęř.ćěľÃL Ť řüÙâŹ ŁăÛ˚ DjĆ ”3 N”3 ŻÅć,ˇ PĘt {7‹ăèŹ + ęř. ..”kernel compile 31”..PĘ#Ź &y` –řL# čńÅ.^^;;

ŁăÛ¸ xØć ,¸ ŞÜź¸8 ŁăÛ˚ ýĄSSŹ /˛˚ ŞÜź tč` üŹ,¸L,ŁăÛ¸ -SSvł¸ .ú xØă8 ŁăÛ˚ {ŇâŹ /˛˚ -SSvł¸. tč` üŹ ,«ęř. \áĆ 0Ę ffiG xØăL ă 8 286œ£ ˛#þ ¡ê –Şˇ......-.-;; ]Á ˛ü ăŹ „ {7‹ù ˛ü ?Žè vG č;ˇ zŤł¸ȷý Ů fflĹĆ G Ůff9Şˇ ˙«ęř. ăŞˇ Ť „ {7‹ĄW˚ §Fù ŁăÛĆ3 ýĄSSĆt ŮffŞ GřÏ < Ł˚ §Fú Ůff3 ľv +ęř..(^ ^);; {7‹ú ĺ\ ýĄSS˚ ˝Ş˚¸ĘL f´ăèŹ Ûffi¸ ˘åęř. ýĄSSŹ qŮ, $9 èȷľê &y–åęř. ı ¸C ŁăÛ˚ {ŇâĆ /êč;˚ kernelú {7‹ ăêÀ ă9åęř. ŁăÛ˚ ýĄSSĘŹ ŽĆ ^£Ï Zuõ ÚščřL f´ăè8 `ęř. ı Ťď.ready..Go!!

˛üÙâ ¯&ffi ˙ăŹ tč˚ /:Üõ æć {7‹ù f´ ˝ČÅ. ‹ý čê ć (üÙâ ‹ş qN3 ü ŹŞ ćě ľÃL řè ľÃŹ +ęř. œL£ ¸ěĆ {7‹č č;ù 2.3.8 Ň, „Ňč;«ęř.

Iœ ¸ě ˛_Ź ŤB ¸b§ă"¸ č ,«ęř.. ˘ı§ vG¸ gŞ` #ąL „Ňč; KAč;¸ ˘ı § #ąL CX` fL ###... IX Íé {¸ č ,«ęř..ů=8 Íý` ăŹ ýĄSSŹ &y–qb ă$ fiÅ.Ť& C f´¸§ê ăuÅ...

1.vG¸Ĺ? 2.„Ňč;,KAč;¸Ĺ? 3.CXĹ? 4.ŹSS Ń§ .. ..

źŞ þĆt ˘¸Æ ¸ć ÍŒ˚ Íé¸ IęĘ ŁăÛY IXÍé{¸¸b§ ă"¸ ăšL ęęř.|Åć, ù ffi Aýý þ@ò˛ď¸Iĺ {7‹¸ gŞ ŁăÛ¸ ˇˇ SŽˇ !IsèL {7‹ú SŽ¸Ęê Ö3 Âăì¡ –3 ýř8 9Ź Ť ¸\˚ §Fù {ú ,«ęř...(^ ^);;

ŁăÛY Ő$Ï vG{7‹ Ő`óĆ ŁăÛ¸ ”ˇ !U œ” êÚ£ řè ŁăÛ¸ N”3 řè ffi Aý ăŇt ÙTć ,¸ –œ8 Ì “`ľt řô ÛĆ3ê vG{7‹ú Ö3 ?Űč ¡ –3 ľsèL ÌÎÌ “ `ľt ÌÎ )Ţ [t` üq ;v˚ ýĄtĆ3 SŽ¸#˝ êÓ¸ ýř8 ÌÎ §C9o. ›Ć Ãè8 N9 Şˇ A˙ XéăřL ŁăÛ¸ ˙;ăì Aê£ #make menuconfigč : #ąŹ -Śõ ř :}åęř..^^;; Xá 4Ì‚Şê ?òŹ -Śê ¡{¸ #ąŞˇ ř :ù ¸îŹ X|¸fiŞ qN3 f§L f` –ŹŞ ?ò Ź \ŒĆtŹ ?Űă§` *ffi$fiÅ.vG{7‹ù ă§ íŞˇ f` #ąŹŞŹ ŤB ćě ÃL òùÚ ü IÌê f` ffiq–řL #ő–Ź [t ü§ê *ffiê YAú Ãš8 ¸0` #ą9Şˇ ¨¿ ŞÍL ^£¨ ¿ ˇffiê Şˇ ffiL éÃ§ {YL ....###ľt #make menuconfigăŞ Mœ8 Ç ¡ê {§Ć IŽ IŹ ,ù {Şˇ ˛ü {7‹Ć ?ŰăèŹ ÛffiĆ3 Ťć Lf KăL ćě uEˇ¸Ęê č ¡ –3 ă§ æľt Ţåęř.. ˘ù êÓ¸ þ Ů ?ò9Şˇ ˙«ęř...ŤŠt ŤÛffi¸ ,,,I..{7‹č: ¸ć -Śffi¸ #ąL I..4 PÏȷ bȷ` ¸ @ÀĆ –L...I ¸,ú zXľb 4` ÙăŹ,¸ ü9u#ăL [tˇ ŤB uEˇ

¸Ęê ľt {7‹ üSSXýă3Ęê ^?:œ£ ?Űč ¡ –êÀ ăLı řœ8 ăŹ ĘŰĆt ¸ľ3 X éăL XŞ˚Şă3 ř :qÎåęř....(^ ^);; ýĄt˚ ć PŁœ£t C` Lfćěľt Xéă3 ř : qnœ8 {7‹ ffi ăèŹ Û¸ Ăw`Ć3 z<ľv: ŞŽ ¸ ŸĆt ŻÅÙÛˇ bŸľt ÈŸţI żž ľ sè8 ˛ü{7‹ ăŹ Ûffiê XÌ Ö3 ¸ľăL żžăèŹ Ûê ĘCê Ú ‹‹¸ ř ŸŁõ ȷĄ K ăŇê üL č , ›It ćě ľÎåęř.....A˙ Ťľ3 êÓ¸ þŞ ?ò9Şˇ ˛üăèŹ Ûffiù q%` q’Şê ffi ?ò$fiÅ..9ê ŤŹL,,,

¸ć Íé¸ ‚Ć KȷèŹÛù 9 IŠ XȷA IXf´{¸ 0Ęă§£ Ę£ `Ňê `ęř..

linux-2.3.8.tar.gz

¸,ú ÃLt kernel Y „Ňč;¸ sýõ SSZ Ûù ğ˚ <Ł˚ ĄW«ęř.. kernel P;: ˚y£Ź ”N ȷ¸, Nfi¸”ĘŹ y«ęř.. Ň ýĄSS NăŢ§` Ę£ vG¸ĘŹ y«ęř.. PŁ˚ î$Y ›o...PŁ¸ î$¸ lŞ Mœ8 U¡ {"¸ ýĄSSê vG¸ Ù6üŞ Mœ8...-.-;;; Ł§t vG¸ ýĄSSČGĆt qE ČÙ:‚ §ăú ăŹŞŹ Ł§x ˙Kă9ýęř.Xœ£ Ł§9§t Ťć îąć ˚yŹ ¡ê {¸ ffiœęń Å...Ł§t ŤB ýĄSS˚ î$¸ĘL ăo....ıL–Ź ^Ňú ůÍŹ......

2.----;ŋÁ ĺÿŋÍáĺÍáşĳ ęÈčÖÞłÆ kernelňź řÛá ĺÏáş¡ąť ňÝñňÛå ěţ ňÑåęťąÉîčÈďť..

ęÈčÖÞłÆňźłÿ şÔÞąÈŋÍÞňÝá ňÿěÍá ąÈčÛòďÛåňÈ ŕÁąťď£ğÏá čţňÝåňÈęťďĳ ňÈąÍðňÛá 3.ňÆęĳ ąÉîčÈďť...

3.----:şÑå,őÉÞ,şÑå,őÉÞ,,,,,,řÿšÛå, łÉíąÉÞąÒáąż, řÿšÛå, łÉíąÉÞąÒáąż....-.-;;

ğÉå ąÆďţęĳ őÉÞłÁčÛá ňÉáŋÍòĺÿŋÍáňź ĺÖöňžŋÝîčÈďť..2čť 4čť 6ďÛò őÉÞłÁęĳ ŋÑáŋţşÉå ěţčÛá őÉÞňÈ ğÉóňťłÿ řÿšÛå(couple)ŕÿęÍí ňÉáŋÍòŋÍÞňÈŋÈğÉá şÑåłÁ 3,5ŕÿęÍí,, şÑåłÁčÛá łÉíąÉÞąÒáąż...-.-;;łÉòďÉòşÈ ĺÖåňÉáşťŋÀ ňť,,ą£ęÑîďť..şÉá ňžŋťňź ďÁčÉíŋť....ĺÖåňÉáşÉá şÏáłÝåňÛå śťšťşťęžąĳ łÝåşÍíŋÍÞňÈąĳ ğĳşÍíŋÍÞňÝá şÊòďÑòňÛå ğÉãňÈ şÉîčÈďť..ňÏáňÝáňÇ ğťňÛíňÛå łťęĳŋÉîąÈ ňÄşţłÿ ğÉåňÝîčÈďť...

ŋÉåď£ğÏá ňÉáŋÍòĺÿŋÍáňÝá őÉÞłÁ řÿšÛåęĳ ňÑåęťąťłÿ ňÉáŋÍòŋÍÞňÝá ňÏáňţłÊòşÒåňÛå şÉå łÁ ňÝñňÆčÈćťňÀ..^^;;

ňÈęţłÿ şÑåłÁňÝá ąţĺÉåĺÿŋÍáňÛá łÝåşÍíŋÍÞňÈęťčÛá ğÖáąÁąť ğÉãňÈ ĺĳňÝîčÈďť..

8.----:ňÏáňÝáňÇ ğťňÛíňÛå łťęĳŋÉîňÆęžąĳ łÉíąÉÞąÒáążň¡ ąÉöňÛá şÑåłÁ ĺÿŋÍáňÈ ďÔáňÈşÁ

ğĳşÍíŋÍÞňÝá ďĳŋÍáňÛå 8ĺÍá şÊñďťčÛá ěÛðňÝîčÈďť. ŋÉåď£ğÏá 8ňźłÿ ąÆŕÝå łÁďĳ ňÝñąĳ ňÉáď£ğÏá ą¡ąÿ 1.3ĺÿŋÍáŕÿęÍí 100ĺÍáňÇ šţŕÈęÛå ąÿŕÝåłÁďĳ ňÝñčÛá ąÍðňÝîčÈďť.

¸C IXf´{¸ XS& {7‹ 0Ęă§õ èȷă9åęř..

ş S&¸ –åęř...

1.XS& 0Ęćř.IXf´{¸....<Â ů ¸ľ3 <ž 4ýŹŞ NšL ăŞ MŹř. (ŤľřL GŽù Ię LÅ...˛üˇ...^^;; ]Á {7‹ “ ăèŹÛffiˇ,, óŁÙĆ ůŤć<žú 4źŹŞ ř z<ľ ȷ`ÍÅ.. Ť ýL Şłê Łă `Ş¸# ‹şù ă#$9ľÃL XÌ řò3 ‘ă3 ăŹ Şłú IèŹ 3 ^åęř.....)

2.Nă 5.2` ŕß \Œõ `Aœ£ èȷęęř. (6.0č;ù qŮ $# \[{åęř...5.2Ćt Ę£ 2.3.8£ L šč3 –$fiÅ) XĆt ˙;ȷź"¸ ˛ü Ûffiú æć ˛_§Ć řŹ CX ČČć Ůffl¸ ȷèŹ ÛÍŹ j ľõ uęęř.. ˛ü ?řú :˚ ıê˚ ?åú f´ă8t....(^ ^);;

3.{7‹ȷzè ȷz$Ź` \¿& |Åă$fiÅ..ŤŠt PromptĆ ıôœ£ Ç&˚ - %ńùý` #ąêÀ 7‹ă#õ &ȷý9ýęř. ĺ\ æXõ Ý‚ľb ă$fiÅ..˛üč:Ź... ]Á IXf´{¸ vi£ ŐL ¡A ăL #|Ć ¸ľăêÀ ă9åęř..

4.make menuconfig õ PÌč ,¸§ :[Ć ncurses` zXüq –ŹŞ Ý‚ęęř. {ř8 ýĄSS zX CD

õ mount ăLt zXęęř.

5.$9 /usr/src IŠĆ kernel /êč;‚ linux-2.3.8.tar.gz õ `êĆt ŃÏ,äĆt ŃÏ,cdĆt uăÏ ľt æ %ńùýĆ uüèÇř.

@ ò 3

ftpňÝå ąÏòňÁ ---ftp.kr.kernel.org

              ftp.bora.net
              updates.redhat.com

webňÝå ąÏòňÁ ---ftp://ftp.kr.kernel.org

              ftp://ftp.bora.net
              ftp://updates.redhat.com

-->ğĳďÁ pubęĳąťłÿ /linux/kernel/v2.3/linux-2.3.8.tar.gzęÛå ąťŋžňÑáďť...

IŠ Ţś èĎ ncftpŠ£ŤŰú `ŞL ftp£ ?Žè Žõ ffi9åęř. ”|Åć ,ù IX f´ {¸.....(^ ^);;......Ùž {¸....” ıŤď....Ù6èȷ...!!

 login: root
 passwd:********

"linux is fun...hi..kyuho!!"

[root@zzem /root]# cd /etc

[root@zzem /etc]# vi profile

-----------------------------------------

ňÉáňź ďÛåňÿąťğÏá

PS1="[\u@\h \W]\\$" ňÈ ĺÁĺÖáňÈ

ňÝñňÛå ąÍîčÈďť...

ňžąÈłÿ ďţğÖáŋť WęÛå łĳğÖáŋť węĳ ĺťćÂŋÁłźňÀ. ąÆęÈąĳ,ŋÿŋÉòşÁ

:wq
-----------------------------------------

[root@zzem /etc]# source profile

[root@zzem /etc]# cd /usr/src

[root@zzem /usr/src]# <----ŋť ňÈŋź

ňÈďÑòşÉá šÖå ąÏòęĳąť ĺĳňÝåąÍðňÈďť....^^;; ŋť ňÈŋź ŋÍîłÑÞşţłÿ ĺÉäňťňĳŋť ,łĳłÆęÛå....

[root@zzem /usr/src]# ncftp ftp.kr.kernel.org

@ ò 4

Guest login ok, access restrictions apply.

----------------------------------------------
ftp.kr.kernel.org /
----------------------------------------------
kr>ls
kr>cd pub
kr>ls
kr>cd linux
kr>ls
kr>cd kernel
kr>ls
kr>cd v2.3
kr>ls
kr>get linux-2.3.8.tar.gz
kr>q ěĳčÛá exit

[root@zzem /usr/src]# ls (ňÉœňÆęĳ ğÏòęÏòčţęÈąĳ ls ęĳ ňÿěÍá ĺÏáş¡ąť

łÊòąÏñčÛáŋÈ şÒÞňÝáşÉáďť..ňžąÈłÿčÛá ŋÈğÏáłÉò łÊòęËÞşťčť ňžęÿĺÖáňÛá ćÑÞ şťłźňÀ..^^;;)

[root@zzem /usr/src]# rm -f linux

[root@zzem /usr/src]# mkdir linux-2.3.8

[root@zzem /usr/src]# ln -s linux-2.3.8 linux

[root@zzem /usr/src]# tar xvzf linux-2.3.8.tar.gz

[root@zzem /usr/src]# cd /usr/include

[root@zzem /usr/include]# ll asm linux scsi

[root@zzem /usr/include]# rm -rf asm

[root@zzem /usr/include]# ln -s /usr/src/linux/include/asm-i386
               /usr/include/asm

[root@zzem /usr/include]# cd /usr/src/linux

[root@zzem /usr/src/linux]# make mrproper

[root@zzem /usr/src/linux]# make menuconfig

[root@zzem /usr/src/linux]# make dep

[root@zzem /usr/src/linux]# make clean

[root@zzem /usr/src/linux]# make bzImage

@ ò 5

[root@zzem /usr/src/linux]# make modules
[root@zzem /usr/src/linux]# make modules_install
[root@zzem /usr/src/linux]# cd arch/i386/boot
[root@zzem /usr/src/linux/arch/i386/boot]# cp bzImage /boot/mykernel-2.3.8
[root@zzem /usr/src/linux/arch/i386/boot]# cd /etc
[root@zzem /etc] # vi lilo.conf
---------------------------------------------
timeout=100
image=/boot/vmlinuz-2.0.36-3kr
           label=linux
           root=/dev/hda6
           read-only

ąÈŋÑáňź ŋÑáŋţşťčÛá ňÄŋÍòĺĳ ňťęţňźďť ňťęţň¡ ąÉöňÈ ŕÍíąťşťąĳ ŋÿŋÉò..

image=/boot/mykernel-2.3.8
           label=mykernel
           root=/dev/hda6
           read-only
---------------------------
[root@zzem /etc] # lilo
Added linux *
Added mykernel
[root@zzem /etc] # reboot
....
........
..........

ŋţĺÁśÝòşÁ

lilo : čťňĳğÏá Tab řÈęÛå ŕžĺÑáďť..
-------------------------
linux mykernel
lilo : mykernel

...

...

...

...

...

AlzzA Linux release 5.2a ( Linux, the Rising Sun)

Kernel 2.3.8 on an i686

zzem login : _

¸,ú Ã8t vy¸..... (^ ^);;¸ľ3 ýř8 ĄW«ęř. ¸C ŁăÛ˚ ýĄSS ćŞãIŠĆ ~„˚ vG¸ U&ă3 ü}åęř... ş ŞŽńŞ˚ YAù IXf´{¸ qE YAú $X# Æ ,¸Ę |^Ć Ł ăÛ¸ qE zAú ľs}Ů=Ć 0Ę ˚˛ýĄSS` ýÛê Gì ,¸L ›^ýĄSS` ý Ûê Gì ,«ę ř. ăŞˇ |Åć ,ù ŁăÛù ¸C ”{7fi”¸ IęĘŹ +ęř. ¸CÙâŹ XÌ řjć ŞłY ıê˚ ” Ź ĺ@ú PĘ GŽ:œ£ {7‹ ă8t ŢÍř Ã8 ŁăÛù qŮ^ {7‹ìş¸ \¿& ďĘ` –Ź , ú Ůffi ,«ęř. Zć ŁăÛ˚ ýĄSS` ˛ľŞL ˙ĘŢ ,ê Ůffi,«ęř. ŤýL ŁăÛ˚ ýĄSSĆ ¡ ˘ù vG¸ U&ă3 þ ¡ê –ú ,«ęř.

¸C X f´ú ă8t NIÃêÀ ă9åęř.

# cd /etc, vi profile, source profile

-->profileňÛá shell ŕĳąÈşÒáąÏòňÛå ŋÉîňťŋÖîčÈďť.

  W ; ďţğÖáŋťęĳ šÀąÈłÈ ğťŋÈğÉÞ ďÈęÎÞśĳęÈğÉáňÛå ĺĳňžŋÖîčÈďť.
  w ; ňÈďÑòşÉá šÖå ďÈęÎÞśĳęÈęÛå ĺĳňžŋÖîčÈďť..ŋÍåďţąÏòęĳ,,,,,

    sourceğÏòęÏòňÛå şÉáĺÍá şţŋÂňű ąÆěţĺÁśÿ ňÝáłÝÞşÉîčÈďť.

  !!ğÉáňËÞ ŋţĺÁśÝòşÁňźďĳ šÖåąÏòęĳąť čťňĳąź şťąĳłÝœňÆłÈğÏá

     /etc/bashrcęÛå vięĳ ňÏåąĳłÿ ěÑÞąÉöňÛá ĺÉòłÝÞňÆęĳ ąĳŕžŋÁğÏá ďÔîčÈďť

şťŋÈğÉá ĺÏåęĳ ąŒáşţďÆęÈąĳ łÝœŋÈčÛá ňÉãłÛîčÈďť.ŕÿňÛíşťłÈčÛá ĺÖáďÛåňÈ řÍíšťňÝåłÈ ąÏòęĳęÛå ŋÉå şÒÞňÝá ğÑðşÉåćťĺ¡ ňÝåłÈŋÍÞňÆęĳ šÖåąÏòęĳąť čťňĳąź şÉáąÍðňÈŋÈ řÍíšťňÝåşÁňźďĳ šÖåąÏòęĳąť čťňÀğÏá ňžęÿĺÖáňÛá ğÏôďÉáążňÇ ďÈęÎÞśĳęÈğÉá čţęžąťďĳ ňžęÿĺÖáňÛá şÉáşÊòňź čÿğÁąÝá promptąť łÊòąžłÿ ğÏòęÏòňÿęÛå ńÛåěţ ĺÖåšÏáşťąÈ ěţğÖáňÝîčÈďť...şťŋÈğÉá šÖåąÏòęĳąť ŋÑøňÆłÈğÏá ąĳŕÈłžďĳ ďÔîčÈďť.ňÏÞłÈ source ğÏòęÏòşťłžňű şÉîčÈďť.

# cd /usr/src

-->şÑÞ ň¿ ňÈąÑðňÆęĳ ňÈďÑòşţłÿ ňÈąÑðňźďť łĳłÆšťňÝåňÛå ąťŋžďť čÑøąĳ

ňÈąÑðňźłÿ šÖåňÿňű şÉîčÈćťęťąĳ ŋÝåğÖáşÉáďťğÏá.....

ň¿ şÊÞłÝåşÍíňÛå ďĳłÈşÉáĺÑÞšÉáňźłÿ ňÉáşťąĳ ŋÿğÍá ňťğÁďĳ ňÍïčÛá łťğÉÞňźłÿ şťčűąĳ ĺÉáğÖáşţŋÁłÝîłÈňÀ.^^;;

ŋÈąÛí ňžęÿĺÖáňÈ ğÉáŋÈąĳ ňÝñčÛá ňÈ łĳłÆčÛá ąţĺÉåĺÿŋÍáňÝîčÈďť....-.-;;

# rm -f linux, mkdir linux-2.3.8 , ln -s linux-2.3.8 linux ,

  tar xvzf linux-2.3.8.tar.gz

-->ąÈŋÑáňÇ ęÝòřÆęÛå ŋÈňÁąĳ łţęĳňÖá ĺÉòňÛå ğÉáďÛáşÁ łţęĳňÖá ęÝòřÆęÛå ąÍåňÿŋÖíňÆęĳńÿ

ąÆąÑðňźłÿ ŋÉÞňÍîňÈ ŋÝáşÊòď£ďĳęÑÞ şţŋÖîčÈďť.

# ncftp ftp.kr.kernel.org

-->ŋťďÑòňÆęĳ anonymousążŋÍòňÆęĳ ŋÍîąÛáď£ňÿ ňÝåĺÉá ftpĺĳďť ő£ćÛí šÏáşÉîčÈďť.^^;;

# cd /usr/include, ll asm linux scsi , rm -rf asm ,

   ln -s /usr/src/linux/include/asm-i386 /usr/include/asm

-->/usr/includečÛá stdio.hň¡ ąÉöňÛá šÀŋÖá c ęťňÈĺÆęÿęÈ şźďÿšťňÝåňÈ ňÄŕÈşťčÛá

ğţňÁ ŋÖòňÀşÉá ŋÉòłĳňÝîčÈďť.

ĺÉäňťňÑá kernel łĳłÆęÛå šÖåğÏá łĳłÆřĳďÆčÛá /usr/src/linux-"ŋťłÝáňÈ ąťŋžňÖá řÿčÍåĺÿŋÍá" ďÈęÎÞśĳęÈňź łÍåŕÈď£čÛáďź kernel compileňÈ ŋÝáşÊòď£ąÈ ňÄşţłÿčÛá ĺťęĳ ňÈ łĳłÆřĳďÆąť /usr/include ňťęţ asm,linux,scsięÉá ňÈęÛíňÆęĳ řÍíšťňÝåşÉå řÿčÍåłĳłÆ ďÈęÎÞśĳęÈňź ňÑåĺťęÆąź ęÝòřÆď£ňÿ ňÝñčÛáŋÈęÛå şÒÞňÝáşţňű şÉîčÈďť.

čÉóňÛá řÿčÍåĺÿŋÍáňźłÿ čÑœňÛá řÿčÍåĺÿŋÍáňÆęĳ ĺťęĳ ňÑåęťąÉå ěţ

.../asm ňÈ -------> ..../asm-i386ňÆęĳ ĺťćÄňÿ ęÝòřÆąť ŋÉåğÑðď£ňÿ

ęÝòřÆąť ćţŋÝá ąÏòňÁ łţęĳňÖá ęÝòřÆęÛå ğÉáďÛåňÿ ŋÁňÿňű şÉîčÈďť. şÑÞ čťğÿŋÈ ęÝòřÆďĳ ćţŋÏñąÿčť ňÍïčÛá ąÏòňÁ łţęĳ ğÉáďÛåňÿ ŋÁňÿňű şÉîčÈďť.

# cd /usr/src/linux

-->ĺÑáąÏÞŋÍÞňÝá řÍíšťňÝå ŋÉÞňÍîňÈ ňÈęÁňÿŋÈčÛá ąÑðňÝîčÈďť.ňÝåğÏò łťğÉÞ!!

ňÈąÑðňźłÿ ŋÉåď£ğÏá ĺÉSSňÆęĳ čťňĳąĳ ňťčÈğÏá ŋÄďĳłţďĳ ğĳęÆąź...

# make mrproper

-->řÍíšťňÝå ŋÉÞňÍîňÛå şÉåěţ ňÏòşËòňÛå ŋÁčÛá ňÈŋÍá ňĳĺÆŋÎÞśÆšťňÝå(.o)ďÛòňÇ ŋÍòĺĳęÛå

řÍíšťňÝå ŋÉÞňÍîłÁşÊòłÈ ňÏòşËòňÈ ňÍïďĳęÑÞ ŕÿęÈşţŋÖîčÈďť.

# make menuconfig

-->3ąťŋÈňÇ řÿčÍåřÍíšťňÝå łÍåŋÍò ĺÉòĺÍîŋÖò şťčťęĳńÿ ąťŋÉò ğÉãňÈ ńÆňÈčÛá ĺÉòĺÍî ŋÖòňź

şťčťňÝîčÈďť.ęÈčÖÞłÆ łÍåŕÈşÒáąÏòą¡ ĺÈłÛðşÉá şÒáąÏòňÛå ŋźąÑòşţŋÖîčÈďť. şÉáąťŋÈ ŋÁňÇ şÉå ąÍðňÛá ncursesęťčÛá ęťňÈĺÆęÿęÈęÛå łťňÕòşÉíňÆęĳ ňÈąÍðňÈ ćÑÞ łÍåŕÈď£ňÿ ňÝñňÿňű şÉîčÈďť.

čťğÿŋÈŋÖò şťčťňÝá configčÛá şÊòďÉáňÄ łÍåŋÍòňÈğž ěĳďťęÛá şťčťňÝá xconfigčÛá ňÎÞłÆ ňÙáďĳňÁşÒáąÏòňźłÿ łťňÕòşÉå łÁ ňÝñłÛîčÈďť.

# make dep

-->łţęĳňÖá řÿčÍåňÛå ğÉáďÛå ąÈŋÍá ňÇŋÑáłÍò ąÍíłťęÛå ŋÝáşÊòşÉîčÈďť.

# make clean

-->ňÈŋÍá řÍíšťňÝå ą¡ŋÍòłÿ łÊòąÝá ŋÉáŋţďÛåňÛå ńťąÆęÈ łÉÞŋźłÈřÝîčÈďť.

ğÖáŋźňÇ łĳŋÈęÛå łÉÞŋź....

# make bzImage

-->řÿčÍå ňÈğÈŋÈ łÊòłÍòğÏòęÏòňÝîčÈďť.ąÆęÈąĳ,řÍíšťňÝå ŕÿňÛíşťčÛáĺÖáďÛåňÈ ąťŋÉò ğÉãňÛá

ňźęÿęÛå čţčÛá ąÑðňÈąÈďĳ şÉîčÈďť.

1.bzImageňźłÿ ďţğÖáŋť "I" ęÛå ňÉá ńÆąĳ łĳğÖáŋť "i" čť

ąÈśť ňĳśťąť čÉñňÛå ąÏòňÁň¡

2.ąÆčËò zImageşÊñčÛáďź ďţĺÁĺÖá ŕÿňÛíşÉåěţ ŋÑøďťąĳ łÊòąÉÞď£čÛá ąÍðňÛá

ďť łÍáśÊÞňÛå şţłÿ

"System is too big. Try using bzImage or modules"

ňÈň¡ ąÉöňÛá ğźłźŋÈęÛå ĺĳčÊåąÏòňÁňÝîčÈďť.ňÈěţ ďťłÈ bzImageşţŋÁňÿďĳ ď£ŋÈğÉá şÒÞłÝáňÈ ňÍïďťğÏá ŕÿňÛíĺÁśÿ bzImageęÛå ńÆąÈ ĺťęÉîčÈďť.

# make modules , make modules_install

-->řÿčÍå şÒáąÏòłÍåŋÍòłÈ ğĳďÚåęĳ łÍáśÊÞşÉá ąÍðďÛåňÛå řÍíšťňÝåşťąĳ

ğĳďÚåş¡ďÔáąÍðňÛå /lib/modules/"ňžęÿĺÖáňÈ řÍíšťňÝåşÉá řÿčÍåĺÿŋÍá" ďÈęÎÞśĳęÈ ňťęţňź copy şÉîčÈďť.

# cd arch/i386/boot , cp bzImage /boot/mykernel-2.3.8

-->ğÉáďÛåňÿŋÝá řÿčÍå ňÈğÈŋÈęÛå /boot ňťęţňź mykernel-2.3.8ňÈęťčÛá

ňÈęÛíňÆęĳ ĺťćÂłÿ copy şÉîčÈďť.

ňÈğÈŋÈ ňÈęÛíňÛá ňŒáşťčÛá ňÿěÍáąÍðňÆęĳ şţďĳ ŋÑøłÛîčÈďť.... ąÈŋÑáňÈğÈŋÈ ňÈęÛíą¡ ąÉöąź şťŋÈğÉá ňÉãčÛáďťğÏá....

# cd /etc , vi lilo.conf .lilo

-->ĺÁśÆęĳďÿňź łţęĳňÖá ňÈğÈŋÈ ŋÍòĺĳęÛå ďÛòęÑÞşťčÛá ą¡ŋÍòňÝîčÈďť.

ąÈŋÑáňÈğÈŋÈ łÍåŋÍòŋÍòĺĳęÛå ąÆďţęĳ ďÖá łÉòśţňźłÿ ąÉöňÛá şÏòłÝÞňÆęĳ ŕÁąťşťď£ ňžęÿĺÖáňÈ łţęĳ ŋÈňÿŋÖá řÿčÍå ňÈğÈŋÈ ňÈęÛíą¡ ňžęÿĺÖáňÈ ňŒáşťčÛá labelğÏòňÛå ŋÖîčÈďť.

timeout ňÛá ąÈŋÑá 50ňźłÿ 100ňÆęĳ ĺťćÁňÿŋÖáąÍðňÛá

ĺĳśÑò ŕÿňÛí řÍíšťňÝå ŋÍîşťłÈčÛá ĺÖáďÛåňÈ ŋţĺÁśÝòşÁ ňžŕťňžŕťşťďťĺĳğÏá ąÈŋÑáňÈğÈŋÈęĳ ďÛåňÿąťčÛá ąÏòňÁąť ğÉãłÛîčÈďť. ňť, ňžąÈłÿ 10ňÛá 1ŕĳęÛå ňÇğÈşÉîčÈďť..

ďÿňÖÞ ňžňÅęĳňÖá ĺÁśÝòňÛå ňŒáşťłÈğÏá ąÆňÈłÉò łÍåŋÍòşţďĳ ďÔîčÈďť. ňÈęÍøąź łÍåŋÍòşťąĳ ŋÿŋÉòşÁ " lilo " ęÛå şÉáĺÍá łÝåşÊòłÈřžŋÁŋÈ ňÉãňÆğÏá ŕÍáĺÍá ğÉáĺÍá ŋţĺÁśÝòşţďĳ ňžęÿĺÖáňÇ ęÈčÖÞłÆňÉáňź łţęĳňÖá łÝÞąÁąť ďÛåňÿňÝñčÛáŋÈ ŋÖÞňÿďĳ ğĳęÛîčÈďť...

lilo łÝåşÊòşţłÿ ňžęÿĺÖáňÈ ŋÈňÿŋÖá ňÈęÛíňÛå ĺĳňťňűğÉá ŋţĺÁśÝòłÈ

ňÝáłÝÞşÉîčÈďť..

ı ¸C CXĘŹ ,ú NIÇń ęęř. CXĹ X|‹ń rŞ£Ęê ĂŽľ Ãı....(^ ^);; patch˚ P;: ˚yŹ ”ń 0æõ łŹ ĳ1S´”«ęř. SŽB SŽB §UĆ –Ź ńĆř Öä(řŹ ˚y` üo.. `ž ąŽ 2.3.8ú ŕUŹÚ 4‹ 2.3.9` #čřL `Aăo 4‹ řè ŹSS linux-2.3.9õ ŕIb čńÅ???...řè ľê `ęř. ăŞˇ patchĹ ; č;Ćt Is ÓŽžÜý Pĺú diffĘŹ <žú ¸Ìľ üI4q ŤÙÛˇ 7‹£ ˇfi ,«ęř. 0Ęt ěù è^Ć ¸ CX7‹ˇ zXă8 ŁăÛ¸ ˇfi mykernel-2.3.8ù £é^Ć

linux-2.3.9£ žêăŹ ,«ęř. CXõ č: řüČ`Ş-/usr/src , £t , patch-kernel ˇ N8 `ęř.

@ ò 9 1.¸ ȷzŃè /usr/src IŠĆt ŢśýřŹ ,Y 2.£tõ ŞĹt CXľb ćřŹ ,Y ( 2.3.8Ćt Ę£ 2.3.10œ£ č ¡ {řŹ ,«ęř. :`õ &G: | ^Ć Ĳ*řý î¸ ă# ˇŞ8 &G ¡ –úń....^^;; ˇc è ŽČĆ Ćú îß P¸ CX` y»#3 ˘I Př8 ‹‹¸ ă$# řè {7‹¸ ăî¸....

3.‹‹¸ {7‹ èĎ /usr/src/linux/scripts/patch-kernel ú ¸Ìă8 ‘ăřŹ ,«ęř. ıŤď ¸,ê IXf´{¸ ‹ş ćě ľÃo....

ňÝåďÉá ğÍáŋÿ patchş¡ňÝåňÛå łÖáłÿďźęĳ ĺÉäňťňÑáşÁ /usr/src şťňźłÿĺÁśÿ şťąÎñłÛîčÈďť.

[root@zzem /usr/src] # ls
patch-2.3.9.gz patch-2.3.10.gz
----łÖáłÿďţęĳ şÉåěţ
[root@zzem /usr/src] # gzip -cd patch-2.3.9.gz | patch -p0
[root@zzem /usr/src] # gzip -cd patch-2.3.10.gz | patch -p0
-----patch-kernel scripts ňÈňÕòłÈ
[root@zzem /usr/src] # linux/scripts/patch-kernel
[root@zzem /usr/src] # cd linux
[root@zzem /usr/src/linux] # find . -name "*.rej"
[root@zzem /usr/src/linux] # find . -name "*.orig" -exec rm -f {} \;
[root@zzem /usr/src/linux] # cd /usr/src
[root@zzem /usr/src] # rm -f linux

[root@zzem /usr/src] # mv linux-2.3.8 linux.2.3.10
[root@zzem /usr/src] # ln -s linux-2.3.10 linux

ı řè Aê òýL f´ă8t NIÃêÀ ăo

# gzip -cd patch-2.3.9.gz | patch -p0 , gzip -cd patch-2.3.10.gz | patch -p0

-->ňÉîŕÖÞňÛå šÖåąĳłÿ ĺťęĳ šťňÈšÆ(|)ęÉáąÍðňÛå śÑòşţ

    patchğÏòęÏòňÈ łÝåşÊòď£ďĳęÑÞ şÉáąÍðňÝîčÈďť.

# linux/scripts/patch-kernel

-->linux/scripts/patch-kernel ňÛå łÝåşÊòłÈřžłÿ /usr/src ğÝöňÛå ąÍíłťşţłÿ

ŋťďÑòňÆęĳ łÖáłÿďţęĳ patch

# cd linux , # find . -name "*.rej" , find . -name "*.orig" -exec rm -f {} \;

-->find ğÏòęÏòňÛå łÝåşÊòłÈřžłÿ şÏáŋţ ďÈęÎÞśĳęÈ ňťęţňź šţŕÈłÝåšţłÈ łÊòąÈčÛá

    .rej šťňÝåňÈ ňÝñčÛáŋÈęÛå ŋĳłťşťčÛá ąÍðňÝîčÈďť...ğÁłĳłÝÞňÈ şÇłĳłÝÞ...

ňťğÁğÉå ňÍïňÈ šÆęÑíšÆśÆąť ěÆğÏá šţŕÈłÍòąÑò,,,,ňťčÈğÏá....TT.TT łÍòąÑòłÈňÎá ďťňÛíňÆęĳ čÿğÿąť ňŒáĺÑášťňÝåňÛå ŋÈňÁčÛá ąÍðňÝîčÈďť.

# cd /usr/src , rm -f linux , mv linux-2.3.8 linux.2.3.10 ,

  ln -s linux-2.3.10 linux

-->ňÈŋź ŋÛåąÿňÖá ğťňÛíňÆęĳ čÉæňÛáąÍðňÛå ĺÿęÈąĳ łţąÍðňÆęĳ ĺťćÁčÛá ąÍðňÝîčÈďť

    .........(^______^);;

‹ş vG{7‹è qE-Ś` #ąŞŹ ŤB ÃLòùÛffiú æľ W^ú uüřåęř.

~ Code maturity level options ---> ~ Processor type and features ---> ~ Loadable module support ---> ~ General Setup ---> ~ I20 device support ---> ~ Plug and Play Support ---> ~ Block devices ---> ~ Networking Options ---> ~ SCSI support ---> ~ Network Device support ---> ~ Amateur Radio Support ---> ~ IrDA Subsystem Support ---> ~ ISDN subsystem ---> ~ Old CD-ROM drives(not SCSI, not IDE) ---> ~ Character devices ---> ~ USB drivers - not for the faint of heart ---> ~ File systems ---> ~ Console drivers ---> ~ Sound ---> ~ Kernel hacking --->

---

~ Load an Alternate Configuration File ~ Save Configuration to an Alternate File

¸C Ł;& {7‹ăL òŞŹ MŞˇ XÌ ČČ& NLòLı ăŹ Ûffiú æľ W^ú ˇffi}åęř.

~ Code maturity level options

@ ò 11

[ ] Promprt for development and/or incomplete Code/drivers

~ Processor type and features

(PPro/6x86MX)Processor family
    ( ) 386
    ( ) 486
    (X) 586/k5/5x86/6x86
    ( ) Pentium/k6/TSC
    ( ) PPro/6x86MX
(1GB)Maximum Phycical memory
    (X) 1GB
    ( ) 2GB
[ ] Math emulation
[*] (Memory Type Range Register ) Support
[ ] Symmetric multi-processing Support

~ Loadable module support

[* ] Enable loadable module support
[* ] Set version information on all symbols for modules
[* ] Kernel daemon support(e.g.sutoload of modules)

~ General Setup

[* ] Networking support
[* ] PCI support
 (Any)PCI acess mode
      [* ] PCI quirks
      [* ] PCI bridge optimization (Experimental)
[* ] Backward compatible /proc/pci
[ ] MCA support
[ ] SGI Visual Workstaion Support
[* ] System V IPC
[ ] BSD Process Accounting
[* ] Sysctl Support
<M> Kernel support for a.out binaries
<* > kernel support for ELF binaries
<M>kernel supportas ELF - if your GCC is ELF-GCC
<M> Parallel port Support
  < > PC-style hardware
    < > Support foreign hardware
[ ] Advance Power Management BIOS Support

  < > Ignore USER SUSPEND
  < > Enable PM at boot time
  < > Make CPU idle calls when idle

@ ò 12

< > Enable console blanking using APM
< > Power off shutdown
< > Ignore multiple Suspend
< > Ignort multiple Suspend/resume cycles
< > RTC stores time in GMT
< > Allow interrupts during APM BIOS calls

~ I20 device support

< > I20 support
< > I20 PCI support
< > I20 Block OSM
< > I20 LAN OSM
< > I20 SCSI OSM
< > I20 /proc support

~ Plug and Play Support

[*] Plug and Play Support

~ Block devices

<*> Normal Floppy Disk Support
[*] Enhanced IDE/MFM/RLL disk/cdrom/tape support
 --Please see documentation/ide.txt for help/info on IDE drives
[ ] Use old disk-only driver on primary interface
<*> Include IDE/ATA-2 DISK support
[ ] use multi-mode by default
<*> Include IDE/ATAPI CDROM support
< > include CD-changer Reporting
< > Include IDE/ATAPI TAPE support
< > Include IDE/ATAPI FLOPPY support(new)
< > SCSI emulation support
[*] CMD640 chipset Bugfix/support
[*] CMD640 enhanced support
[*] RZ1000 chipset Bugfix/support
[*] Generic PCI IDE chipset Support
[*] Generic PCI bus-master DMA Support
[ ] Boot off-board chipsets first Support
[ ] Other IDE chipset support
  -----Additional Block Devices
[M] Loopback device Support
[M] Network block device Support
[ ] Multiple devices driver Support
    < > Linear (Append) mode
    < > RAID-0 (Striping) mode
    < > RAID-1 (Mirroring) mode
    < > RAID-4/RAID-5 mode

@ ò 13

< > RAM disk support
    [ ] Initial RAM disk(initrd) support
< > XT haddisk support
[ ] Parallel port IDE device Support

~ Networking Options

<*> Packet Socket
[ ] Kernel/User netlink Socket
[ ] Routing messages
  < > Netlink device emulation
[*] Network firewalls
[ ] Socket filtering
<*> Unix domain Sockets
[*] TCP/IP networking
[*] IP: Multicasting
[ ] IP: Advanced router
[ ] IP: ketnel Level autoconfiguration
[ ] IP: Optimize as router not host
< > IP: Tunneling
< > IP: GRE tunnels over IP
[*] IP: Aliasing support
[ ] IP: TCP Syncookes Support ( not enabled per deault )
 ---( it is safe to Leave these untouched )
< > IP: Riverse ARP
[*] IP: Allow large windows ( not recommended if < 16Mb of memory )
 ---
< >The IPX protocol
[ ] IPX: Full internal IPX network
[ ] Appletalk DDP

~ SCSI support

<*> SCSI support
  --SCSI Support type (disk,tape,CD-ROM)
<*> SCSI disk support
< > SCSI tape support
< > SCSI CD-ROM support
<*> SCSI generic support
  --Some SCSI device (e.g. CD jukebox) Support multiple LUNS
[*] Probe all LUNs on each SCSI device
[*] Verbose SCSI error reporting (kernel size +=12K)
SCSI low-level drivers -->
< > 7000FASST SCSI support
< > Adaptec AHA152X/2825 support
< > Adaptec AHA1542 support
< > Adaptec AHA1740 support
< > Adaptec AIC7xxx support

@ ò 14

< > AM53/79c974 PCI SCSI support
< > BusLogic SCSI support
< > DTC3180/3280 SCSI support
< > EATA-DMA(DPT,NEC,AT,SNI,AST,Olivetti,Alphatronix) support
< > EATA-PIO (old DPT PM2001, PM2012A) support
< > Future Domain 16xxSCSI support
< > GDT SCSI Disk Array Controller Support
< > Generic NCR5380/53c400 SCSI support
< > Initio 9100U(W) Support
< > Initio INI-A100U2W Support
< > NCR5380/53c400 mapping method (use Port for T130B)
< > Symbios 53c416 SCSI Support
< > NCR53c406a SCSI support
< > NCR53c8xx SCSI support
<*> SYM53c8xx SCSI support
(4) Default tagged command Queue depth
(32) maximum number of queued commands
(20) synchronous transfers frequency in MHz
[ ] enable profiling
[ ] use normal IO
[ ] Include support for the NCR PQS/PDS SCSI card
< > PAS16 SCSI support
< > PCi2000 support
< > PCi2220i support
< > PCi2240i support
< > Qlogic FAS SCSI support
< > Qlogic ISP SCSI support
< > Qlogic ISP FC support
< > Seagate ST-02 and Future Domain TMC-8xx SCSI support
< > Tekram DC-390(T) SCSI support
< > Trantor T128/T128F/T228 SCSI support
< > UltraStor 14F/34F support
< > UltraStor SCSI support

~ Network Device support

[*] Network device support
< > ARCnet Support
<M> Dummy net driver support
< > EQL (serial line load balancing) support
[*] Ethernet (10 or 100Mbit)
[ ] 3COM cards
  < > 3c501 support
  < > 3c503 support
  < > 3c505 support
  < > 3c507 support
  < > 3c509/3c579 support
  < > 3c515 ISA Fast EtherLink
  < > 3c590/3c900 series (592/595/597/900/905) "Vortex/Boomeriang" support

@ ò 15

<*> AMD LANCE and PCnet (AT1500 and NE2100) support
[ ] Western Digital/SMC cards
[ ] Racal-interlan (Micom) NI cards
[ ] Other ISA cards
[*] EISA,VLB.PCI and on board controllers
<*> AMD PCInet32 (VLB and PCI) support
< > Apricot Xen-II on board Ethernet
< > CS8x0 support
< > Generic DECchip & DIGITAL EtherWORKS PCI/EISA
< > DECchip Tulip (dc21x4x) PCI support
< > Digi Intl . RightSwitch SE-X support
<*> EtherExpressPro/100 support
< > PCI NE2000 support
< > TI ThunderLAN support
< > IA Rhine support
 [ ] Pocket and portable adaptors
 [ ] FDDI driver support
< > Frame relay DLCI support
<M> PPP (point-to-point) support
<*> SLIP (serial line) support
[ ] Wireless LAN (non - hamradio)
[ ] Token Ring driver support
< > Comtrol Hostess SV-11 support
< > COSA/SRP sysc serial boards support
< > Red Creek Hardware VPN (EXPERIMENTAL)
 [ ] WAN drivers

~ Amateur Radio Support

[ ] Amateur Radio Support
  --packet radio protocols
< > Amateur Radio AX.25 Level 2 protocols
  --Misc hamradio Protocols

~ IrDA Subsystem Support

< > IrDA Subsystem Support
< > IrDA subsystem support
---IrDA protocols
< > IrLAN protocols
< > IrCOMM protocols
< > IrLPT protocols
    < > IrLPT client support
    < > IrLPT server support
< > IrDA protocol options
--- IrDA options
[ ] Cache last LSAP
[ ] Fast RRs
[ ] Debug infomation

@ ò 16

[ ] IrLAP compression
 Infrared-port device drivers -->
       --- SIR device drivers
      < > IrTTY (users linux serial driver )
            IrPORT (IrDA serial driver)
       --- FIR device drivers
      < > NSC PC87108
      < > Winbond W83977AF (IR)
      < > Sharp UIRCC
      < > Toshiba Type-0 IR Port
      < > SMC IrCC
       --- Dongle support
      [ ] Serial dongle support
      < > ESI JetEye PC dongle
      < > ACTiSYS IR-220L and IR220L+ dongle
      < > Tekram IrMate 210B dongle
      < > Greenwich GirBIL dongle
      < > Parallax LiteLink dongle

~ ISDN subsystem

< > ISDN support
[ ] Support synchronous PPP
  [ ] Use VJ-compression with synchronous PPP

[ ] Support audio via ISDN
[ ] X.25 PLP on top of ISDN (Experimental)
< > ICN 2B and 4B support
< > ISDNloop Support
< > PCBIT-D support
< > HiSax SiemensChipSet driver support
< > AVM-B1 with CAPI2.0 support

~ OLD CD-ROM drivers(not for SCSI or IDE/ATAPI drives)

[*] Support non-SCSI/IDE/ATAPI CDROM drives
< > Aztech/Orchid/Okano/Wearnes/TXC/CyDROM CDROM support
< > Goldstar R420 CDROM support
< > Matsushita/Panasonic/Creative, Longshine, TEAC CDROM support

< > Mitsumi (standard) [no XA/Multisession] CDROM support
< > Mitsumi [XA/MultiSession] CDROM support
< > Optics Storage DOLPHIN 8000AT CDROM support
< > Philips/LMS CM206 CDROM support
< > Sanyo CDR-H94A CDROM support
< > ISP16/MAD16/Mozart soft configurable cdrom interface support

@ ò 17

< > Sony CDU31A/CDU33A CDROM support
< > Sony CDU535 CDROM support

~ Character devices

[*] Vitual terminal
[*] Support for console on Vitual terminal
<M> Standard/generic (dumb) Serial Support
[ ] Support for console on Serial port
[ ] Extended dumb Serial driver options
  [ ] Support more than 4 serial ports
  [ ] Support for Sharing Serial ports (unsafe)
  [ ] Autodetect IRQ on Standard ports
  [ ] Support special multiport boards
  [ ] Support the Bell Technologies HUB6 card
[ ] Non-Standard Serial port Support
[*] Unix98 PTY Support
  (256) Maximum number of Unix98 PTYS in use (0-2048)
[*] Mouse Support (not serial mice)
Mice--->
  < > ATIXL busmouse support
  < > Logitech busmouse support
  < > Microsoft busmouse support
  [*] PS/2 mouse (aka "auxiliary device") support
  [*] C 82C710 mouse port support (as on TI Travelmate)
  < > PC110 digitizar pad Support
[ ] QIC-02 tape support
[ ] Watchdog Timer Support
[ ] /dev/nvram Support
[ ] Enhanced Real Time Clock Support
 Video for Linux -->
     <M>video for linux
     < > AIMslab RadioTrack ( aka Radio Reveal ) support
     < > AIMslab RadioTrack FF support
     < > A : tech/Packard Bell Radio
     < > Miro PCM20 Radio
     < > Gemtek Radio Card support
     < > BT848 Video For Linux
     < > Modiavision Pro Movie Studio Video For Linux
     < > SAA5249 TeleText processor
     < > SF16FMI Radio
     < > Typhon Radio ( a.k.a EcoRadio )
     < > Zoltrix Radio
 Joystick Support -->
     <*> Joystick support
     < > Classic PC analog joysticks gamepads
     < > FPGaming and MadCatz A3D controllers
     < > Gravis GrIP joysticks gamepads
     < > Logitech Digital joysticks gamepads

@ ò 18

    < > Microsoft SideWinder, Genius Digital joysticks and gamepads
    < > ThrustMaster DirectConnect joysticks and game pads
    < > PDPI Lightning 4 gamecards

< > Double talk PC internal Speech card Support
 Ftape,the floppy tape device driver

~ USB drivers - not for the faint of heart

<*> Support for USB ( Expermental )
<*> UHCI ( intel PIIX4 and others ) support
< > OHCI ( compaq and some others ) support
< > OHCI-HCD ( other OHCI opt,virt,Root HUb ) support
<*> USB hub support
<*> USB mouse support
<*> USB keyboard support
< > USB audio parsing support
< > USB abstract control Model support
< > USB printer support
< > USB SCSI support

~ File systems

 [*] Quota support
 <*> Kernel automounter support (experimental)
 < > Amiga FFS filesystem support (EXPERIMENTAL)
 < > Apple Macintosh filesystem Support
 <M > DOS FAT fs support
    <M > MSDOS fs support
       < > umsdos: Unix like fs on top of std MSDOS FAT fs
    <M > VFAT (Windows-95) fs support
 <M> ISO9660 cdrom filesystem support
 [*] Microsoft joliet CDROM extentions
 < > Minix fs support
 < > NTFS filesystem Support (read only)
 [ ] NTFS read-write Support (DANGEROUS)
 [ ] OS/2 HPFS filesystem support (read only)
 [*] /proc filesystem support
 [*] /dev/pts filesystem Support (readonly)
 < > QNX filesystem Support
 < > ROM filesystem Support
 <*> Second extended fs Support
 < > System V and Coherent filesystem support
 < > UFS filesystem support (read only)

Network filesystems-->
  < > Coda filesystem support ( advanced networks fs )

@ ò 19

  <*> NFS filesystem support
  < > SMB filesystem support (to mount WfW shares dtc.)
  < > NCP filesystem support(to mount NetWare volumes)
[ ] Packet signatures
[ ] Proprietary file Locking
[ ] Clear remove/delete inhibit when neede
[ ] Use NFS namespace if available
[ ] Use long ( os/2 ) namespace if available
[ ] Allow mouthing of volume subdirectories
[ ] Use Native language Support
[ ] Enale symbolic links and Execute flags
Partition Types ->
[ ] BSD disklabel ( BSD partiton tables ) support
[ ] Macintosh partition map Support
[ ] SMD disklabel ( sun partition tables ) support
[ ] Solaris ( X86 ) partition table support
[ ] SGI disklabel support

~ Consoledrivers

[*] VGA text console
[ ] Video mode Selection Support

~ Sound

<M> Sound card support
< > C-media PCI (CMI8338/8378 )
< > Ensoniq AudioPCI
< > Creative Ensoniq AudioPCI 97 (ES1371)
< > S3 SonicVibes
< > Support for Turtle Beach MutiSound Classic, Tahiti , Monterey
< > Support for Turtle Beach MutiSound Pinnacle, Fiji
<M> OSS sound modules
       < > ProAudioSpectrum 16 support
       <M> 100% Sound Blaster compatibles (SB16/32/64,ESS,Jazz16) support
       <M> Generic OPL2/OPL3 FM synthesizer support
       < > Gravis Ultrasound support
       < > MPU-401 support (NOT for SB16)
       < > PSS (AD1848,ADSP-2115,ESC614) support
       < > Microsoft Sound System support
       < > Ensoniq SoundScape support
       < > MediaTrix AudidTric Pro support
       < > Support for OPTi MAD16 and/or Morzart based cards
       < > Full support for Turtle Beach WaveFront (Tropez Plus, Tropez)
       < > Support for Crystal CS4232 based (PnP) cards
       < > Support for Aztech Sound Galaxy (non-PnP) cards
       < > Limited support for Turtle Beach Wave Front (Maui,Tropez)
       < > Support for Aztech Sound Galaxy (non-PnP) cards
       < > Yamaha OPL3-SA1 audio controller

@ ò 20

     < > SoftOSS software wave table engine
     <*>FM synthesizer(YM3812/OPL-3 ) support
     <*> Loopback MIDI device support
     < > 6850 UART support
Additional low level sound drivers --->
     < > Additional low level sound drivers
     < > ACI mixer (microPCM12)
     < > AWE32 synth
     < > Gallant Audio Cards (SC-6000 and SC-6600 based )

~ Kernel hacking

[ ] Kernel profiling support

*^^*

¸C #Ć3 ”Ź /:˚ {7‹ú uüă§; ›q~8 ˘ù œS` þ,«ęř.řŹ ÙTă$# z<¸ { $#ć,ffi¸ ˘ùÚ ŁăÛ¸ –Œsè§ ĘŃęř.

~ Code maturity level options

[ ] Promprt for development and/or incomplete Code/drivers

 -->řÿčÍå řĳďÆňÇ łÍòłÖÞďĳęÛå łÍáśÊÞşťčÛá ĺÁĺÖáňÆęĳ ąţĺÉåĺÿŋÍá łÁŋÖáňÇ łĳłÆęÛå

łťňÕòşťąźćÛí łÍáśÊÞşţŋÁčÛá ąÍðňÝîčÈďť.

ňÈąÍðňÛá ňÉåšťĺÿŋÍáďÛåňÛå řÿčÍåňź šĳşÉíłÈřÝåąÍðňÝáŋÈ ğÖäčÛá şÉòğÑÞňÝîčÈďť.

~ Processor type and features

(PPro/6x86MX)Processor family

--> ŋťłÝáňÇ řÍíšÅśÿ CPU ęÛå ąÑåęťŋÁğÏá ďÔîčÈďť.

!!..řÍíšťňÝåşÁ ŋţĺÁśÝòłÈ ňÝåňÿčťčÛá PanicşÏáłÉòňÇ ďţĺÁĺÖáňÛá ňÈąÑðłÍåŋÍò ŋÉåğÑðňÈ

ğÉãňÆčÈ ąÉÞĺÏåşÈ ŋÁňÇşťąÝå ĺťęťğž ćÑÞ ďťłÈşÉáĺÍá şÒÞňÝáşÁ čÍíňÿąťďĳęÑÞ şťłźňÀ. ŋÉå ğĳęÆąÿčť ľÈőťCPU(^_^)ęťğÏá ňÉáŋÍáşťąź 386ňÛå łÍáśÊÞşťŋť...!!

    ( ) 386
    ( ) 486
    (X) 586/k5/5x86/6x86
    ( ) Pentium/k6/TSC
    ( ) PPro/6x86MX

(1GB)Maximum Phycical memory

--->řÿčÍå 2.2ĺÿŋÍáĺÁśÿ ąÛîąÏÞşÈ ňÑåęťąÉá ŋÈňŒáğźğĳęÈňÝîčÈďť....

ňťğť ňÈąÍðňÛå 2GBćťŋÈ łťňÕòşÉå łťňÕòŋťąť ňÝñňÛåŋÈ ğĳęÆąÎñłÛîčÈďť.... ąÑä 4GBňÈłÉòćťŋÈ ŋÈňŒáňÈ ąťčÛòşÉåćÿęťąĳ şÉîčÈďť....

    (X) 1GB

    ( ) 2GB

[ ] Math emulation

-->ęÈčÖÞłÆąť řĳšÆęĳłźłÿąť ňÍïčÛá řÍíšÅśÿňźłÿ řĳšÆęĳłźłÿňÇ ąÈčÛòňÛå

łÁşÊòşţŋÁčÛá ąÈčÛòňÛå ğÉåşÉîčÈďť.

řÍíšÅśÿňÇ ďÁč£ęť şÉåłÁ ňÝñčÛá CPU ňźłÿ ĺÑÞŋÉîşÉá łÁşÉÞążłÉáňÇ ąÏòňÁčÛá

CPU ňź ŋÁčÛá ĺÁďÉíňÈ řÆąÈ ěţğÖáňź řĳšÆęĳłźłÿęťčÛá ŕÝîňÛå ĺÏåďĳęĳ

ŋÉòŕÉÞşťąĳ ňÝñčÛáďź šÎáśÈňÍíňÈčť 486DX ňÈłÉòňÇ ąÈŋÑòňÛá řĳšÆęĳłźłÿęťčÛá ŕÝîňÛå ěťęĳ ŋÉòŕÉÞşťąĳňÝñąÈ ěţğÖáňź ňÈ ąÈčÛòňÛá ĺÏåęĳ šÝåňÀąť ňÍïłÛîčÈďť.

486DX ňÈşťňÇ ąÈŋÑòňÛå ąťŋÝá łťňÕòŋťčÛá łÍáśÊÞňÛå şťąÈ ĺťęÉîčÈďť.

łÍáśÊÞňÛå şťąź ď£ğÏá ĺĳŋĳ šÆęĳłźłÿąť łťňÕòď£ąĳ ňźğÚåęźňÈłÏáňÛá ğÁłÈď£ąź ďÔîčÈďť.

[ ] MTTR (Memory Type Range Register ) Support

 -->Pentium ProňÈłÉòňÇ łÈłÆśÎíňÈąĳ PCIčť AGPĺÿłÆ ĺÈďÈňĳřťďÆąť

ňÝñďťğÏá łÍáśÊÞşÉîčÈďť.

ňÈğÈŋÈęÛå 2ĺţňÈłÉò ľÉåęÈ ńÛå łÁ ňÝñąÈ ěţğÖáňÝîčÈďť.

[ ] Symmetric multi-processing Support

-->SMPąÈčÛòňÇ ŋÈňŒáňÝîčÈďť.

ňÈąÍðňÛå łťňÕòłÈ Charater devices-->Enhanced real time clock support ďĳ łÍáśÊÞşţňű şÉîčÈďť.

ěĳşÉá General setup---->Advanced power management BIOS support čÛá "N"

~ Loadable module support

[ ] Enable loadable module support

-->řÿčÍåňźłÿ ğĳďÚåňÛå łťňÕòşÉåłÁ ňÝñąź şţŋÁčÛáąÍðňÝîčÈďť.

ďÑòŋÍÞ ğĳďÚå ąÈčÛòňÛå ąťčÛòşťąźćÛí şţŋÁčÛá ąÈčÛòňÆęĳńÿ ňÙáşťčÛá ąÈčÛòňÛå ğźğĳęÈňź ňÑåęžčÑøąĳ šÝåňÀňÍïčÛá ąÈčÛòňÛá ğźğĳęÈňźłÿ ľţčţčÛá ąÈčÛòňÛå şţŋÁčÛáąÍðňÝîčÈďť.

[ ] Set version information on all symbols for modules

-->řÿčÍåňÈ ĺťćÄňÿďĳ ąÈŋÑáňÇ ğĳďÚåňÛå łťňÕòşťąź şţ ŋÁąź şťčÛáąÍðňÝîčÈďť.

[ ] Kernel daemon support(e.g.sutoload of modules)

-->ğĳďÚåňź ďţşţ řÿčÍåňÈ şÉòłÉò ďţĺÈşţ ŋÁďĳęÑÞ łÍåŋÍòşťčÛáąÍðňÝîčÈďť.

Insmod čť rmmod ğÏòęÏòňÛå łťňÕòşťŋÈ ňÉãąĳ kerneld ęťčÛá šÆęĳąÆęÊíňÈ

ŋťďÑòŋÍÞňÆęĳ ğĳďÚåňÈ ňÿčÆ ąÈčÛòňÛå łÁşÊòşťŋÈ ňÉãňÆğÏá ŋťďÑòŋÍÞňÆęĳ ğĳďÚåňÛå ğźğĳęÈňź ňÑåęÈąĳ,ňÝåŋÍòłÈąÉá ąÆ ğĳďÚåňÛå łťňÕòşťŋÈ ňÉãňÛåłÈňźčÛá ŋťďÑòŋÍÞňÆęĳ ğĳďÚåňÛå ğźğĳęÈňźłÿ ŋźąÿşťčÛá ąÈčÛòňÛå ąťŋÝá ňÅňÕòşÉá šÆęĳąÆęÊíňÝîčÈďť.

~ General Setup

[ ] Networking support

-->ęÈčÖÞłÆňź čźśÆňÂřÝòňÛå łťňÕòşťąź şţŋÁčÛá ąÈčÛòňÝîčÈďť.

ęÈčÖÞłÆąť ďťęÛá łťňÕòňÖáňÏòŕźŋźň¡ňÇ ĺÈąÀňź ňÝñňÿłÿ ąÉòŋÍíňÛá ĺťęĳ čźřÆňÂřÝòňź ňÝñłÛîčÈďť.

ęÈčÖÞłÆňźłÿ čźśÆňÂřÝòňÛå şťęžğÏá ćÑÞ łÍáśÊÞşÉîčÈďť.

[ ] PCI bios(---şÒÞňÝáşÉåąÍð--) support

-->pci ĺťňÈňĳłÆęÛå ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.

šÎáśÈňÍí ňÈłÉòňÇ šÆęĳłźłÿąť ďÉåęÝá řÍíšÅśÿňźłÿčÛá pci ąť čţŋÉòď£ňÿ ňÝñňÆğÆęĳ łÍáśÊÞşťąÈ ĺťęÉîčÈďť.

 (Any)PCI acess mode

-->AnyčÛá řÿčÍåňÈ ĺťňÈňĳłÆ ďĳňÖíňÍïňÈ ŋÝÞŋÍîŋÍîąÛáşţ ĺĳąĳ ĺÉáňÛòňÈ ňÍïňÆğÏá

   biosęĳ ąťčÛá łÍåŋÍòğĳďÆňÝîčÈďť..

ňÈň£ňź "bios"ň¡ "direct"ąť ňÝñňÆğž..

ğÉåąÆďţęĳ ŋÍáŋťčÛá biosňÇŋÑáňÈąĳ şÁŋťčÛá ĺÈňÇŋÑáňÝîčÈďť.

[ ] PCI quirks

-->"Y" ; BIOSąť ćţŋÏñňÛåěţ

   "N" ; " ŋÍòłÉòňÝåěţ

[ ] PCI bridge optimization (Experimental)

-->PCI ĺÆęÝðŋÈęÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.

  CPU ň¡ PCI , PCIň¡ ISA łťňÈňź ĺÆęÈŋÈąť ňÝñňÿ łÿęĳ ďťęÛá

ĺÿłÆłťňÈňźłÿ ďźňÈśÿęÛå ŋÍáłÑòşÉå łÁ ňÝñďĳęÑÞ čÑáęÈŋÍÞňÝá ąÈčÛòňÛå şÉîčÈďť.

ĺťňÈňĳłÆňź ąÖäňÈ ğÖáŋźąť ňÍïďťğÏá "N" ,ňÝñďťğÏá "Y" łÝåşÍíŋÍÞňÝáąÍðňÛá ď£ďĳęÑÞ łÍáśÊÞňź łÝáŋÖòňÛå....

[ ]Backward compatible /proc/pci

-->ňĳęţďÔá šÖåąÆęÝíňÛå ňÈňÕòşţ PCIŋÍòĺĳęÛå ňÝæňÛåěţ šÝåňÀşÉîčÈďť.

[ ] MCA support

-->"MICRO CHANNEL ARCHITECTURE" IBM PS/2 ğÿłÝáňźłÿ

šÝåňÀşÉîčÈďť.

[ ] SGI Visual Workstaion Support

-->SGI 320,540 Workstationňźłÿ šÝåňÀşÉîčÈďť.

[ ] System V IPC

 -->System V IPCęÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.

ęÈčÖÞłÆňźłÿčÛá ďĳłÆňÕò šÆęĳąÆęÊíňÛå ňźğÚåęźňÈśÿęÛå śÑòşţłÿ łÝåşÊòłÈřÝåłÁ ňÝñłÛîčÈďť. šÆęĳłźłÆ łťňÈňźłÿ ďÑòąÈş¡ň¡ ŋÍòĺĳąÀşÒáňÛå ňÄşÉá ęťňÈĺÆęÿęÈ şÉíłÁň¡ łÈłÆśÎí řÑå ğĳňÛíňÝîčÈďť.

ňÈ şÉòğÑÞňÛå łÍáśÊÞşťąź ď£ğÏá, ęÈčÖÞłÆ ĺÉÞłÆčÛá System V IPC ęĳ ŋÉÞďÑòňÛå şťąź ď£ğž,ęÈčÖÞłÆňźłÿ ďĳłÆňÕò šÆęĳąÆęÊíňÛå łťňÕòşÉåłÁ ňÝñąź şţŋÖîčÈďť.

[ ] BSD Process Accounting

-->šÆęĳłźłÆąť ŋÑáŋţşÉå ěţňźčÛá ňÍáŋźčť řÿčÍåňź ňÇşţ šÆęĳłźłÆ ŋÍòĺĳ
  (łĳňÅąŒá,łÊòłÍòłÈąÉá,ğźğĳęÈŋÍíňÅłÉòśţďÛò..)ąť šťňÝåňź ŕÁąť.

[ ] Sysctl Support

-->Sysctl interfacečÛá kernel compile ŋţŋÝåňÈčť łÈłÆśÎí ŋţĺÁśÝò ňÍîňÈ

łÝåşÊòŋÖòňÝá řÿčÍå ğţąţĺÏáłÁęÛå ďÑòŋÍÞňÆęĳ ĺÏáąÏòşťčÛá ĺÉòĺÍîňÛå ŋźąÑòşÉîčÈďť. ŋÁ ňÝáśÿšźňÈłÆčÛá łÈłÆśÎířÑåęĳ ňÈęÁňÿŋž ňÝñŋÈğÉá /proc šťňÝåłÈłÆśÎíňÈ łÍåŕÈď£ňÿ ňÝñďťğÏá šÏáŋÝî ąťčÛòşÉá SysctlňÀłĳ śÆęÈčÛá /proc/sys ďÈęÎÞśĳęÈ ňťęţ łÊòłÍòďÔå ąÍðňÝîčÈďť.řÿčÍå řÆąÈąť 8kb čÛåňÿčÉîčÈďť.

< > Kernel support for a.out binaries

-->řÿčÍåňÈ a.out łÝåşÊò šťňÝå şÏòłÝÞňÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.

   a.out ňÈęÉá? (Assembler.OUTput) ňÇ ňËÞŋťęĳ ŕĳŕÉòąÈ ňÅčÝÞłÆňźłÿ

ńÆňÈďÍá łÝåşÊò šťňÝå şÏòśţňÝîčÈďť.

< > kernel support for ELF binaries

-->řÿčÍåňÈ ELF łÝåşÊò šťňÝå şÏòłÝÞňÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.
  ELF čÛá a.out ňÈşÁňź ďÛòŋÉòşÉá ĺťňÈčÿęÈ şÏòłÝÞňÈğÏáłÿ ęÈčÖÞłÆ ĺťňÈčÿęÈ

šĳğÊðňÇ šÀŋÖáňÈğÆęĳ ĺÉáďÆłÈ łÍáśÊÞşťďĳęÑÞ şÉîčÈďť..

< > Compile kernel as ELF - if your GCC is ELF-GCC

-->řÿčÍå şÏòśţęÛå ELF şÏòłÝÞňÆęĳ ğÉáďÆčÛáąÍðňÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.
  GCC čÛá ęÈčÖÞłÆňźłÿ ŋÖòňÀşÉá řÍíšťňÝåňÈğÏáłÿ, ğĳďÛá ňÅčÝÞłÆňźłÿ şĳşÒáňÈ

ď£čÛá řÍíšťňÝåęÿňÝîčÈďť.

ňÈ şÉòğÑÞňÛå ŋÈňŒáşťąź şţŋÁğÏá, GCC ąť ELF łÝåşÊò šťňÝå şÏòśţňÝåěţňź, řÿčÍå şÏòłÝÞďĳ ELF ęĳ řÍíšťňÝå şÉåłÁ ňÝñąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.

@ ò 24

< > kernel support for JAVA binaries

--> řÿčÍåňÈ JAVA łÝåşÊò šťňÝå şÏòłÝÞňÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.

ňÈ şÉòğÑÞňÛå łÍáśÊÞşťğÏá, řÿčÍå ŋťŕźňźłÿ JAVA ĺťňÈčÿęÈęÛå łÝåşÊòśĳęÑÞ ŋÈňŒáşţŋÖîčÈďť.

< > Parallel port Support

-->Parallel portęÛå ňÈňÕòşţłÿ printer,zip driveďÛòňÛå łťňÕòşÉáďťğÏá łÍáśÊÞşÉîčÈďť.

    < > PC-style hardware

    -->PC-style Parallel port ňÍïďťğÏá "N"

    < > Support foreign hardware

[ ] Advance Power Management BIOS Support

  < > Ignore USER SUSPEND

  -->APM ęÛå łÍåŋÍòşÉá łťňÕòŋťęťğÏá ňÈ ąÈčÛòňÛå NO ęĳ łÍáśÊÞşÉîčÈďť.

ňÝåĺÉá łťňÕòŋťňźąźčÛá šÝåňÀňÍïčÛá şÉòğÑÞňÝîčÈďť.

< > Enable PM at boot time

< > Make CPU idle calls when idle

-->ďÅňÍå CPU ňÈłÉòňÇ CPU ňÇ łÁęÛå ąťŋÈąĳ ňÝñčÛá łťňÕòŋťąť ňťčÈ ęťğÏá

ąÆčËò śÑòą¡.

< > Enable console blanking using APM

-->ŋÍáňŒáąÒáęÈęÛå ňÄşţłÿ čĳśÆĺÖÞňÇ ĺÊÞęťňÈśÆ ąÈčÛòňÛå ćÆčÛá ąÈčÛòňÝîčÈďť.

< > Power off shutdown

--> łÈłÆśÎíňÛå ŋÑòęÀşÉåěţ čťňĳčÛá ğźłźŋÈ"SYSTEM IS HALTED"ąť čťňĳčÛá

ďÑòłÈňź ŋÍáňŒáňÛå ŕťďÉáşťčÛá ąÈčÛòňÛå ŋÈňŒáşÉîčÈďť.

řÍíšÅśÿňÇ ĺťňÈňĳłÆňź ěťęť ąÈčÛòňÈ ŋÍÞŋÍåşÈ şÒåňÕòď£ŋÈ ňÉãňÛå ěţąť ňÝñďť.

< > Ignore multiple Suspend
< > Ignort multiple Suspend/resume cycles
< > RTC stores time in GMT
< > Allow interrupts during APM BIOS calls

~ I20 device support

< > I20 support

@ ò 25

      < > I20 PCI support
      < > I20 Block OSM
      < > I20 LAN OSM
      < > I20 SCSI OSM
      < > I20 /proc support

-->ňťŋÝÞňÈąź ğŒáŋÈ ğĳęÛîčÈďť....-.-;;

şÑÞ ňťłÈčÛáĺÖáňÛá ďÊðąÛåňÛå ďÉåňťŋÁłźňÀ..(^___^);; ~ Plug and Play Support

   [ ] Plug and Play Support

-->łÍåŋÍòşţňű ŋÑøňÛáąÿ ďť ňťłÈŋÀ.

~ Block devices

< > Normal floppy disk support

-->ęÈčÖÞłÆňźłÿ šÛåęĳšÈ ďÆęťňÈĺÿ ŋÉòŕÈęÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.

[ ] Enhanced IDE/MFM/RLL disk/cdrom/tape support

 --> IDE driveęÛå łťňÕòşÉåłÁ ňÝñąź ŋÈňŒáşťąź şţŋÖîčÈďť.
     Personal Computer ňźłÿčÛá şťďÆďÈłÆřÆň¡ CD-ROM ďÆęťňÈĺÆąť

   IDE ňź łÑÞşťčÛáďź,IDE ďÆęťňÈĺÆčÛá 4ąţćťŋÈ łťňÕòşÉåłÁ ňÝñąĳ,

ęÈčÖÞłÆňźłÿ IDE ŋÉòŕÈęÛå łťňÕòşťęžğÏá łÍáśÊÞşÉîčÈďť.

 --Please see documentation/ide.txt for help/info on IDE drives
[ ] Use old disk-only driver on primary interface

-->ňżŋÍáňź ŕÖåłÈďÔá şťďÆďÈłÆřÆęÛå šÆęťňÈğÿęÈęĳ łťňÕòşÉåłÁ ňÝñąź şţŋÁčÛá

ąÈčÛòňÝîčÈďť.ňÈ şÉòğÑÞňÛå łÍáśÊÞşťğÏá, şťčťňÇ ňÝáśÿšźňÈłÆňź ňĳŋÝÞ ďÁąţňÇ şťďÆďÈłÆřÆğÉáňÛå ŋÈňŒáşťąź şţŋÖîčÈďť.

< > Include IDE/ATA-2 DISK support
     [ ] use multi-mode by default
< > Include IDE/ATAPI CDROM support

-->ATAPI ĺÉòłÝÞňÇ CD-ROM ňÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.
   SCSI ňÕò CD-ROM ňÈčť 2ĺţłÑÞ ňÈşťňÇ CD-ROM ŋÖò śÛÞĺÏåşÉá

ŋÉòŕÈęÛå ŋźň£şťąĳčÛá ňÈąÍðňÛå łÍáśÊÞşťğÏá ęÈčÖÞłÆňź CD-ROM ňÛå łťňÕòşÉåłÁąť ňÝñłÛîčÈďť.

      < > include CD-changer Reporting
< > Include IDE/ATAPI TAPE support

--> IDE ĺÉòłÝÞňÇ TAPE ďÆęťňÈĺÿęÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.
    TAPE ďÆęťňÈĺÆčÛá ňÂřÆłÆśźňÈłÏáňÈčť ąÈśť ŋÖò,ďţşÏò łÿĺÿąÛî

ňÈłÉòňÇ ąÈŋÑòňźłÿ ĺÊÞňÍîňÕòňÆęĳ şťňÕòşťčÛá ğźŕźňÈğÆęĳ ňÝåĺÉá PC łťňÕòŋťďÛåňÛá łÍáśÊÞşÉå šÝåňÀ ňÍïłÛîčÈďť.

< > Include IDE/ATAPI FLOPPY support(new)

--> SCSI šÆęĳśĳřÑåňÛå łťňÕòşťčÛá łţęĳňÖá ĺÉòłÝÞňÇ IDE cdrom/tape/floppy

    driverň¡ ďÑòďÛòşÉá ATAPI şÏòłÝÞňÇ FLOPPY ęÛå ŋÈňŒáşťąź şţŋÁčÛá

şÉòğÑÞňÝîčÈďť.ATAPI ZIP ďÆęťňÈĺÆčť LS_120, łÅšÿ ďÆęťňÈĺÆ ąÉöňÛá ďÆęťňÈĺÿęÛå ąťŋÈąĳ ňÝñčÛá łťňÕòŋťčÛá ňÈ şÉòğÑÞňÛå łÍáśÊÞňÆęĳ łÍåŋÍòşťğÏá łťňÕòşÉåłÁąť ňÝñłÛîčÈďť.

< > SCSI emulation support

-->IDE ATAPI ďÈĺťňÈłÆ ŋÉòŕÈęÛå SCSI ŋÉòŕÈŕÿęÍí ňźğÚåęźňÈśÆ şţŋÁčÛá

ąÈčÛòňÛå ŋÈňŒáşţŋÖîčÈďť. ňżęÛå ďÛåŋťğÏá, ATAPI PD-CD dirve ň¡ ąÉöňÛá ŋÉòŕÈęÛå SCSI ň¡ ďÑòďÛòşÉá ĺÉòłÝÞňÆęĳ łťňÕòşťąź ćÛí şţŋÁčÛá ĺÉòłÝÞňÝîčÈďť..

[ ] CMD640 chipset bugfix/support

-- MD640 ŕÝîłÎðňÇ ĺÿąÆęÛå ąĳŕÝá şÉòğÑÞňÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞşÉîčÈďť.

    CMD640 ŕÝîłÎðňÛá ňÝåĺÉáŋÍÞňÆęĳ 486ňÈłÉò šÎáśÈňÍí ĺĳďÆňź ŋÁęĳ ńÆňÈčÛá

ŕÝîłÎðňÝáďź,ŋÁęĳ Netune ňÈčť SiS ň¡ ąÉöňÛá ŕÝîłÎðňź ŋÁęĳ ąÉöňÈ ńÆňÝîčÈďť. řÍíšÅśÿňÇ ğťďÿĺĳďÆňźłÿ CMD640 ęÛå ŋÈňŒáşÉáďťğÏá, ňÈ ąÈčÛòňÛå łÍáśÊÞşťąÈ ĺťęÉîčÈďť.

[ ] CMD640 enhanced support

--> CMD640 ŕÝîłÎðňÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.

řÍíšÅśÿňÇ ğťďÿĺĳďÆňźłÿ CMD640 ęÛå ŋÈňŒáşÉáďťğÏá, ňÈ ąÈčÛòňÛå łÍáśÊÞşťąÈ ĺťęÉîčÈďť.

[ ] RZ1000 chipset bugfix/support

-->RZ1000 ŕÝîłÎðňÇ ĺÿąÆęÛå ąĳŕÝá şÉòğÑÞňÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.

    RZ1000 ŕÝîłÎðňÛá ňÝåĺÉáŋÍÞňÆęĳ 486ňÈłÉò šÎáśÈňÍí ĺĳďÆňź ŋÁęĳ ńÆňÈčÛá

ŕÝîłÎðňÝîčÈďť.řÍíšÅśÿňÇ ğťďÿĺĳďÆňźłÿ RZ1000 ňÛå ŋÈňŒáşÉáďťğÏá, ňÈ ąÈčÛòňÛå łÍáśÊÞşťąÈ ĺťęÉîčÈďť.

[ ] Generic PCI bus-master DMA Support

[ ] Boot off-board chipsets first Support

[ ] Other IDE chipset support

-->čťňÑá ŕÝîłÎð ňÈň£ňÇ ďťęÛá ŕÝîłÎðňÛå ŋÈňŒáşťąź şţŋÁčÛá şÉòğÑÞňÝîčÈďť.

ďťňËòşÉá ŋÑòęÅňÇ ŕÝîłÎðňÛå łÍáśÊÞşÉåłÁ ňÝñąźşţŋÖîčÈďť. ŋťłźşÈ ğĳęÛáďťğÏá ğťďÿĺĳďÆňÇ ğźčÅňÍåňÛå ŋťłźşÈ ĺĳąÿčť, N ňÆęĳ łÍåŋÍòşťąĳ čÍíňÿąťąÈ ĺťęÉîčÈďť.

-----Additional Block Devices

[ ] Loopback device Support

--> şťčťňÇ šťňÝåňÛå şťčťňÇ šťňÝåłÈłÆśÎíňÆęĳńÿ ňÝáłÝÞşťąźćÛí ŋÈňŒáşţŋÖîčÈďť.

ňżęÛå ďÛåŋťğÏá, šÛåęĳšÈ ďÈłÆřÆňÇ ňÈğÈŋÈ šťňÝåňÈčť CD-ROM ňÛå ąÖîąÈ ňÄşÉá šťňÝåňÛå ğÉáďÛåňÍñňÛåěţ, ąÆ ňÈğÈŋÈęÛå şťčťňÇ šťňÝåłÈłÆśÎí ňÆęĳńÿ ňÝáłÝÞşÉíňÆęĳńÿ ąÆ šťňÝåňÇ čţňÕòňÛå şÒÞňÝáşťąźćÛí şţŋÖîčÈďť. ŋťłÝáňÇ řÍíšÅśÿňź CD-R ňÈ ňÝñčÛá łťęÉíňÛá łÍáśÊÞşÉîčÈďť.

[ ] Network block device Support

[ ] Multiple devices driver Support

-->ďťŋÖò ŋÉòŕÈ ŋÈňŒáňÛå ŋÈňŒáşťąźćÛí şţŋÁčÛá şţŋÖîčÈďť.

ňžęÿąţňÇ şťďÆďÈłÆřÆňź ňÝñčÛá šťśÈłÏáňÛå ğÖSSňÿłÿ şťčťňÇ čÑáęÈŋÍÞňÝá ďÆęťňÈĺÆęÛå łťňÕòşÉåłÁ ňÝñąźćÛí şţŋÖîčÈďť.

ňżęÛå ďÛåňÿłÿ ňÕòęËòňÈ ŋÉÞňÛá ňžęÿąţňÇ şťďÆďÈłÆřÆęÛå ąťŋÈąĳ ňÝñčÛá łťňÕòŋťňźąźčÛá ňÅňÕòşÉá łÍåŋÍòňÝîčÈďť.

< > Linear (append) mode

 --> Multiple devices driver support ęÛå ŕźřÆşťğÏá şÒåłÍòş¡ď£čÛá

łÍåŋÍòňÆęĳńÿ, ňžęÿąţňÇ şťďÆďÈłÆřÆňź ňÝñčÛá šťśÈłÏáňÛå ďÉáłÖáşťąź čťňÏåşťčÛá ĺÉòłÝÞňÛå ŋÈňŒáşÉîčÈďť.

     < > RAID-0 (striping) mode

     < > RAID-1 (mirroring) mode

     < > RAID-4/RAID-5 mode

< > RAM disk support

--> ğźğĳęÈňÇ ňÝåĺÁęÛå şťďÆ ďÈłÆřÆ ŕÿęÍí łťňÕòşťąź ŋÈňŒáşţŋÁčÛá

şÉòğÑÞňÆęĳ,ęÊí ďÈłÆřÆęĳ łÍåŋÍòďÔá ğźğĳęÈčÛá şťďÆ ďÈłÆřÆň¡ ğťŕÉáąťŋÈęĳ łťňÕòşÉå łÁąť ňÝñłÛîčÈďť.

łÑÞďĳğÏáňźłÿ şťďÆďÈłÆřÆň¡čÛá ĺÈąÀşÉåłÁ ňÍïňÛå ğÉářÛí ľťęÛîčÈďť. ąÆęÿčť ňÝåĺÉá łťňÕòŋťňźąźčÛá šÝåňÀňÍïčÛá şÉòğÑÞňÈğž, ğźğĳęÈ ňËòňÈ ŕÖòĺÖáşÉá łťňÕòŋťčÛá şÉá ĺÍá łÍáśÊÞşţĺÑîčÈďť.

[ ] Initial RAM disk(initrd) support

--> ęÊí ďÈłÆřÆęÛå Lilo ň¡ ąÉöňÛá ĺÁśÝò ąÒáęÈŋťňź ďÛòęÑÞňÛå şţłÿ

ĺÁśÝòňÈ łÝåşÊòď£ąÈ ŋÍáňź ęÊí ďÈłÆřÆňź ňÝñčÛá ğÍáŋÿ łÝåşÊòłÈřÝåłÁ ňÝñďĳęÑÞ şţŋÖîčÈďť.ęÊí ďÈłÆřÆęÛå łÍåŋÍòşÉá łťňÕòŋťčÛá ňÈ şÉòğÑÞďĳ ąÉöňÈ łÍåŋÍòşťąÈ ĺťęÉîčÈďť.

< > XT haddisk support

--> XT ęÛå łťňÕòşťďÍá 8BIT şťďÆ ďÈłÆřÆ řÍáśÆęÑåęÿęÛå ŋÈňŒáşťąźćÛí

şţŋÖîčÈďť.

[ ] Parallel port IDE device Support

Networking Options

  < > Packet Socket

  [ ] Kernel/User netlink Socket

  [ ] Routing messages

    < > Netlink device emulation

  [ ] Network firewalls

 --> ęÈčÖÞłÆ łÈłÆśÎíňÛå čźśÆňÂřÆ šťňÈňÿňŒåęĳ ŋÉÞďÑòşťďĳęÑÞ şţŋÖîčÈďť.

šťňÈňÿňŒåęĳ ęÈčÖÞłÆ łÈłÆśÎíňÛå ŋÉÞďÑòłÈřÈğÏá čźřÆňÂřÆ łÉòňźłÿ ĺĳňÒáňÛå ňÅŋÈłÈřžŋÖîčÈďť.ŋťłÝáňÇ ęÈčÖÞłÆ ĺÉÞłÆąť ĺÉòş¡ĺÏÞňÇ ąÈčÛòňÛå şťąĳŋť şÉáďťğÏá łÍáśÊÞşťąÈ ĺťęÉîčÈďť.

ňÈ şÉòğÑÞňÛå łÍåŋÍòşťğÏá, čźśÆňÂřÆ łÑÞďĳąť ěÍåňÿŋÈčÛá ąÍðňÛå ąÉíłÁşţňű şÉîčÈďť.ąÆęÈąĳ, şÏáŋţ ęÈčÖÞłÆ łÈłÆśÎíňÇ čźśÆňÂřÆąť TCP/IP ęĳ ŋÉÞďÑòşťąĳ ňÝñňÆğÏá,IP firewalling şÉòğÑÞďĳ łÍáśÊÞşÉîčÈďť.

[ ] Socket filtering

< > Unix domain Sockets

[ ] TCP/IP networking

-->ęÈčÖÞłÆ łÈłÆśÎíňÈ TCP/IP čźśÆňÂřÆąť ď£ąź ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

    TCP/IP čÛá ŋÈňÏÞ čźśÆňÂřÆ ğÝô ňÝáśÿčÎð šÀŋÖá šÆęĳśĳřÑåňÈğž,

ňÝáśÿčÎðňÛå śÑòşťŋÈ ňÉãčÛá Standalone řÍíšÅśÿęť şÉåŋÈęťďĳ, TCP/IP čÛá šÝåňÀşÉîčÈďť.termą¡ XWindow ąÉöňÛá šÆęĳąÆęÊíňÛá TCP/IP šÆęĳśĳřÑåňÛå łťňÕòşťąÈ ěţğÖáňÝîčÈďť.

[ ] IP: multicasting

--> čźśÆňÂřÆ łÉòňźłÿ ęÈčÖÞłÆ łÈłÆśÎíňÛå ğÍåśÈ řţłÆśÝòňÈ ąťčÛòşťąź

şţŋÖîčÈďť.ğÍåśÈ řţłÆśÝòňÈęÉá, čźśÆňÂřÆ łÉòňź ňÏáąÏåďÔá řÍíšÅśÿňźłÿ čźśÆňÂřÆňÇ ğĳďÛá şĳłÆśÆęĳďźňÈśÿęÛå ĺĳčţčÛá ąÍðňÛå ňÇğÈşÉîčÈďť. IP:forwarding/gatewaying ęÛå łÍáśÊÞşťňÏñňÆğÏá, ňÈąÍðďĳ łÍáśÊÞşÉîčÈďť.

[ ] IP: Advanced router

[ ] IP: ketnel Level autoconfiguration

[ ] IP: Optimize as router not host

< > IP: Tunneling

--> şťčťňÇ šÆęĳśĳřÑå şÏòłÝÞňÇ ŋťęÀęÛå řÊîłÚåňź ŋÿŋÉòşţłÿ ďťęÛá

šÆęĳśĳřÑåęĳ ŕţčÍåňÛå śÑòşţ ĺĳčÊå ěţ ňÝáłÝÞşťďĳęÑÞ ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

< > IP: GRE tunnels over IP

[*] IP: Aliasing support

 --> ň£ĺÁňźłÿ ďÉáňÝå čźśÆňÂřÆ ňÝáśÿšźňÈłÆłÉòňźłÿ şĳłÆśÆğÏòňÛå śÑòşţłÿ ŋÍîłÑÞşÉåłÁ ňÝñďĳęÑÞ şţŋÁčÛá ąÈčÛòňÝîčÈďť.

ňžęÿ ąţňÇ čźśÆňÂřÆ řťďÆąť ŋÉòŕÉÞďÔá řÍíšÅśÿňźłÿčÛá ğţňÁ ňÅňÕòşÉá ąÈčÛòňÝîčÈďť.ňÝåĺÉá łťňÕòŋťňźąźčÛá šÝåňÀňÍïčÛá ąÈčÛòňÝîčÈďť.

 [ ] IP: TCP Syncookes Support ( not enabled per deault )

 --> łÿĺÈłÆ ąÿĺÁ ąÑòąÏÞňÛå ĺÉäňÛåěţ ďţŕÿşţŋÁčÛá šţřÝðňÝîčÈďť.

    ---( it is safe to Leave these untouched )

< > IP: Riverse ARP

--> łťňÕòŋťňÇ ęÈčÖÞłÆ łÈłÆśÎíňźłÿ čźśÆňÂřÆłÉòňÇ ěĳ ďťęÛá čźřÆňÂřÆ

řÍíšÅśÿąť IP ŋÁłĳęÛå ğÖåňÿňÒñňÛåěţ, ďţďÉîňÛå şţŋÁčÛá ąÈčÛòňÝîčÈďť. ŋÛÞ,čźśÆňÂřÆłÉòňź ğÖåęžŋÝá řÍíšÅśÿňÇ ňÈďÿčÎð řťďÆňÇ ŋÁłĳčÛá ňÉåŋÈğÉá, łÈŋÉÞłÈ IP ŋÁłĳęÛå ğĳęÆąź ď£ğÏá, ňÏÞ ŋÁłĳ ąÏåą¡ŕÈęÛå ąťŋÈąĳ šÆęĳśĳřÑåňÛå ŕÉóňťŋÁčÛá ąÈčÛòňÝîčÈďť.

[*] IP: Allow large windows

       ( not recommended if < 16Mb of memory )

 --> ďţňÕòęËòňÇ ŋťęÀęÛå ŋÍáłÑòşÉå łÁ ňÝñąź şţŋÁďĳęÑÞ ŋÈňŒáşţŋÖîčÈďť.

ğźğĳęÈ 16ğźąť ňÈłÉòňÈğÏá ňÈ şÉòğÑÞňÛå łÍåŋÍòşţŋÖîčÈďť.

---

 < >The IPX protocol

 --> čźśÆňÂřÆ ňÖáňÏòŕźŋźęĳ ňÅğÏòşÉá čĳĺÎå čźśÆňÃňÿňÇ ąÈĺÑá šÆęĳśĳřÑåňÝá
   IPX šÆęĳśĳřÑåňÛå ŋÈňŒáşťąź şţŋÖîčÈďť.

čĳĺÎå čźśÆňÃňÿ šťňÝå łÈłÆśÎíňÈčť šÆęÝáśÿęÛå łťňÕòşťęžğÏá ňÈ ňÑîłÏáňÛå łÍáśÊÞşÉîčÈďť.

[ ] IPX: Full internal IPX network

-->čţĺÁ čźśÆňÂřÆłÉòňźłÿ ďťęÛá ąťłÉò čĳďÆłÉòňź łĳřÎðňÛå

ĺţĺÖáĺÉäąź şťčÛá łÍåŋÍòňÝîčÈďť.

     The IPX protocol şÉòğÑÞňÛå łÍáśÊÞşÊñďťğÏá łÍáśÊÞşÉîčÈďť.

[ ] Appletalk DDP

--> Appletalk šÆęĳśĳřÑåňÇ ŋÈňŒáňžĺÁęÛå ąÏåŋÍòşťčÛá şÉòğÑÞňÝîčÈďť.

     Appletalk čÛá ňţšÛå řÍíšÅśÿňÇ čźśÆňÂřÆ šÆęĳśĳřÑåňÝîčÈďť.

~ SCSI support

< > SCSI support

-->łÈłÆśÎíňź SCSI ŋÉòĺÈąť ňÝñďťğÏá ňÈ şÉòğÑÞňÛå łÍáśÊÞşÉîčÈďť.

--SCSI Support type (disk,tape,CD-ROM)

< > SCSI disk support

@ ò 30

-->łÈłÆśÎíňź SCSI şťďÆďÈłÆřÆčť IOMEGA parallel ZIP ďÆęťňÈĺÆęÛå

ąťŋÈąĳ ňÝñďťğÏá ňÈ şÉòğÑÞňÛå YłÍáśÊÞşÉîčÈďť.

 < > SCSI tape support

-->łÈłÆśÎíňź SCSI tapedrive ęÛå ąťŋÈąĳ ňÝñďťğÏá,łÍáśÊÞşÉîčÈďť.

 < > SCSI CD-ROM support

 -->łťňÕòŋťňÇ ęÈčÖÞłÆ łÈłÆśÎíňź SCSI CD-ROM ňÈčť CD-R ęÛå

ąťŋÈąĳ ňÝñďťğÏá, ňÈ şÉòğÑÞňÛå łÍáśÊÞşÉîčÈďť.

< > SCSI generic support

--> SCSI ňÕòňÆęĳ čťňĳčÛá ŋźšÖíŋÖòňźčÛá şťďÆďÈłÆřÆčť CD-ROM ğÉåąĳďĳ

łÁğÉãňÛá ŋźšÖíďÛåňÈ ňÝñłÛîčÈďť.

SCSI ĺÉòłÝÞňÇ łÆřţčÿčť łÝáďÈłťňÈŋÿ, CD-writer ďÛòňÛå ąťŋÈąĳ

ňÝñďťğÏá ňÈ şÉòğÑÞňÛå YES ęĳ łÍåŋÍòşťąÈ ĺťęÉîčÈďť.

  --Some SCSI device (e.g. CD jukebox) Support multiple LUNS
[ ] Probe all LUNs on each SCSI device

--> SCSI čÛá ąÉÞ SCSI ŋÉòĺÈňź čÑáęÈŋÍÞňÝá ĺÍáşĳ, ŋÛÞ(LUN) ęÛå şÉåďÉòşťčÛáďź,
     SCSI ňÿďÊîśÿ ŋÖò ĺÑÞłÁňÇ LUN ňÛå ŋÈňŒáşťčÛá ŋźšÖíďÛåňÈ ňÝñłÛîčÈďť.

ňÈęÿşÉá ĺÑÞłÁňÇ LUN ňÛå ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.

[ ] Verbose SCSI error reporting (kernel size +=12K)

--> SCSI şťďÆňÃňÿňźłÿ ňÝåňÿčťčÛá ňźęÿğźłÈŋÈęÛå ňÈşţşťąÈ łÄňÿŋÝîčÈďť.

ąťąÛîŋÍÞ SCSI ŋÉòĺÈęÛå ąťŋÈąĳ ňÝñčÛá łťňÕòŋťčÛá ňÈ şÉòğÑÞňÛå łÍáśÊÞşÉîčÈďť.

 SCSI low-level drivers -->
 < > 7000FASST SCSI support

 -->ňÃłÆśÍá ďÈŋÈśÉåłťňÇ 7000 łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.

 < > Adaptec AHA152X/2825 support
 < > Adaptec AHA1542 support
 < > Adaptec AHA1740 support
 < > Adaptec AIC7xxx support

-->ňťďÉîśÎÞłťňÇ łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.

    aic7xxx ęÛå ŋÈňŒáşťčÛá łÆřťłÈ řÍáśÆęÑåęÿşÉòğÑÞňÛá 274X EISA řťďÆ,
    284X VLB řťďÆ, 294x PCIřťďÆ, 394X PCI řťďÆ, 3985 PCI řťďÆęÛå

ŋÈňŒáşÉîčÈďť.

< > AM53/79c974 PCI SCSI support

 -->AM53/79c974 łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.

@ ò 31

Tekram DC390(T) PCI-SCSI şĳłÆśÆ ňÿďÊîśÿęÛå ąťŋÈąĳ ňÝñďťğÏá

ąÈĺÑáŋÍÞňÆęĳ DC390 ďÆęťňÈĺÿęÛå ąťŋÈąĳ ňÝñłÛîčÈďť. ňÈ şÉòğÑÞňÛá DC390 ğÝô AM53/79c974 łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşÉîčÈďť.

< > BusLogic SCSI support
-->BusLogic MultiMaster SCSI ňÿďÊîśÿęÛå ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.
< > DTC3180/3280 SCSI support
-->DTC 3180/3280 łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.
< > EATA-DMA(DPT,NEC,AT,SNI,AST,Olivetti,Alphatronix)
     support
-->SmartCache III/IV, SmartRAID, PM2011B/PM2012B ďÛòňÇ łÆřťłÈ

ňÿďÊîśÿąť łťňÕòşťčÛá EATA-DMA šÆęĳśĳřÑåňÛå ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.

< > EATA-PIO (old DPT PM2001, PM2012A) support
--> DPT PM2001, PM2012A ďÛòňÇ łÆřťłÈ ňÿďÊîśÿąť łťňÕòşťčÛá
     EATA-PIO šÆęĳśĳřÑå ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.

ňÈ ďÆęťňÈĺÿčÛá ďÉáŋÈ harddisks ğÝô lacks ňÇ ğÉãňÛá śÛÞŋÝòďÛåňÛå ŋÈňŒáşţ ŋÁčÛá ąÈčÛòňÇ ňÏÞşÉåğÉáňÛå şÉîčÈďť.

< > Future Domain 16xxSCSI support
-->Future Domain 16Bit łÆřťłÈ ňÿďÊîśÿčť Future Domain ňÇ

ŕÝîłÎðňÛå łťňÕòşťčÛá łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.

< > GDT SCSI Disk Array Controller Support
< > Generic NCR5380/53c400 SCSI support
--> NCRňÇ łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.

łÍáśÊÞşťąź ď£ğÏá ęÈčÖÞłÆ řÿčÍåňźłÿ ŋÈňŒáşťčÛá ğÉãňÛá ŋÑòęÅňÇ

  NCRłÆřťłÈ ňÿďÊîśÿęÛå łťňÕòşÉåłÁ ňÝñąź ďÔîčÈďť.

< > Initio 9100U(W) Support
< > initio INI-A100U2W Support
< > NCR5380/53c400 mapping method (use Port for T130B)
--> NCR5380 ą¡ NCR53c400 łÆřťłÈ ňÿďÊîśÿňźłÿ T130B ĺÉòłÝÞňÆęĳ

ğźğĳęÈęÛå ğţšÝò şţŋÁčÛá ąÈčÛòňÛå ŋÈňŒáşťčÛá ĺÉòłÝÞňÝîčÈďť.

< > Symbios 53c416 SCSI Support
< > NCR53c406a SCSI support
--> NCR53c406a łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşţŋÁčÛá şÉòğÑÞňÝîčÈďť.
< > NCR53c8xx SCSI support

@ ò 32

< > SYM53c8xx SCSI support

--> NCR53C8XX ążňÏåňÇ PCI ňÕò łÆřťłÈ ňÿďÊîśÿęÛå łťňÕòąťčÛòşťďĳęÑÞ

ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.Parity check, FAST SCSI II ďÛòňÛå ŋÈňŒáşťčÛáďÛò ďťňËòşÉá ąÈčÛòňÛå łťňÕòşÉåłÁ ňÝñłÛîčÈďť.

(4) Default tagged command Queue depth
(32) maximum number of queued commands

-->ňÿěÿşÉá ďţąÈğÏòęÏòňÈ ŋÁňÿŋÏñňÛåěţ, ąÆňź ěťęÛá ďÈĺťňÈłÆňź ŕ£łĳ ğÝô

ŕ£ďţ ğÏòęÏòłÁęÛå ĺÁňžşťčÛá ąÈčÛòňÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť. ąÈĺÑáŋÍÞňÆęĳ 4, ŕ£łĳąÉïňÆęĳčÛá 2, ŕ£ďţąÉïňÆęĳčÛá 12 ňÇ ğÏòęÏòłÁęÛå ĺÁňžşţŋÖîčÈďť.

(20) synchronous transfers frequency in MHz
[ ] enable profiling
[ ] use normal IO

-->X86ňÛå ąÈĺÉáňÆęĳşťčÛá łÈłÆśÎíňźłÿ ğźğĳęÈňÇ IOęÛå ğţšÝòşţŋÁčÛá

ąÈčÛòňÛå ŋÈňŒáşÉîčÈďť.

[ ] Include support for the NCR PQS/PDS SCSI card
< > PAS16 SCSI support

 -->PAS 16 łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşţŋÁčÛá şÉòğÑÞňÝîčÈďť.

< > PCi2000 support
< > PCi2220i support
< > PCi2240i support
< > Qlogic FAS SCSI support

-->Qlogic ňÇ FastSCSI ęÛå ŋÈňŒáşţŋÁčÛá şÉòğÑÞňÝîčÈďť.

ŋÈňŒáşťčÛá şÉòğÑÞňÛá PCI ĺÉòłÝÞňÈ ňťčÝá ISA, VLB, PCMCIA ĺÉòłÝÞňÝîčÈďť.

< > Qlogic ISP SCSI support

 -->PCI ĺÉòłÝÞňÇ łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşţŋÁčÛá şÉòğÑÞňÝîčÈďť.

< > Qlogic ISP FC support
< > Seagate ST-02 and Future Domain TMC-8xx SCSI support

-->8BIT ňÕò łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşţŋÁčÛá şÉòğÑÞşÉîčÈďť.

< > Tekram DC-390(T) SCSI support

 -->Am53C974A ŕÝîňÛå łťňÕòşťčÛá Tekram DC390(T) PCI łÆřťłÈ

ňÿďÊîśÿęÛå ŋÈňŒáşţŋÁčÛá şÉòğÑÞňÝîčÈďť.

< > Trantor T128/T128F/T228 SCSI support

@ ò 33

--> Trantor T128/T128F/T228 łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşţŋÁčÛá şÉòğÑÞňÝîčÈďť.
< > UltraStor 14F/34F support
 -->UltraStor 14F/34F łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşţŋÁčÛá şÉòğÑÞňÝîčÈďť.
< > UltraStor SCSI support
 -->UltraStor 14F/34F ň£ňź 24F ďÛòňÇ łÆřťłÈ ňÿďÊîśÿęÛå ŋÈňŒáşÉîčÈďť.
     UltraStor 14F/34F ŋÈňŒáşÉòğÑÞą¡ ąÏîŕÈčÛá łÆřťłÈ ňÿďÊîśÿąť ňÝñčÛáďź,

ďÖåŋÖòňÇ şťčťęÛå łÍáśÊÞşţňűğÉá şÉîčÈďť. ~ Network Device support

[ ] Network device support

-->ŋťłÝáňÇ řÍíšÅśÿąť čźśÆňÂřÆňź ňÏáąÏåď£ňÿ ňÝñąÿčť SLIPňÈčť PPPęÛå

łťňÕòşťęžğÏá łÍáśÊÞşÉîčÈďť.

< > ARCnet Support
-->ARCnet ŕÝîłÎðňÈ ňÝñčÛá čźśÆňÂřÆ řťďÆęÛå ąťŋÈąĳ ňÝñďťğÏá łÍáśÊÞşÉîčÈďť.
< > Dummy net driver support
-->IP ňÿďÆęźłÆęÛå ąÁłÍòşťčÛáďź ňÝñňÿłÿ šÝåłÁŋÍÞňÝá ďÈĺťňÈłÆęÛå

ŋźąÑòşÉîčÈďť.SLIPňÈčť PPPęÛå łťňÕòşÉáďťğÏá Yęĳ łÍåŋÍòşťąÈ ĺťęÉîčÈďť.

< > EQL (serial line load balancing) support

-->şÉá řÍíšÅśÿňź ďÁąţňÇ ğĳďÎíą¡ ŋÍáş¡łÍá ďÁąţęÛå ňÈňÕòşťňž ďÑòłÈňź

ŋÍîłÑÞşÉåłÁ ňÝñąź şţŋÖîčÈďť.ďťęÛá řÍíšÅśÿň¡ 2ąţňÇ łÈęÈňÍå ňÏáąÏåňÈ ď£ňÿ ňÝñňÆğž, ąÆąÍðňÛå śÑòşţ SLIPňÈčť PPPęÛå łťňÕòşÉáďťğÏá, ňÈ ňÑîłÏáňÆęĳ 2ąţęÛå şťčťęĳ ğÉáďÛåňÿŋÁňÿ 2ĺţňÇ łÑÞďĳęÛå čÊå łÁ ňÝñąź şţŋÖîčÈďť.

[ ] Ethernet (10 or 100Mbit)

-->ęÊářťďÆąť ňÝñňÛåłÈňźčÛá ňÈ şÉòğÑÞňÛå łÍáśÊÞşţ ŋÖîčÈďť.

[ ] 3COM cards
  < > 3c501 support
  < > 3c503 support
  < > 3c505 support
  < > 3c507 support

@ ò 34

  < > 3c509/3c579 support
  < > 3c515 ISA Fast EtherLink
  < > 3c590/3c900 series (592/595/597/900/905) "Vortex/Boomerang"
       support

 -->ňÈ şÉòğÑÞňÛá 3COM čźśÆňÂřÆ řťďÆęÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

AMD LANCE and PCnet (AT1500 and NE2100) support

-->AT1500 ěĳčÛá NE2000 şĳşÒáňÝá AMD LANCE/PCnet łÆřťłÈ

ňÿďÊîśÿęÛå ŋÈňŒáşţŋÁčÛá şÉòğÑÞňÝîčÈďť.

[ ] Western Digital/SMC cards

 -->Western Digital/SMC čźśÆňÂřÆ řťďÆęÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

[ ] Racal-interlan (Micom) NI cards
[ ] Other ISA cards

-->łÍåŕÈďÔá čźřÆňÂřÆ řťďÆąť ňÄňÇ şţďÉòłťşÉòňź ňÍïąÿčť.

čźśÆňÂřÆ řťďÆąť ISA ňÕòňÝåěţňźčÛá ňÈ şÉòğÑÞňÛå łÍáśÊÞşÉîčÈďť.

[ ] EISA,VLB.PCI and on board controllers

-->ĺĳďÆňź čţŋÉòďÔá čźśÆňÂřÆ řťďÆęÛå ąťŋÝá łťňÕòŋťęťğÏá ňÈ şÉòğÑÞňÛå

łÍáśÊÞşÉîčÈďť.

< > AMD PCInet32 (VLB and PCI) support

-->PCI ğÝô VLB ĺÉòłÝÞňÛå ŋÈňŒáşťčÛá AMD PCInet32 łÆřťłÈ ňÿďÊîśÿęÛå

łťňÕòąťčÛòşťďĳęÑÞ ŋÈňŒáşţŋÁčÛá şÉòğÑÞňÝîčÈďť.

< > Apricot Xen-II on board Ethernet
< > CS8x0 support
< > Generic DECchip & DIGITAL EtherWORKS PCI/EISA
< > DECchip Tulip (dc21x4x) PCI support
< > Digi Intl . RightSwitch SE-X support
< > EtherExpressPro/100 support

-->ňÈďÿčÎð čźśÆňÂřÆ ňÝáśÿšźňÈłÆ řťďÆ(NIC)ąť łÍåŕÈď£ňÍñďťğÏá

łÍáśÊÞşÉîčÈďť.

< > PCI NE2000 support

 -->PCI ĺÉòłÝÞňÇ NE2000 čźśÆňÂřÆ řťďÆęÛå ŋÈňŒáşţŋÁčÛá şÉòğÑÞňÝîčÈďť.

< > TI ThunderLAN support
< > IA Rhine support
 [ ] Pocket and portable adaptors
 [ ] FDDI driver support

< > Frame relay DLCI support
<M> PPP (point-to-point) support

-->šźęÿęÎå šĳśÆň¡ řÆęĳłÆ řźňÈĺÛåňÛå ňÈňÕòşţ ďÁ ęÈčÖÞłÆ ĺÉÞłÆęÛå

ňÏáąÏåşÉåłÁ ňÝñłÛîčÈďť.

TCP/IPęÛå ňÈňÕòşťğž "FX"řźňÈĺÛåňÛå śÑòşţłÿ 4bits ńÝÞ

ŋÍáłÑòşÉå łÁ ňÝñčÛá mode0ň¡ śÛÞĺÏåşÉá PILPřźňÈĺÛåňÛå ňÈňÕòşţ 8bitsńÝÞ ŋÍáłÑòşÉå łÁ ňÝñčÛá mode1ňÈ ŋźąÑòďÔîčÈďť.

<*> SLIP (serial line) support

   -->PPP ňÈŋÍáňź ğÉãňÈ łťňÕòşÊñďÍá łÈęÈňÍå ęťňÝáňÛå ŋÈňŒáşťčÛá čźśÆňÂřÆ

šÆęĳśĳřÑåňÝîčÈďť.

[ ] Wireless LAN (non - hamradio)

  -->RADIOň¡ ğÁłÍá LANňÛå ŋÈňŒáşÉîčÈďť.

[ ] Token Ring driver support

 -->IBM łťňÇ ŋźšÑíňźłÿ ęĳřÍå čźśÆňÂřÆęÛå ňÏáąÏåşťčÛá śĳřÛáęÝò ĺÉòłÝÞňÇ

ďÆęťňÈĺÿęÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

śĳřÛá ęÝò řťďÆęÛå łťňÕòşťęžğÏá ňÈąÍðňÛå łÍáśÊÞşÉîčÈďť.

< > Comtrol Hostess SV-11 support
< > COSA/SRP sysc serial boards support
< > Red Creek Hardware VPN (EXPERIMENTAL)
[ ] WAN drivers

~ Amateur Radio Support

[ ] Amateur Radio Support
  --packet radio protocols
< > Amateur Radio AX.25 Level 2 protocols
  --Misc hamradio Protocols

~ IrDA Subsystem Support

-->ŋÍÞň£łÍáňÛå ňÈňÕòşÉá ąÛáąÿęÈ ğÁłÍáśÑòłÝáňÈčť šÆęÝáśÿ,łÈęÈňÍå ŋÉòŕÈ ďÛòňÇ

šÀŋÖá šÆęĳśĳřÑåňÛå ŋÈňŒáşÉîčÈďť.

ŋÈąÛíňÛá ŋÑí čÉółÍåŋÈğÉá ŋĳğÉáąÉáňź ňťŋÁ ňÝÞłÖÞşţŋÝå ňÅňÕòşÉá ąÈčÛòňÝîčÈďť. łÊòąÉÞşţĺĳŋÀ ążłÉáąÈğÉáşÉá řÍíšÅśÿęÛå ąťŋÈąĳ ďťčÈďť ğÁłÍáňÆęĳ ąÛáŕÿňź ŋÍîąÛáşťčÛá ąÍðğÉáňÆęĳ ŋťęÀąť ŋÍáłÑòďÔáďťğÏá..

ĺÍåńÿ łÎåĺÝÞąÉöňÛá PDAŋÑòęÅčť ąĳąÛîłťňËòňÇ čĳśÆĺÖÞňźłÍá ŋÈňŒáşťąĳ ňÝñłÛîčÈďť. šÝåŋťčÛá ňÈŋÍòďĳĺÉSSňź ğĳęÆŋÈğÉá ňÉœňÆęĳ ğÉãňÈ ňÈňÕòďÔå ąÈłÖåňÈčÈ ňťęţňÇ ąÈłÖåňÛå łÍåğÏòşÉåłÁ ňÝñčÛá ĺÖáňÈ ňÝñďťğÏá ďÊðąÛåňÛå ďÉåňťłÿ ďÿ łÉåňÛå ĺÖöňž

@ ò 36

ŋÑíďÿ ğÉãňÛá ęÈčÖÞłÿąť ąÑòňÅşťąź ď£ąÝå ĺÝîčÈďť.

< > IrDA Subsystem Support
< > IrDA subsystem support
---IrDA protocols
< > IrLAN protocols
< > IrCOMM protocols
< > IrLPT protocols
    < > IrLPT client support
    < > IrLPT server support
< > IrDA protocol options
--- IrDA options
[ ] Cache last LSAP
[ ] Fast RRs
[ ] Debug infomation
[ ] IrLAP compression
 Infrared-port device drivers -->
       --- SIR device drivers
      < > IrTTY (users linux serial driver )
            IrPORT (IrDA serial driver)
       --- FIR device drivers
      < > NSC PC87108
      < > Winbond W83977AF (IR)
      < > Sharp UIRCC
      < > Toshiba Type-0 IR Port
      < > SMC IrCC
       --- Dongle support
      [ ] Serial dongle support
      < > ESI JetEye PC dongle
      < > ACTiSYS IR-220L and IR220L+ dongle
      < > Tekram IrMate 210B dongle
      < > Greenwich GirBIL dongle
      < > Parallax LiteLink dongle

~ ISDN subsystem

-->ňÍåğťŋÍáğÉáşţďĳ łÊòłĳşÊñďÍá ąÈłÖåňÈŋÈğÉá ňÈŋźčÛá ğĳďÎíŕÿęÍí şÛáşţŋÏñłÛîčÈďť.

ňÈŋź ąÑä ęÈčÖÞłÆąť ŋź şÝíą¡ ąÈłÖåňÛå ĺÉåşÄşÉåłÁ ňÝñčÛá ąĳłÑÞ čźřÆňÂřÆňÇ łźążęĳ łÍòřÛí ďťąťąÉá ąÍð ąÉöňťłÿ ąÈĺÖáňÈ ŋÑøňťŋÈčÛáąÖáňÀ..(^___^);; ňžęÿĺÖáďĳ ňťłÈąÎñŋÈğÉá ęÈčÖÞłÆčÛá čźśÆňÂřÆň¡ ňÏáąÏåďÔå ěţ ğÁşÉáňÇ ąÈčÛòą¡ şÝíňÛå ĺÉåşÄşÉîčÈďť.

ňÑåşţĺÁśÿ ĺÁőÍÞ čÛåňÿčÉá ąÉÞ śÑòłÝáłťňÇ ISDN ąÒòąĳěĳşÉá ęÈčÖÞłÆňźłÿňÇ

ISDNŋÈňŒáňź şÝíňÛå ŋÁąĳ ňÝñłÛîčÈďť.

< > ISDN support

--> ISDN řťďÆęÛå ňÈňÕòşţłÿ čźśÆňÂřÆčť ňÝáśÿčÎðňÛå łťňÕòşťęžğÏá

ňÈ şÉòğÑÞňÛå łÍáśÊÞşÉîčÈďť.

@ ò 37

[ ] Support synchronous PPP
 -->ISDN ňÛå śÑòşţ ďÑòąÈş¡ďÔá PPP ęÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

ďÑòąÈş¡ďÔá PPP čÛá ŋÁęĳ SUN ňÈčť CISCO ňźłÿ łťňÕòď£ňÿŋÝîčÈďť.

[ ] Use VJ-compression with synchronous PPP

-->ďÑòąÈş¡ďÔá PPPňźłÿ VJ ňÉîŕÖÞ(Van Jacobson header compression)ňÛå

ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.

[ ] Support audio via ISDN
 -->ISDN ňÛå śÑòşţ ňÛíłÍòąÈčÛòňÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

ŋťłÝáňÇ ęÈčÖÞłÆ ĺÉÞłÆąť ISDN ęÛå śÑòşţ ňÛíłÍò śÑòş¡ąť ąťčÛòşťąź şťęžğÏá,ňÈ ąÈčÛòňÛå łÍáśÊÞşÉîčÈďť.

 [ ] X.25 PLP on top of ISDN (Experimental)
 < > ICN 2B and 4B support
-->ICN ňÈęť ĺÖåęÈčÛá ďÁ ŋÑòęÅňÇ ISDN řťďÆęÛå ğĳďÁ ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.
    ICN 2B čÛá şťčťňÇ ISDN ęťňÝáňź 2ąţňÇ B ŕţčÍåňÛå ąťŋÝá
    ISDN šÀŋÖáĺÉòłÝÞňÝîčÈďť. ICN 4B čÛá ďÁąţňÇ ISDN ęťňÝáňÛå ŋÈňŒáşÉîčÈďť.
 < > ISDNloop Support

 -->śźłÆśÆęÛå ňÄşÉá ąťłÉò ISDN CardęÛå ŋźąÑòşţ ŋÖîčÈďť.

 < > PCBIT-D support

 -->ňÈ şÉòğÑÞňÛá šĳśÆśÁřÉåňÇ Octal łťąť ğÉáďÛåňÿčÊá PCBIT ISDN řťďÆęÛå

ŋÈňŒáşťčÛá şÉòğÑÞňÝîčÈďť.

 < > HiSax SiemensChipSet driver support
  -->Siemens Chipset ęÛå łťňÕòşťčÛá AVM A1, Elsa ISDN cards,
     Teles S0-16.0, Teles S0-16.3,Teles S0-8, Teles/Creatix PnP,
     ITK micro ix1 ďÛò ISDN řťďÆęÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.
< > AVM-B1 with CAPI2.0 support
 -->CAPI2.0 ňÝáśÿšźňÈłÆęÛå ŋÉòŕÉÞşÉá AVM B1 řťďÆęÛå ŋÈňŒáşţŋÁčÛá

şÉòğÑÞňÝîčÈďť.

~ OLD CD-ROM drivers(not for SCSI or IDE/ATAPI drives)

[ ] Support non-SCSI/IDE/ATAPI CDROM drives

 -->ęÈčÖÞłÆ ĺÉÞłÆňź łÍåŕÈďÔá CD-ROM ęÛå ŋÈňŒáśĳęÑÞ şţŋÁčÛá ąÈčÛòňÝîčÈďť.

@ ò 38 ňÀŋÛí čťňĳčÛá CD-ROM ňÛá IDE čť ATAPI ĺÉòłÝÞňÆęĳ ŋÉÞďÑòď£čÛá

CD-ROM ňÈğÆęĳ şţďÉòłťşÉòňÈ ňÍïąĳ,IDE čť ATAPI ąť

čťňĳąÈŋÍáňÇ ąÁşÏòğĳďÎåňÇ CD-ROM ňÛå ŋÈňŒáşţ ŋÖîčÈďť.

   SCSI CD-ROM ęÛå ąťŋÈąĳ ňÝñčÛá łťňÕòŋť ěĳşÉá šÝåňÀňÍïčÛá ąÈčÛòňÝîčÈďť.

< > Aztech/Orchid/Okano/Wearnes/TXC/CyDROM CDROM support
-->Aztech łťňÇ CDA268-01A, Orchid łťňÇ CD-3110,
   Okano ň¡ WearnessňÇ CDD110, Conrad łťňÇ TXC ğÝô CyDROM ňÇ
   CD-ROM ňÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.
< > Goldstar R420 CDROM support
-->LGňÇ ŕĳŕÉòąÈ ğĳďÎåňÈňÍñďÍá R420 CD-ROM ňÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.
< > Matsushita/Panasonic/Creative, Longshine, TEAC CDROM support

 -->ğťőÆłÈďť CR-521, CR-522, CR-523, CR-562, CR-563 CD-ROM ğÝô

řÆęÈňźňÈśÈĺÆęÊîňÇ CD200,Longshine łťňÇ LCS-7260,TEAC łťňÇ

CD-55A CD-ROM ďÛòňÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

łťňÖáďÆ ĺÛåęťłÆśÿň¡ şÉíćź ňÝñďÍá CD-ROM ďÛåňÈ ďţĺÁĺÖáňÈğž, ňÈŋÍáňź łťňÖáďÆ ĺÛåęťłÆśÿň¡ şÉíćź CD-ROM ňÛå ąÁňÝîşÉá łťňÕòŋťęťğÏá ďţĺÁĺÖá ňÈ şÉòğÑÞňź ďÛåňÿąÉå ąÍðňÝîčÈďť.

< > Mitsumi (standard) [no XA/Multisession] CDROM support

 -->ğÈőÆğÈłťňźłÿ ŋźŋÉÞďÔá LU-005, FX-001, FX-001D CD-ROMęÛå

ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť. ğÈőÆğÈłťňÇ FX-001DE CD-ROM ęÛå ąťŋÈąĳ ňÝñčÛá łťňÕòŋťęťğÏá łÍáśÊÞşţłÿčÛá ňÉáďÔîčÈďť.

    FX-001DE CD-ROM ňÛá IDE/ATAPI ĺÉòłÝÞňÛå ŋÈňŒáşťąÈ ěţğÖáňÝîčÈďť.
< > Mitsumi [XA/MultiSession] CDROM support

 -->ğÈőÆğÈłťňźłÿ ŋźŋÉÞďÔá LU-005, FX-001, FX-001D CD-ROM ęÛå

ŋÈňŒáşÉîčÈďť.ňÈşÉòğÑÞňÛá XA ĺÉòłÝÞňÈčť Photo CD ęÛå ŋÈňŒáşťąÈďĳ şÉîčÈďť.

< > Optics Storage DOLPHIN 8000AT CDROM support
  -->34šÝá řźňÈĺÛåęĳ ŋÉÞďÑòď£čÛá DOLPHIN ňÇ CD-ROM ęÛå ŋÈňŒáşÉîčÈďť.
< > Philips/LMS CM206 CDROM support
 -->CM260 ňÈęťčÛá ňÿďÊîśÿřťďÆęÛå ňÈňÕòşťčÛá šÝåęÝîłÆłťňÇ
     CM206 CD-ROM ęÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.
< > Sanyo CDR-H94A CDROM support

 -->ňÈ şÉòğÑÞňÛá łÉáňÀłťňÇ CDR-H94A CD-ROM ęÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

@ ò 39

< > ISP16/MAD16/Mozart soft configurable cdrom interface support

 -->ISP16, MAD16, Mozart ďÛòňÇ CD-ROM ňÝáśÿšźňÈłÆ řťďÆęÛå

ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

< > Sony CDU31A/CDU33A CDROM support

 -->ňżŋÍáňÇ SONY łťňÇ CD-ROM ŋźšÖíąÖáňÛá ďÑåšÝá ŋźšÖíąÖáą¡ ğťŕÉáąťŋÈęĳ
   34šÝá řźňÈĺÛåňÛå łťňÕòşťňÏñłÛîčÈďť. ňÈ ŋźšÖí ěĳşÉá 34šÝá řźňÈĺÛåňÛå

łťňÕòşťčÛá SONY łťňÇ CDU33A CD-ROMňÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

< > Sony CDU535 CDROM support

 -->SONY łťňÇ 34šÝá řźňÈĺÛåňÛå łťňÕòşťčÛá CDU535 ğÝô CDU-531
     CD-ROM ęÛå ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

~ Character devices

[ ] Vitual terminal

-->ňžęÿąţňÇ ąťłÉò śÿğÈčÍåňÛå łÝåşÊòşÉåłÁ ňÝñčÛá ąÍðňÛá ňťğť ęÈčÖÞłÆňźłÿğÉá

čÆćÝåłÁ ňÝñčÛá ąÉòęÏÞşÉá ąÈčÛòňÈ ňťčÝáąť şÉîčÈďť. ğÖåęÑá ňžęÿąţňÇ X śÿğÈčÍåďĳ ąťčÛòşťąź şţŋÖîčÈďť.

[ ] Support for console on Vitual terminal
< > Standard/generic (dumb) Serial Support

-->ňÝåĺÉáŋÍÞňÝá łÈęÈňÍå šĳśÆęÛå łťňÕòąťčÛòşťďĳęÑÞ ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť,

ňÈďÿčÎðňÛå śÑòşţłÿ ňØî łÿĺÿęÛå ąÁŕÖÞşťňÏñąÿčť,ňÝåĺÉá łÈęÈňÍå ğťňÁłÆęÛå łťňÕòşťŋÈ ňÉãąĳ ĺÿłÆğťňÁłÆęÛå łťňÕòşťčÛá łťňÕòŋťčÛá łÍáśÊÞşťŋÈ ňÉãďĳęÑÞ şÉîčÈďť.ňžąÈłÿčÛá łÈęÈňÍå šĳśÆęÛå łťňÕòşťčÛá łťňÕòŋťğÉá łÍáśÊÞşťąÈ ĺťęÉîčÈďť.

[ ] Support for console on Serial port

-->łÈłÆśÎí řÑáłÑåňÛá ğĳďÛá řÿčÍå ğźłÈŋÈň¡ ąÏòąĳ ğźłÈŋÈęÛå łÁŕÄşťąĳ ,

ďÉáďÑÞ łťňÕòŋť ğĳďÆňźłÿ ęĳąÆňÝáňÛå şÿňÕòşťčÛá ŋÉòŕÈňÝîčÈďť. łÍáśÊÞłÈ "console=tty3"ň¡ ąÉöňÛá ğÏòęÏòňÛå łťňÕòşťňž łÈłÆśÎířÑáłÑåęĳ łťňÕòşÉå łÁ ňÝñłÛîčÈďť.

[ ] Extended dumb Serial driver options
  [ ] Support more than 4 serial ports
  [ ] Support for Sharing Serial ports (unsafe)
  [ ] Autodetect IRQ on Standard ports
  [ ] Support special multiport boards
  [ ] Support the Bell Technologies HUB6 card
[ ] Non-Standard Serial port Support
[ ] Unix98 PTY Support
  (256) Maximum number of Unix98 PTYS in use (0-2048)

< > Parallel printer Support

-->25šÝá őťęÈ šţęÿęÍå šĳśÆęÛå łťňÕòşťčÛá šÆęÝáśÿęÛå łťňÕòąťčÛòşťďĳęÑÞ

ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť. ňžąÈłÿ ŋÁňÇşÉå ŋÍíňÛá ďÁąţňÇ šţęÿęÍå šĳśÆ(printer ň¡ PLIP)ęÛå şÉíćź łťňÕòşťčÛá łťňÕòŋťčÛá ňÈ şÉòğÑÞą¡ PLIP şÉòğÑÞňÛå ąÉöňÈ ğĳďÚå(M) ęĳńÿ łÍåŋÍòşťąÈ ĺťęÉîčÈďť. ďÁąţňÇ šţęÿęÍå šĳśÆęÛå ąÉÞąÉÞ ěťęĳ łťňÕòşťčÛá łťňÕòŋťęťğÏá łÍáśÊÞşÉîčÈďť.

[ ] Mouse Support (not serial mice)

-->łÈęÈňÍå ğťňÁłÆčť ğťňÈřÆęĳ şĳşÒá ğťňÁłÆęÛå łťňÕòşťŋÈ ňÉãčÛá ĺÿłÆ

ğťňÁłÆčť PS/2 ğťňÁłÆ łťňÕòŋťňźąź şţďÉòď£čÛá łťşÉòňÝîčÈďť.

Mice--->

  [ ] Mouse Support (not serial mouse)

  -->łÈęÈňÍå ğťňÁłÆęÛå ŋźň£şÉá ŋÉòŕÈęÛå łťňÕòąťčÛòřź şţŋÖîčÈďť.

  < > ATIXL busmouse support

 -->ňÈ ĺÿłÆğťňÁłÆčÛá ATI ąÆęţšÝÞ řťďÆňÇ ďÙðğÏáňź ćÑîčÛá ňÀŋÛíňÛá ĺĳąÈ

şÝíďÛá ğťňÁłÆňÝîčÈďť.

< > Logitech busmouse support

-->9šÝá őťęÈňÇ ęĳŋÈśÎÞ ĺÿłÆ ğťňÁłÆęÛå łťňÕòąťčÛòşťďĳęÑÞ ŋÈňŒáşţŋÁčÛá

ąÈčÛòňÝîčÈďť.

< > Microsoft busmouse support

 -->ďţąţ şÒÞŋÉò ĺĳďÆňź łÉîňÝîď£čÛá 9šÝá őťęÈňÇ ňŒáşÏò šĳśÆňź ćÑîşÈčÛá

ğťňÈřÆęĳłĳšÆśÆ ĺÿłÆğťňÁłÆęÛå łťňÕòąťčÛòşťďĳęÑÞ ŋÈňŒáşÉîčÈďť.

[ ] PS/2 mouse (aka "auxiliary device") support

-->PS/2 ğťňÁłÆęÛå ŋÈňŒáşťčÛá şÉòğÑÞňÆęĳ, ATX ĺĳďÆęÛå ŋÉòŕÉÞşÉá

ęÈčÖÞłÆĺÉÞłÆ ęťğÏá ňÝåĺÉáŋÍÞňÆęĳ PS/2 ğťňÁłÆ šĳśÆęÛå ąťŋÈąĳ ňÝñłÛîčÈďť.ňŒáşÏòňÇ 6šÝáőťęÈ šĳśÆęÛå ąťŋÝá ğťňÁłÆęťğÏá PS/2 ğťňÁłÆňÝîčÈďť.

[ ] C 82C710 mouse port support (as on TI Travelmate)

-->PS/2 ğťňÁłÆňÇ ŋÑòęÅňÝá C 82c710 ğťňÁłÆ šĳśÆęÛå łťňÕòąťčÛòşťďĳęÑÞ

ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

  < > PC110 digitizar pad Support

[ ] QIC-02 tape support

-->łÆřťłÈ ĺÉòłÝÞňÈ ňťčÝá śźňÈšÆ ďÆęťňÈĺÿęÛå łťňÕòąťčÛòşťďĳęÑÞ ŋÈňŒáşţŋÁčÛá

ąÈčÛòňÝîčÈďť.

@ ò 41

[ ] Watchdog Timer Support

-->WatchdogęťčÛá ąÈčÛòňÛå łťňÕòąťčÛòşťďĳęÑÞ şţŋÁčÛá ąÈčÛòňÝîčÈďť.

ňÈąÈčÛòňÛá ňÿěÿşÉá šťňÝåňÛå ňÏåąÿčť ňÿěÍá šťňÝåňź ńÆčÛá ňÝåňÛå 1ĺÖáňÈłÉò łÝåšţşÉå ąÏòňÁňź ŋťďÑòŋÍÞňÆęĳ řÍíšÅśÿęÛå ęÈĺÁśÝò łÈřÈčÛá ąÈłÖåňÛå ŋźąÑòşÉîčÈďť. čźśÆňÂřÆňÇ ľťęÛá ĺÉáňÛòňÛå ňÍäąÈ ňÄşţłÿ ňÅňÕòşťąź ńÆňÈčÛá ąÈčÛòŋÖòňÇ şťčťňÝîčÈďť.

[ ] /dev/nvram Support

-->PCňźłÿ CMOS(BIOS)Atari Non-Volatile RAMňÈęť ĺÁęÆčÛá

ĺÈşÄĺÉåłÍò ğźğĳęÈ ąťňÖáďź 50bytesęÛå ňÝæąÿčť ńÛå łÁ ňÝñďĳęÑÞ şÉáďť. şťďÆďÈłÆřÆňź ďÁąÈčÛá ňÄşÍíşÉá ďźňÈśÿčť ŋÍáňŒáňÈ ćÿŋžďĳ ňÝìňÿĺÿęÈğÏá ňÉáď£čÛá ğţňÁ ŋÖòňÀşÉá ďźňÈśÿęÛå ŋÿŋÉòşťčÛáďź ńÆňÝîčÈďť.

[ ] Enhanced Real Time Clock Support

-->łĳšÆśÆňÃňÿąť řÍíšÅśÿ łÝåłÈąÉá łÈążęÛå łťňÕòşÉå łÁ ňÝñďĳęÑÞ şťčÛá

ąÈčÛòňÝîčÈďť.ğÍåśÈ šÆęĳłźłÿ ğÿłÝáňÛå ąťŋÈąĳ ňÝñąĳ SMP ąÈčÛòňÛå łťňÕòşÉáďťğÏá łÍáśÊÞşÉîčÈďť.ěĳşÉá ŋÁąÈŋÍÞňÝá Data Sampling ďÛò ňÈąÈčÛòňÛå ňÅňÕòşťąź ńÛå ŋÉòŕÈąť ňÝñďťğÏá łÍåŋÍòşÉîčÈďť.

 Video for Linux -->

-->FM radio cardčť audio/video capturečť Overlay boardęÛå ŋÈňŒáşţ ŋÖîčÈďť.

ŋťłÝáňźąź ğÉóčÛá ąÍðňÈ ňÝñčť ňÅłÝíşÈ łÉåšžĺĳłźňÀ..

ąÆęÈąĳ ŋÉå łÍòąÑòşťğÏá ďťęÛáĺÖáďÛåňÛå ňÄşţ ďÊðąÛåňÛå ďÉåňťŋÁłźňÀ...(^___^);;

 < >video for linux
    < > AIMslab RadioTrack ( aka Radio Reveal ) support
    < > AIMslab RadioTrack FF support
    < > A : tech/Packard Bell Radio
    < > Miro PCM20 Radio
    < > Gemtek Radio Card support
    < > BT848 Video For Linux
    < > Modiavision Pro Movie Studio Video For Linux
    < > SAA5249 TeleText processor
    < > SF16FMI Radio
    < > Typhon Radio ( a.k.a EcoRadio )
    < > Zoltrix Radio

Joystick Support -->

-->JoystickňÛå ňÈňÕòşÉá łÝáčťčÛá ąźňÝíňÛå łťňÕòşťąĳšÛá łťňÕòŋťęťğÏá

@ ò 42

ňÅłÝíşÈ ĺÑáşÁ łÍáśÊÞşťŋť..ňÏÞłÈ ŋÉå łÍòąÑòşťğÏá ďťęÛáęÈčÖÞłÿęÛå ňÄşţ łÍòąÑòďÉíňÛå ďÊðąÛå ďÉåňťŋÁłÈğÏá ąĳğÉîąÎñłÛîčÈďť..(^___^);;

     < > Joystick support
     < > Classic PC analog joysticks gamepads
     < > FPGaming and MadCatz A3D controllers
     < > Gravis GrIP joysticks gamepads
     < > Logitech Digital joysticks gamepads
     < > Microsoft SideWinder, Genius Digital joysticks and gamepads
     < > ThrustMaster DirectConnect joysticks and game pads
     < > PDPI Lightning 4 gamecards

< > Double talk PC internal Speech card Support
Ftape,the floppy tape device driver--->

-->šÛåęĳšÈ řÍáśÆęÑåęÿňź ňÏáąÏåď£ňÿ ňÝñčÛá śźňÈšÆ ďÆęťňÈĺÆęÛå ąťŋÈąĳ

ňÝñčÛá łťňÕòŋťęťğÏá ňÈ şÉòğÑÞňÛå łÍåŋÍòşťąÈ ĺťęÉîčÈďť. ňÝåĺÉá łťňÕòŋťňźąźčÛá šÝåňÀňÍïčÛá şÉòğÑÞňÝîčÈďť.

~ USB drivers - not for the faint of heart

-->ňÈąÈčÛò ňÏÞłÈ ğÈęţňÇ šÀŋÖáňÆęĳ ŋťęÈŋÉîňť ąťąĳ ňÝñŋÀ.^^;;

     < > Support for USB ( Expermental )
     < > UHCI ( intel PIIX4 and others ) support
     < > OHCI ( compaq and some others ) support
     < > OHCI-HCD ( other OHCI opt,virt,Root HUb ) support
     < > USB hub support
     < > USB mouse support
     < > USB keyboard support
     < > USB audio parsing support
     < > USB abstract control Model support
     < > USB printer support
     < > USB SCSI support

~ File systems

[ ] Quota support

-->łťňÕòŋťňźąź łťňÕòşÉåłÁ ňÝñčÛá ďÈłÆřÆ ąÑòąÉáňÛå ŋźşÉáşÉåłÁ ňÝñčÛá

ňťŋÁ ňÅňÕòşÉá ąÈčÛòňÝîčÈďť.ňØîşĳłÆśÝòňÈčť şÉÞą¡łÿĺÿęÛå ňÖáňÏòşťęž şÉáďťğÏá łÍáśÊÞşťčÛáąź ŋÑøłÛîčÈďť.

< > Kernel automounter support (experimental)

-->ňÀŕÍòňź ěťęť ňŒáąÏÞ šťňÝåłÈłÆśÎíňÛå ŋťďÑòňÆęĳ ğťňÖáśÆşÉåłÁ ňÝñąź şţŋÖîčÈďť.

@ ò 43

BSDňÇ amdň¡ ďťęÆąź ğţňÁ ŋÍÞňÛá łťňÕòŋť ąÑòąÉáňÛå ŕťŋÈşťčÛá ďźğÑáňÈďť.

ňÈ ąÈčÛòňÛå łťňÕòşťęž şÉáďťğÏá "NFS Filesystem Support"şÉòğÑÞďĳ łÍáśÊÞşÉîčÈďť.

< > Amiga FFS filesystem support (EXPERIMENTAL)
< > Apple Macintosh filesystem Support
< > DOS FAT fs support

 -->FAT ąÈĺÉáňÇ MSDOS fs Support,VFAT(Windows-95) fs supportďÛò

   MSňÇ šťňÝåłÈłÆśÎíňÛå ŋťŋÁ ğťňÖáśÆşťňž łťňÕòşÉáďťğÏá łÍáśÊÞşÉîčÈďť.

ďţłÝá ňťęţ łťşÉòňÛå łÍáśÊÞşţ ŋÂňű şÉáďť.

ĺÿśÆ, umsdosşÉòğÑÞňÛá şÉòğÑÞňÛá ŋÍåďţ łÍáśÊÞşťŋÈ ňÉãąÝå ĺťęÉîčÈďť.

< > MSDOS fs support
      < > umsdos: Unix like fs on top of std MSDOS FAT fs
   < > VFAT (Windows-95) fs support
< > ISO9660 cdrom filesystem support

-->ISOňźłÿ ŋźňÉáşÉá łÈďÈęÑíňÛå ňÄşÉá šÀŋÖá šťňÝåłÈłÆśÎíňÝîčÈďť.

łÈďÈęÑíňÛå ŋťŋÁ ğťňÖáśÆşťňž ńÛáďťğÏá šÝåłÁňÀ,ňťčÈďÿęťďĳ ćÑÞ łÍáśÊÞşťąÝå ĺťęÉîčÈďť.

[ ] Microsoft joliet CDROM extentions

 -->Microsoftňźłÿ ąţĺÉåşÉá ňÅčÈřĳďÆ şÏòłÝÞňÇ ąÝá šťňÝåňÈęÛíňÛå ŋÈňŒáşťčÛá

şÒÞŋÉò ISO 9660 CDROM šťňÈłÈłÆśÎíňÝîčÈďť.

< > Minix fs support

-->śĳĺÉåŋÆŕÿęÍí ňÈąÍðňÆęĳ řÿčÍåąÑòĺÁęÛå łÈŋÉÞşţ ĺÑåłÁ ňÝñłÛîčÈďť.

ďÉá ňťłÈčÛáĺÖáğÉá łÍáśÊÞşťłźňÀ.

< > NTFS filesystem Support (read only)

 -->Microsoft NT filesystemňÛå ňÝæňÛåłÁ ňÝñąź şţŋÖîčÈďť.

[ ] NTFS read-write Support (DANGEROUS)

-->ňÄşÍíşÉîčÈďť.łÍáśÊÞşťŋÈ ğťłźňÀ.

[ ] OS/2 HPFS filesystem support (read only)

 -->OS/2 filesystem ňÛå ňÝæňÛåłÁ ňÝñąź şţŋÖîčÈďť.

[ ] /proc filesystem support

-->řÿčÍåą¡ šÆęĳłźłÆęÛå ňÄşÉá ąťłÉòňÇ šťňÝåłÈłÆśÎíňÝîčÈďť.

łÝåŋźęĳ ďÈłÆśÆąÑòąÉáňÛå ŕťŋÈşťŋÈčÛá ňÉãňÆğÏáłÿ šÆęĳłźłÆ ŋÍòĺĳ ďÛòňÛå ĺÑåłÁ ňÝñąź şţŋÖîčÈďť.

[ ] /dev/pts filesystem Support (readonly)

< > QNX filesystem Support

 -->QNX4 ňÖáňÏòŕźŋźňźłÿ łťňÕòşťčÛá šťňÝåłÈłÆśÎíňÝîčÈďť.

< > ROM filesystem Support

-->ŋÁęĳ ňÝáłÆśÑå ďÈłÆřÆňÇ ęÊíďÈłÆřÆęÛå ŕĳąÈş¡şťęžčÛá ğţňÁ ŋÉÞňÛá

ňÝæąÈŋÍáňÕò šťňÝåłÈłÆśÎíňÝîčÈďť.

   < > Second extended fs Support

  -->şÏáŋţ ęÈčÖÞłÆňźłÿ łťňÕòşťčÛá šťňÝåłÈłÆśÎíňÝîčÈďť.ĺÉáďÆłÈ łÍáśÊÞşÉîčÈďť.

< > System V and Coherent filesystem support

 -->Xeniaň¡ Cherentň¡ ąÉöňÛá ňÝáśÎå ąÈŋÑòňÛå ňÄşÉá łÉòňÕò ňÅčÝÞłÆ łÈłÆśÎíňÛå

ŋÈňŒáşÉîčÈďť.

< > UFS filesystem support (read only)

 -->BSDň¡ Unixňźłÿ šťłÊòďÔá ĺÿŋÍá

    (SunOS,FreeBSD,NetBSD,OpenBSD,NextStep)ďÛåňÛá UFSęťčÛá

šťňÝåłÈłÆśÎíňÛå łťňÕòşÉîčÈďť.

ňÿěÍá System V ňÅčÝÞłÆčÛá ďÈłÆřÆ šťśÈłÏáňÈčť šÛåęĳšÈ ďÈłÆřÆňź UFS šťňÝåłÈłÆśÎíňÛå łťňÕòşťąÈďĳ şÉîčÈďť.

   NFSęÛå łťňÕòşÉáďťğÏá ňÈ ňÑîłÏáňÛå łÍáśÊÞşťğÏá ňÉáďÔîčÈďť.

Network filesystems-->

     < > Coda filesystem support ( advanced networks fs )

      -->NFSň¡ ĺÈłÛðşÉá ŋÝáĺĳďÔá čźśÆňÂřÆ šťňÝåłÈłÆśÎíňÝîčÈďť.

ĺÈŋÍîłÑÞ ňÖáňÏò,řţłÈ,ĺĳňÉáą¡ ňÝáŋÛò ďÛò NFSĺĳďť ŋÑøňÛá ŋÍíňÈ ğÏôąťŋÈ ňÝñňÛîčÈďť.ňÈąÍðňÛå łÍáśÊÞşťğÏá Coda řÛåęťňÈňÍáśÆęĳ ďÑòŋÉÞşťğž łÿĺÿň¡ řÛåęťňÈňÍáśÆ ğĳďÁ ŋÈňŒáşţňű şÉîčÈďť.

< > NFS filesystem support

 -->čźśÆňÂřÆ šťňÝåłÈłÆśÎíňÛå ŋÈňŒáşÉîčÈďť.

< > SMB filesystem support (to mount WfW shares etc.)

 -->ęÈčÖÞłÆňźłÿ MS windows 95,98/NT čźśÆňÂřÆ ŋťňŒáňÛå ąÑòňÅşÉåłÁ

ňÝñąź şţŋÁčÛá ąÈčÛòňÝîčÈďť.

NTň¡ windows 95,98 şÉíćź čźśÆňÂřÆęÛå łťňÕòşÉáďťğÏá ňÅňÕòşťąź

ńÆňÝîčÈďť.

@ ò 45

      < > NCP filesystem support(to mount NetWare volumes)

       -->NCP(Netware Core Prptocol)ňÛá IPX ęÛå ňÈňÕòşÉá ęÊá šÆęĳśĳřÑåňÝîčÈďť.

      [ ] Packet signatures

       -->NCPňź ĺĳňÉáňÛå ąÉòş¡łÈřž ŋÁčÛá ąÈčÛòňÛå ŋźąÑòşÉîčÈďť.

      [ ] Proprietary file Locking

    -->ęÈğĳśÆ ĺÑåęÚíłÉòňź ęźřĳďÆęÛå lockingşÉîčÈďť.

      [ ] Clear remove/delete inhibit when neede

   -->šťňÝå šÛåęţąÆ ŋĳŋÉÞňÛå şÿňÕòşÉîčÈďť.

      [ ] Use NFS namespace if available
      [ ] Use long ( os/2 ) namespace if available
      [ ] Allow mouthing of volume subdirectories
      [ ] Use Native language Support
      [ ] Enale symbolic links and Execute flags
 Partition Types ->
      [ ] BSD disklabel ( BSD partiton tables ) support
      [ ] Macintosh partition map Support
      [ ] SMD disklabel ( sun partition tables ) support
      [ ] Solaris ( X86 ) partition table support
      [ ] SGI disklabel support
 Native Language Support -->

-->ňťłÙîąźďĳ ňťŋÝÞşÉáąÖÞňÿňÇ ŋÈňŒáňÈ ňÍïłÛîčÈďť.

şÉáąÛå řĳďÆšźňÈŋÈęÛå 949ęÛå łťňÕòşťęžğÏá šţŕÈęÛå łÁşÊòşţňű şÉîčÈďť.

~ Consoledrivers

[ ] VGA text console
[ ] Video mode Selection Support

~ Sound

< > Sound card support

-->ŋťłÝáňÇ ęÈčÖÞłÆĺÉÞłÆňź łťňÖáďÆ řťďÆąť ňÝñďťğÏá łÍáśÊÞşÉîčÈďť.

< > C-media PCI (CMI8338/8378 )
< > Ensoniq AudioPCI
< > Creative Ensoniq AudioPCI 97 (ES1371)

< > S3 SonicVibes

< > Support for Turtle Beach MutiSound Classic, Tahiti , Monterey

< > Support for Turtle Beach MutiSound Pinnacle, Fiji

< > OSS sound modules

 -->OSS(Ooen Sound System)łťňÖáďÆ řťďÆ ďÆęťňÈĺÿ ğĳňÛíňÝîčÈďť.

łÍáśÊÞłÈ ňťęţňť ąÉöňÈ ďťňËòşÉá şÉòğÑÞňÈ čťňÑîčÈďť.

< > ProAudioSpectrum 16 support

-->ProAudioSpectrum 16, ProAudio Studio 16,

    Logitec SoundMan 16 łťňÖáďÆ řťďÆęÛå ęÈčÖÞłÆňźłÿ

łťňÕòąťčÛòşťďĳęÑÞ ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

Media Vision ěĳčÛá Logitec ňźłÿ čťňĳčÛá ďťęÛá łťňÖáďÆ

řťďÆęÛå ąťŋÈąĳ ňÝñčÛá łťňÕòŋťęťğÏá łÍáśÊÞşÉîčÈďť.

    !!PAS16 ą¡čÛá şĳşÒáď£ŋÈ ňÉãłÛîčÈďť.

< > 100% Sound Blaster compatibles (SB16/32/64,ESS,Jazz16)

     support

-->łťňÖáďÆ řťďÆŋÖòňźłÿ ąťŋÉò ňÝåĺÉáŋÍÞňÆęĳ łťňÕòď£čÛá łťňÖáďÆ

ĺÛåęťłÆśÿň¡ łťňÖáďÆ ĺÛåęťłÆśÿ şĳşÒá łťňÖáďÆ řťďÆęÛå łÍåŋÍòşťčÛá şÉòğÑÞňÝîčÈďť.ŋťłÝáňÇ łťňÖáďÆ řťďÆąť łťňÖáďÆ ĺÛåęťłÆśÿ ňÈąÿčť łťňÖáďÆ ĺÛåęťłÆśÿşĳşÒáňÈęťąĳ łÊòąÉÞď£ğÏá łÍáśÊÞşÉîčÈďť.

< > Generic OPL2/OPL3 FM synthesizer support

-->łťňÖáďÆ řťďÆąť ňűğťşťłťňźłÿ ğÉáďÛá FM ŕÝîňÛå ąťŋÈąĳ ňÝñčÛá

łťňÕòŋťęťğÏá łÍáśÊÞşÉáďť.

ďţĺÁĺÖáňÇ łťňÖáďÆ řťďÆčÛá ňűğťşťňÇ FM ŕÝîňÛå łťňÕòşťğž, łťňÖáďÆ ĺÛåęťłÆśÿ ążňÏåňÇ łťňÖáďÆ řťďÆčÛá ąÈĺÑáŋÍÞňÆęĳ ďÛåňÿňÝñčÛá ŕÝîňÝîčÈďť. łťňÖáďÆ ĺÛåęťłÆśÿ čť łťňÖáďÆ ĺÛåęťłÆśÿ şĳşÒá łťňÖáďÆ řťďÆęÛå ąťŋÝá łťňÕòŋťęťğÏá łÍáśÊÞşÉîčÈďť.

< > Gravis Ultrasound support

 -->Gravis Ultrasound cardęÛå łťňÕòąťčÛòşťąź şţŋÖîčÈďť.

< > MPU-401 support (NOT for SB16)

-->łťňÖáďÆ řťďÆňÇ ğÈďÈ ňÝáśÿšźňÈłÆňÝá MPU-401 ňÛå ŋÈňŒáşťčÛá

ąÈčÛòňÝáďź, ąÿňÇ ğĳďÛáłťňÖáďÆ řťďÆąť ňÈ ňÝáśÿšźňÈłÆęÛå ŕţśÊÞşťąĳ ňÝñňÛîčÈďť.ąÆęÍøďťąĳ şţłÿ ğÁŋĳąÍá łÍáśÊÞşţłÿčÛá ňÉáďÔîčÈďť. ŋÝáőťęĳ MPU-401 ğÈďÈ řťďÆąť ňÝñčÛá łťňÖáďÆ řťďÆęÛå ąťŋÈąĳ ňÝñčÛá łťňÕòŋťğÉá łÍáśÊÞşÉîčÈďť.

łťňÖáďÆ ĺÛåęťłÆśÿ ążňÏå ąťŋÈąĳ ňÝñďťğÏá łÍáśÊÞşťğÏá ňÉáďÔîčÈďť.

< > PSS (AD1848,ADSP-2115,ESC614) support

-->PSS ŕÝîňź ąÈĺÉáňÛå ďÖá Orchid SW32, Cardinal DSP16

@ ò 47

łťňÖáďÆ řťďÆęÛå łťňÕòąťčÛòşťďĳęÑÞ ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

      < > Microsoft Sound System support

-->łťňÖáďÆ ĺÛåęťłÆśÿ łťňÕòŋťęťğÏá ŋÁňÇęÛå ąÈňÖåňžňű şťčÛá ĺÁĺÖáňÝîčÈďť.

łťňÖáďÆ ĺÛåęťłÆśÿ ążňÏå ŋÖò ğťňÈřÆęĳ łĳšÆśÆ łťňÖáďÆ łÈłÆśÎíňÛå ŋÈňŒáşťčÛá łťňÖáďÆ řťďÆęÛå ąťŋÈąĳ ňÝñčÛá łťňÕòŋťęťğÏá ňÈ şÉòğÑÞňÛå łÍáśÊÞşťąÈ ĺťęÉîčÈďť.ňÈňÅčÛá łťňÖáďÆ ĺÛåęťłÆśÿ şÉòğÑÞňÛå łÍáśÊÞşťąź ď£ğÏá łťňÖáďÆčÛá 8Bit ęĳ ŋÉÞďÑòşťąź ď£ąĳ,ňÈşÉòğÑÞňÛå łÍáśÊÞşťğÏá

16Bit ęĳ ŋÉÞďÑòşťąź ďÔîčÈďť.

łťňÖáďÆ ĺÛåęťłÆśÿ şÉòğÑÞą¡ ňÈ şÉòğÑÞňÛå ąÉöňÈ łÍáśÊÞşÉåłÁčÛá ňÍïłÛîčÈďť. łťňÖáďÆ ĺÛåęťłÆśÿ ążňÏåňÇ łťňÖáďÆ řťďÆęÛå ąťŋÈąĳ ňÝñčÛá łťňÕòŋťčÛá ňÝåďÉá ğţčÅňÍåňÛå ňÅłÝíşÈ ĺĳąĳ čťłÿ ŋťłÝáňÈ ğťňÈřÆęĳ łĳšÆśÆ łťňÖáďÆ łÈłÆśÎíňÛå ŋÈňŒáşÉáďťąĳ şÒÞłÝáňÈłÿğÏá ňÈ şÉòğÑÞňÛå łÍáśÊÞşťąÈ ĺťęÉîčÈďť.

< > Ensoniq SoundScape support

--> Ensoniq SoundScape ŕÝîłÎðňź ąÈĺÉáňÛå ďÖá łťňÖáďÆ řťďÆęÛå

ŋÈňŒáşÉîčÈďť.

< > MediaTrix AudidTric Pro support

--> MediaTrix AudioTrix Pro łťňÖáďÆ řťďÆęÛå łťňÕòąťčÛò

şťďĳęÑÞ ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

< > Support for OPTi MAD16 and/or Morzart based cards

 -->Mozart(Oak OTi-601) ňÈčť
     MAD16(OPTi 82C928/82C929)ŕÝîłÎðňÛå ąÈĺÉáňÆęĳ şťčÛá

łťňÖáďÆ řťďÆęÛå łťňÕòąťčÛòşťďĳęÑÞ şţŋÖîčÈďť.

< > Full support for Turtle Beach WaveFront
     (Tropez Plus, Tropez)
< > Support for Crystal CS4232 based (PnP) cards

-->Crystal CS4232 ŕÝîłÎðňÛå ąÈĺÉáňÆęĳ şťčÛá łťňÖáďÆ řťďÆęÛå

łťňÕòąťčÛòşťďĳęÑÞ ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

< > Support for Aztech Sound Galaxy (non-PnP) cards
< > Limited support for Turtle Beach Wave Front
     (Maui,Tropez)
< > Support for Aztech Sound Galaxy (non-PnP) cards
< > Yamaha OPL3-SA1 audio controller
< > SoftOSS software wave table engine
< >FM synthesizer(YM3812/OPL-3 ) support

-->ňÈ şÉòğÑÞňÛá FM łÝáłÿłÈŋÿęÛå łťňÕòąťčÛòşťďĳęÑÞ ŋÈňŒáşţŋÁčÛá

ąÈčÛòňÝîčÈďť.łÍáśÊÞşÉîčÈďť.

< > Loopback MIDI device support

-->MIDIčÛá FMą¡ ďťęÆąź łÝåŋź łĳęÈęÛå ňÛíňŒáňÆęĳ şÉîčÈďť.

    /dev/sequencer ň¡ /dev/musicňÛå ňÈňÕòşÉá MIDIšĳśÆňÇ

ŋÍîłÑÞą¡ /dev/midixxęÛå łťňÕòşťŋÈ ňÉãňÛå ąÿęťğÏá łÍáśÊÞşťŋÈ ňÉãčÛáąźŋÑøłÛîčÈďť.

     < > 6850 UART support

Additional low level sound drivers --->

     < > Additional low level sound drivers

   -->ŕÁąťŋÍÞňÝá ąÈĺÑáďÛòąÛî ďÆęťňÈĺÿęÛå łťňÕòşÉå ąÍð ňÝáąťęÛå łÍåŋÍòşťčÛá

ąÈčÛòňÝîčÈďť. AWEłťňÖáďÆ ĺÛåęťłÆśÿęÛå łťňÕòşÉáďťğÏá łÍáśÊÞşÉîčÈďť.

< > ACI mixer (microPCM12)

-->ňÈ şÉòğÑÞňÛá ACI ğÝÞłÿęÛå łťňÕòąťčÛòşťďĳęÑÞ ŋÈňŒáşţŋÁčÛá

ąÈčÛòňÝîčÈďť.

  ACI ğÝÞłÿęÛå ŋÈňŒáşťďĳęÑÞ łÍåŋÍòşťęžğÏá łÍáśÊÞşÉîčÈďť.

< > AWE32 synth

-->łťňÖáďÆ ĺÛåęťłÆśÿňÇ AWE32 łÝáďÈ łťňÖáďÆęÛå łťňÕòşÉåłÁ ňÝñąź

ŋÈňŒáşţŋÁčÛá ąÈčÛòňÝîčÈďť.

ŋťłÝáňÇ łťňÖáďÆ řťďÆąť AWE ŋÈňŒá łťĺÛåňÛå ąťŋÈąĳ ňÝñďťğÏá łÍáśÊÞşÉîčÈďť.

ěĳşÉá, Emu8k ďĳ ŋÈňŒáşÉîčÈďť.

< > Gallant Audio Cards (SC-6000 and SC-6600 based )

~ Kernel hacking

 [ ] Kernel profiling support

-->ňÈ şÉòğÑÞňÛå łÍåŋÍòşťğÏá řÿčÍåňźłÿ ňÈęÁňÿŋÈčÛá ğĳďÛá ŋÍåŕťďÛåňÈ

    /proc ęťčÛá ďÈęÎÞśĳęÈňź profile ňÈęťčÛá šťňÝåęĳńÿ ŋÿŋÉòď£ňÿ

šťňÝåňÛå ňÝæňÿłÿ ŋÍåŕťďÛåňÛå şÒÞňÝáşÉåłÁ ňÝñąź şţŋÖîčÈďť. řÿčÍåňÇ čţĺÁ ąÁŋĳęÛå ňÉåąĳ łÝœňÛá łťňÕòŋťęťğÏá łÍáśÊÞşţĺÑîčÈďť.

epilog...

Ł§ńŞ ąè8t SŽ ¸Ęê qů3ˇ ŮŒÏ vG {7‹Ć Âľt SŽ¸Ęê ˇú !œŞř8 9Ź

...(^ ^);;«ęř. ˘ùÛffi¸ Xœ£ ˘ù èśóąõ $XL ŢÍ8t Şéú Ł§Ć SŽB 8`èĹ

{7‹ú ˛ü ?ăŹ ˘ù ýĄtffiĆ3 SŽ¸#˝ êÓ¸ ü}œ8 ^9åęř.řèćě ¸ ˛_õ uüă 8t Xéă§ˇ ăL 3ýŹ §Á:‚ ÙÛĆ ˘ù êÓsê á\Ţ(http://accellinux.mdworld.com/ )ńY ðËÞ(electuz@chollian.net)ńY ěŒõ(iqzero76@chollian.net)ńÍ řèćě ˇPȷ^ęř. ŤýL ¸ě Č y# uüăê ?fiÛffi3 ¡LăŞřŹ ˙;ú ¸ ıýõ ßq ȷ^ęř.

”ýĄSSŹ ŕ(zzem)–åęř...Linux is fun!!”...(^ ^);;;